## Panasonic Tags

These tags are used in Panasonic/Leica cameras.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | ImageQuality | int16u | (quality of the main image, which may be in a different file)
> 1 = TIFF 2 = High 3 = Normal 6 = Very High |  | 7 = RAW 9 = Motion Picture 11 = Full HD Movie 12 = 4k Movie
> 0x0002 | FirmwareVersion | undef | (for some camera models such as the FZ30 this may be an internal production reference number and not the actual firmware version)
> 0x0003 | WhiteBalance | int16u |
> 1 = Auto 2 = Daylight 3 = Cloudy 4 = Incandescent 5 = Manual 8 = Flash 10 = Black & White |  | 11 = Manual 2 12 = Shade 13 = Kelvin 14 = Manual 3 15 = Manual 4 19 = Auto (cool)
> 0x0007 | FocusMode | int16u |
> 1 = Auto 2 = Manual 4 = Auto, Focus button 5 = Auto, Continuous |  | 6 = AF-S 7 = AF-C 8 = AF-F
> 0x000f | AFAreaMode | int8u[2] | (DMC-FZ10) '0 1' = Spot Mode On '0 16' = Spot Mode Off (other models)
> 16 = Normal? '0 1' = 9-area '0 16' = 3-area (high speed) '0 23' = 23-area '0 49' = 49-area '0 225' = 225-area '1 0' = Spot Focusing '1 1' = 5-area '16 0' = 1-area '16 16' = 1-area (high speed) '16 32' = 1-area + '17 0' = Full Area '32 0' = Tracking '32 1' = 3-area (left)? '32 2' = 3-area (center)? '32 3' = 3-area (right)? '32 16' = Zone '32 18' = Zone (horizontal/vertical) '64 0' = Face Detect '64 1' = Face Detect (animal detect on) '64 2' = Face Detect (animal detect off) '128 0' = Pinpoint focus '240 0' = Tracking
> 0x001a | ImageStabilization | int16u |
> 2 = On, Optical 3 = Off 4 = On, Mode 2 5 = On, Optical Panning 6 = On, Body-only 7 = On, Body-only Panning 9 = Dual IS 10 = Dual IS Panning 11 = Dual2 IS 12 = Dual2 IS Panning
> 0x001c | MacroMode | int16u | 1 = On 2 = Off 257 = Tele-Macro 513 = Macro Zoom
> 0x001f | ShootingMode | int16u |
> 1 = Normal 2 = Portrait 3 = Scenery 4 = Sports 5 = Night Portrait 6 = Program 7 = Aperture Priority 8 = Shutter Priority 9 = Macro 10 = Spot 11 = Manual 12 = Movie Preview 13 = Panning 14 = Simple 15 = Color Effects 16 = Self Portrait 17 = Economy 18 = Fireworks 19 = Party 20 = Snow 21 = Night Scenery 22 = Food 23 = Baby 24 = Soft Skin 25 = Candlelight 26 = Starry Night 27 = High Sensitivity 28 = Panorama Assist 29 = Underwater 30 = Beach 31 = Aerial Photo 32 = Sunset 33 = Pet 34 = Intelligent ISO 35 = Clipboard 36 = High Speed Continuous Shooting 37 = Intelligent Auto 39 = Multi-aspect 41 = Transform 42 = Flash Burst |  | 43 = Pin Hole 44 = Film Grain 45 = My Color 46 = Photo Frame 48 = Movie 51 = HDR 52 = Peripheral Defocus 55 = Handheld Night Shot 57 = 3D 59 = Creative Control 60 = Intelligent Auto Plus 62 = Panorama 63 = Glass Through 64 = HDR 66 = Digital Filter 67 = Clear Portrait 68 = Silky Skin 69 = Backlit Softness 70 = Clear in Backlight 71 = Relaxing Tone 72 = Sweet Child's Face 73 = Distinct Scenery 74 = Bright Blue Sky 75 = Romantic Sunset Glow 76 = Vivid Sunset Glow 77 = Glistening Water 78 = Clear Nightscape 79 = Cool Night Sky 80 = Warm Glowing Nightscape 81 = Artistic Nightscape 82 = Glittering Illuminations 83 = Clear Night Portrait 84 = Soft Image of a Flower 85 = Appetizing Food 86 = Cute Dessert 87 = Freeze Animal Motion 88 = Clear Sports Shot 89 = Monochrome 90 = Creative Control 92 = Handheld Night Shot
> 0x0020 | Audio | int16u | 1 = Yes 2 = No 3 = Stereo
> 0x0021 | DataDump | no |
> 0x0023 | WhiteBalanceBias | int16s |
> 0x0024 | FlashBias | int16s |
> 0x0025 | InternalSerialNumber | undef[16] | (this number is unique, and contains the date of manufacture, but is not the same as the number printed on the camera body)
> 0x0026 | PanasonicExifVersion | undef |
> 0x0027 | VideoFrameRate | int16u | (only valid for older models) 0 = n/a
> 0x0028 | ColorEffect | int16u |
> 1 = Off 2 = Warm 3 = Cool 4 = Black & White |  | 5 = Sepia 6 = Happy 8 = Vivid
> 0x0029 | TimeSincePowerOn | int32u | (time in 1/100 s from when the camera was powered on to when the image is written to memory card)
> 0x002a | BurstMode | int16u | (decoding may be different for some models)
> 0 = Off 1 = On 2 = Auto Exposure Bracketing (AEB) 3 = Focus Bracketing 4 = Unlimited 8 = White Balance Bracketing 17 = On (with flash) 18 = Aperture Bracketing
> 0x002b | SequenceNumber | int32u |
> 0x002c | ContrastMode | int16u | (this decoding seems to work for some models such as the LC1, LX2, FZ7, FZ8, FZ18 and FZ50, but may not be correct for other models such as the FX10, G1, L1, L10 and LC80)
> 0x0 = Normal 0x1 = Low 0x2 = High 0x5 = Normal 2 0x6 = Medium Low 0x7 = Medium High 0xd = High Dynamic 0x18 = Dynamic Range (film-like) 0x2e = Match Filter Effects Toy 0x37 = Match Photo Style L. Monochrome 0x100 = Low 0x110 = Normal 0x120 = High
> (these values are used by the G2, GF1, GF2, GF3, GF5 and GF6) 0 = -2 1 = -1 2 = Normal 3 = +1 4 = +2 5 = Normal 2 7 = Nature (Color Film) 9 = Expressive 12 = Smooth (Color Film) or Pure (My Color) 17 = Dynamic (B&W Film) 22 = Smooth (B&W Film) 25 = High Dynamic 26 = Retro 27 = Dynamic (Color Film) 28 = Low Key 29 = Toy Effect 32 = Vibrant (Color Film) or Expressive (My Color) 33 = Elegant (My Color) 37 = Nostalgic (Color Film) 41 = Dynamic Art (My Color) 42 = Retro (My Color) 45 = Cinema 47 = Dynamic Mono 50 = Impressive Art 51 = Cross Process 100 = High Dynamic 2 101 = Retro 2 102 = High Key 2 103 = Low Key 2 104 = Toy Effect 2 107 = Expressive 2 112 = Sepia 117 = Miniature 122 = Dynamic Monochrome 127 = Old Days 132 = Dynamic Monochrome 2 135 = Impressive Art 2 136 = Cross Process 2 137 = Toy Pop 138 = Fantasy 256 = Normal 3 272 = Standard 288 = High (these values are used by the TZ10 and ZS7) 0 = Normal 1 = -2 2 = +2 5 = -1 6 = +1
> 0x002d | NoiseReduction | int16u | (the encoding for this value is not consistent between models)
> 0 = Standard 1 = Low (-1) 2 = High (+1) 3 = Lowest (-2) 4 = Highest (+2) 5 = +5 |  | 6 = +6 65531 = -5 65532 = -4 65533 = -3 65534 = -2 65535 = -1
> 0x002e | SelfTimer | int16u |
> 0 = Off (0) 1 = Off 2 = 10 s 3 = 2 s 4 = 10 s / 3 pictures 258 = 2 s after shutter pressed 266 = 10 s after shutter pressed 778 = 3 photos after 10 s
> 0x0030 | Rotation | int16u | 1 = Horizontal (normal) 3 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 0x0031 | AFAssistLamp | int16u | 1 = Fired 2 = Enabled but Not Used 3 = Disabled but Required 4 = Disabled and Not Required
> 0x0032 | ColorMode | int16u | 0 = Normal 1 = Natural 2 = Vivid
> 0x0033 | BabyAge | string | (or pet age)
> 0x0034 | OpticalZoomMode | int16u | 1 = Standard 2 = Extended
> 0x0035 | ConversionLens | int16u | 1 = Off 2 = Wide 3 = Telephoto 4 = Macro
> 0x0036 | TravelDay | int16u |
> 0x0038 | BatteryLevel | int16u |
> 1 = Full 2 = Medium 3 = Low 4 = Near Empty |  | 7 = Near Full 8 = Medium Low 256 = n/a
> 0x0039 | Contrast | int16u | 0 = Normal
> 0x003a | WorldTimeLocation | int16u | 1 = Home 2 = Destination
> 0x003b | TextStamp | int16u | 1 = Off 2 = On
> 0x003c | ProgramISO | int16u | -1 = n/a 65534 = Intelligent ISO 65535 = n/a
> 0x003d | AdvancedSceneType | int16u | (used together with SceneMode to derive Composite AdvancedSceneMode)
> 0x003e | TextStamp | int16u | 1 = Off 2 = On
> 0x003f | FacesDetected | int16u |
> 0x0040 | Saturation | int16u | 0 = Normal
> 0x0041 | Sharpness | int16u | 0 = Normal
> 0x0042 | FilmMode | int16u |
> 0 = n/a 1 = Standard (color) 2 = Dynamic (color) 3 = Nature (color) 4 = Smooth (color) |  | 5 = Standard (B&W) 6 = Dynamic (B&W) 7 = Smooth (B&W) 10 = Nostalgic 11 = Vibrant
> 0x0043 | JPEGQuality | int16u | 0 = n/a (Movie) 2 = High 3 = Standard 6 = Very High 255 = n/a (RAW only)
> 0x0044 | ColorTempKelvin | int16u |
> 0x0045 | BracketSettings | int16u |
> 0 = No Bracket 1 = 3 Images, Sequence 0/-/+ 2 = 3 Images, Sequence -/0/+ 3 = 5 Images, Sequence 0/-/+ 4 = 5 Images, Sequence -/0/+ 5 = 7 Images, Sequence 0/-/+ 6 = 7 Images, Sequence -/0/+
> 0x0046 | WBShiftAB | int16u | (positive is a shift toward blue)
> 0x0047 | WBShiftGM | int16u | (positive is a shift toward green)
> 0x0048 | FlashCurtain | int16u | 0 = n/a 1 = 1st 2 = 2nd
> 0x0049 | LongExposureNoiseReduction | int16u | 1 = Off 2 = On
> 0x004b | PanasonicImageWidth | int32u |
> 0x004c | PanasonicImageHeight | int32u |
> 0x004d | AFPointPosition | rational64u[2] | (X Y coordinates of primary AF area center, in the range 0.0 to 1.0, or "n/a" or "none" for invalid values)
> 0x004e | FaceDetInfo | - | --> Panasonic FaceDetInfo Tags
> 0x0051 | LensType | string |
> 0x0052 | LensSerialNumber | string |
> 0x0053 | AccessoryType | string |
> 0x0054 | AccessorySerialNumber | string |
> 0x0059 | Transform | undef[4] | (decoded as two 16-bit signed integers) '-1 1' = Slim Low '-3 2' = Slim High '0 0' = Off '1 1' = Stretch Low '3 2' = Stretch High
> 0x005d | IntelligentExposure | int16u | (not valid for some models) 0 = Off 1 = Low 2 = Standard 3 = High
> 0x0060 | LensFirmwareVersion | undef[4] |
> 0x0061 | FaceRecInfo | - | --> Panasonic FaceRecInfo Tags
> 0x0062 | FlashWarning | int16u | 0 = No 1 = Yes (flash required but disabled)
> 0x0063 | RecognizedFaceFlags? | undef[4] |
> 0x0065 | Title | undef |
> 0x0066 | BabyName | undef | (or pet name)
> 0x0067 | Location | undef |
> 0x0069 | Country | undef |
> 0x006b | State | undef |
> 0x006d | City | undef | (City/Town as stored by some models, or County/Township for others)
> 0x006f | Landmark | undef |
> 0x0070 | IntelligentResolution | int8u | 0 = Off 1 = Low 2 = Standard 3 = High 4 = Extended
> 0x0076 | MergedImages | int16u | (number of images in HDR or Live View Composite picture)
> 0x0077 | BurstSpeed | int16u | (images per second)
> 0x0079 | IntelligentD-Range | int16u | 0 = Off 1 = Low 2 = Standard 3 = High
> 0x007c | ClearRetouch | int16u | 0 = Off 1 = On
> 0x0080 | City2 | undef | (City/Town/Village as stored by some models)
> 0x0086 | ManometerPressure | int16u |
> 0x0089 | PhotoStyle | int16u |
> 0 = Auto 1 = Standard or Custom 2 = Vivid 3 = Natural 4 = Monochrome 5 = Scenery 6 = Portrait |  | 8 = Cinelike D 9 = Cinelike V 11 = L. Monochrome 12 = Like709 15 = L. Monochrome D 17 = V-Log 18 = Cinelike D2
> 0x008a | ShadingCompensation | int16u | 0 = Off 1 = On
> 0x008b | WBShiftIntelligentAuto | int16u | (value is -9 for blue to +9 for amber. Valid for Intelligent-Auto modes)
> 0x008c | AccelerometerZ | int16u | (positive is acceleration upwards)
> 0x008d | AccelerometerX | int16u | (positive is acceleration to the left)
> 0x008e | AccelerometerY | int16u | (positive is acceleration backwards)
> 0x008f | CameraOrientation | int8u |
> 0 = Normal 1 = Rotate CW 2 = Rotate 180 |  | 3 = Rotate CCW 4 = Tilt Upwards 5 = Tilt Downwards
> 0x0090 | RollAngle | int16u | (converted to degrees of clockwise camera rotation)
> 0x0091 | PitchAngle | int16u | (converted to degrees of upward camera tilt)
> 0x0092 | WBShiftCreativeControl | int8u | (WB shift or style strength. Valid for Creative-Control modes)
> 0x0093 | SweepPanoramaDirection | int8u | 0 = Off 1 = Left to Right 2 = Right to Left 3 = Top to Bottom 4 = Bottom to Top
> 0x0094 | SweepPanoramaFieldOfView | int16u |
> 0x0096 | TimerRecording | int8u | 0 = Off 1 = Time Lapse 2 = Stop-motion Animation 3 = Focus Bracketing
> 0x009d | InternalNDFilter | rational64u |
> 0x009e | HDR | int16u |
> 0 = Off 100 = 1 EV 200 = 2 EV 300 = 3 EV |  | 32868 = 1 EV (Auto) 32968 = 2 EV (Auto) 33068 = 3 EV (Auto)
> 0x009f | ShutterType | int16u | 0 = Mechanical 1 = Electronic 2 = Hybrid
> 0x00a1 | FilterEffect | rational64u[0.5] |
> '0 0' = Off '0 1' = Expressive '0 2' = Retro '0 4' = High Key '0 8' = Sepia '0 16' = High Dynamic '0 32' = Miniature Effect '0 1024' = Dynamic Monochrome '0 1048576' = Sunshine '0 134217728' = Silky Monochrome '0 16384' = One Point Color '0 2048' = Soft Focus '0 2097152' = Bleach Bypass '0 256' = Low Key '0 32768' = Star Filter '0 33554432' = Monochrome '0 4096' = Impressive Art '0 4194304' = Toy Pop '0 512' = Toy Effect '0 524288' = Old Days '0 67108864' = Rough Monochrome '0 8192' = Cross Process '0 8388608' = Fantasy
> 0x00a3 | ClearRetouchValue | rational64u |
> 0x00a7 | OutputLUT | yes | (2-column by 432-row binary lookup table of unsigned short values for converting to 16-bit output (1st column) from 14 bits (2nd column) with camera contrast)
> 0x00ab | TouchAE | int16u | 0 = Off 1 = On
> 0x00ac | MonochromeFilterEffect | int16u | 0 = Off 1 = Yellow 2 = Orange 3 = Red 4 = Green
> 0x00ad | HighlightShadow | int16u[2] |
> 0x00af | TimeStamp | string |
> 0x00b3 | VideoBurstResolution | int16u | 1 = Off or 4K 4 = 6K
> 0x00b4 | MultiExposure | int16u | 0 = n/a 1 = Off 2 = On
> 0x00b9 | RedEyeRemoval | int16u | 0 = Off 1 = On
> 0x00bb | VideoBurstMode | int32u |
> 0x1 = Off 0x4 = Post Focus 0x18 = 4K Burst 0x28 = 4K Burst (Start/Stop) 0x48 = 4K Pre-burst 0x108 = Loop Recording 0x408 = Focus Stacking 0x810 = 6K Burst 0x820 = 6K Burst (Start/Stop) 0x1001 = High Resolution Mode
> 0x00bc | DiffractionCorrection | int16u | 0 = Off 1 = Auto
> 0x00bd | FocusBracket | int16u | (positive is further, negative is closer)
> 0x00be | LongExposureNRUsed | int16u | 1 = No 2 = Yes
> 0x00bf | PostFocusMerging | int32u[2] | '0 0' = Post Focus Auto Merging or None
> 0x00c1 | VideoPreburst | int16u | 0 = No 1 = 4K or 6K
> 0x00c4 | LensTypeMake | int16u |
> 0x00c5 | LensTypeModel | int16u |
> 0x00ca | SensorType | int16u | 0 = Multi-aspect 1 = Standard
> 0x00d1 | ISO | int32u |
> 0x00d2 | MonochromeGrainEffect | int16u | 0 = Off 1 = Low 2 = Standard 3 = High
> 0x00d6 | NoiseReductionStrength | rational64s |
> 0x00de | AFAreaSize | rational64u[2] | (relative to size of image. "n/a" for manual focus)
> 0x00e4 | LensTypeModel | int16u |
> 0x00e8 | MinimumISO | int32u |
> 0x00e9 | AFSubjectDetection | int16u |
> 0 = n/a 1 = Human Eye/Face/Body 2 = Animal 3 = Human Eye/Face 4 = Animal Body 5 = Animal Eye/Body 6 = Car 7 = Motorcycle 8 = Car (main part priority) 9 = Motorcycle (helmet priority) 10 = Train 11 = Train (main part priority) 12 = Airplane 13 = Airplane (nose priority)
> 0x00ee | DynamicRangeBoost | int16u | 0 = Off 1 = On
> 0x00f1 | LUT1Name | string |
> 0x00f3 | LUT1Opacity | int8u |
> 0x00f4 | LUT2Name | string |
> 0x00f5 | LUT2Opacity | int8u |
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x2003 | TimeInfo | - | --> Panasonic TimeInfo Tags
> 0x8000 | MakerNoteVersion | undef |
> 0x8001 | SceneMode | int16u |
> 0 = Off 1 = Normal 2 = Portrait 3 = Scenery 4 = Sports 5 = Night Portrait 6 = Program 7 = Aperture Priority 8 = Shutter Priority 9 = Macro 10 = Spot 11 = Manual 12 = Movie Preview 13 = Panning 14 = Simple 15 = Color Effects 16 = Self Portrait 17 = Economy 18 = Fireworks 19 = Party 20 = Snow 21 = Night Scenery 22 = Food 23 = Baby 24 = Soft Skin 25 = Candlelight 26 = Starry Night 27 = High Sensitivity 28 = Panorama Assist 29 = Underwater 30 = Beach 31 = Aerial Photo 32 = Sunset 33 = Pet 34 = Intelligent ISO 35 = Clipboard 36 = High Speed Continuous Shooting 37 = Intelligent Auto 39 = Multi-aspect 41 = Transform 42 = Flash Burst |  | 43 = Pin Hole 44 = Film Grain 45 = My Color 46 = Photo Frame 48 = Movie 51 = HDR 52 = Peripheral Defocus 55 = Handheld Night Shot 57 = 3D 59 = Creative Control 60 = Intelligent Auto Plus 62 = Panorama 63 = Glass Through 64 = HDR 66 = Digital Filter 67 = Clear Portrait 68 = Silky Skin 69 = Backlit Softness 70 = Clear in Backlight 71 = Relaxing Tone 72 = Sweet Child's Face 73 = Distinct Scenery 74 = Bright Blue Sky 75 = Romantic Sunset Glow 76 = Vivid Sunset Glow 77 = Glistening Water 78 = Clear Nightscape 79 = Cool Night Sky 80 = Warm Glowing Nightscape 81 = Artistic Nightscape 82 = Glittering Illuminations 83 = Clear Night Portrait 84 = Soft Image of a Flower 85 = Appetizing Food 86 = Cute Dessert 87 = Freeze Animal Motion 88 = Clear Sports Shot 89 = Monochrome 90 = Creative Control 92 = Handheld Night Shot
> 0x8002 | HighlightWarning | int16u | 0 = Disabled 1 = No 2 = Yes
> 0x8003 | DarkFocusEnvironment | int16u | 1 = No 2 = Yes
> 0x8004 | WBRedLevel | int16u |
> 0x8005 | WBGreenLevel | int16u |
> 0x8006 | WBBlueLevel | int16u |
> 0x8008 | TextStamp | int16u | 1 = Off 2 = On
> 0x8009 | TextStamp | int16u | 1 = Off 2 = On
> 0x8010 | BabyAge | string | (or pet age)
> 0x8012 | Transform | undef[4] | (decoded as two 16-bit signed integers) '-1 1' = Slim Low '-3 2' = Slim High '0 0' = Off '1 1' = Stretch Low '3 2' = Stretch High

## Panasonic DSA Tags

XMP Digital Shift Assistant tags written by some Leica cameras.

These tags belong to the ExifTool XMP-xmpDSA family 1 group.

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> ApplyAutomatically | boolean/ |
> CorrectionAlreadyApplied | boolean/ |
> FocalLength35mm | real/ |
> NormalizedCropCorners | real/+ |
> PitchAngle | real/ |
> RollAngle | real/ |
> ScalingFactorHeight | real/ |
> TargetAspectRatio | real/ |
> ValidCropCorners | boolean/ |
> Version | string/ |

## Panasonic FaceDetInfo Tags

Face detection position information.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | NumFacePositions | int16u | (number of detected face positions stored in this record. May be less than FacesDetected)
> 1 | Face1Position | int16u[4] | (4 numbers: X/Y coordinates of the face center and width/height of face. Coordinates are relative to an image twice the size of the thumbnail, or 320 pixels wide)
> 5 | Face2Position | int16u[4] |
> 9 | Face3Position | int16u[4] |
> 13 | Face4Position | int16u[4] |
> 17 | Face5Position | int16u[4] |

## Panasonic FaceRecInfo Tags

Tags written by cameras with facial recognition. These cameras not only detect faces in an image, but also recognize specific people based a user-supplied set of known faces.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FacesRecognized | int16u |
> 4 | RecognizedFace1Name | string[20] |
> 24 | RecognizedFace1Position | int16u[4] | (coordinates in same format as face detection tags above)
> 32 | RecognizedFace1Age | string[20] |
> 52 | RecognizedFace2Name | string[20] |
> 72 | RecognizedFace2Position | int16u[4] |
> 80 | RecognizedFace2Age | string[20] |
> 100 | RecognizedFace3Name | string[20] |
> 120 | RecognizedFace3Position | int16u[4] |
> 128 | RecognizedFace3Age | string[20] |

## Panasonic TimeInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PanasonicDateTime | undef[8] |
> 16 | TimeLapseShotNumber | int32u |

## Panasonic Leica2 Tags

These tags are used by the Leica M8.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0300 | Quality | int16u | 1 = Fine 2 = Basic
> 0x0302 | UserProfile | int32u | 1 = User Profile 1 2 = User Profile 2 3 = User Profile 3 4 = User Profile 0 (Dynamic)
> 0x0303 | SerialNumber | int32u |
> 0x0304 | WhiteBalance | int16u | (values above 0x8000 are converted to Kelvin color temperatures)
> 0 = Auto or Manual 1 = Daylight 2 = Fluorescent 3 = Tungsten |  | 4 = Flash 10 = Cloudy 11 = Shade
> 0x0310 | LensType | int32u | --> Panasonic LensType Values
> 0x0311 | ExternalSensorBrightnessValue | rational64s | ("blue dot" measurement)
> 0x0312 | MeasuredLV | rational64s | (imaging sensor or TTL exposure meter measurement)
> 0x0313 | ApproximateFNumber | rational64u |
> 0x0320 | CameraTemperature | int32s |
> 0x0321 | ColorTemperature | int32u |
> 0x0322 | WBRedLevel | rational64u |
> 0x0323 | WBGreenLevel | rational64u |
> 0x0324 | WBBlueLevel | rational64u |
> 0x0325 | UV-IRFilterCorrection | int32u | 0 = Not Active 1 = Active
> 0x0330 | CCDVersion | int32u |
> 0x0331 | CCDBoardVersion | int32u |
> 0x0332 | ControllerBoardVersion | int32u |
> 0x0333 | M16CVersion | int32u |
> 0x0340 | ImageIDNumber | int32u |

## Panasonic LensType Values

the LensType value is obtained by splitting the stored value into 2 integers: The stored value divided by 4, and its lower 2 bits. The second number is used only if necessary to identify certain manually coded lenses on the M9, or the focal length of some multi-focal lenses.

> Value | LensType | Value | LensType
> --- | --- | --- | ---
> 1 | = Elmarit-M 21mm f/2.8 | 42 | = Tri-Elmar-M 28-35-50mm f/4 ASPH.
> 3 | = Elmarit-M 28mm f/2.8 (III) | 43 | = Summarit-M 35mm f/2.5
> 4 | = Tele-Elmarit-M 90mm f/2.8 (II) | 44 | = Summarit-M 50mm f/2.5
> 5 | = Summilux-M 50mm f/1.4 (II) | 45 | = Summarit-M 75mm f/2.5
> 6 | = Summicron-M 35mm f/2 (IV) | 46 | = Summarit-M 90mm f/2.5
> 7 | = Summicron-M 90mm f/2 (II) | 47 | = Summilux-M 21mm f/1.4 ASPH.
> 9 | = Elmarit-M 135mm f/2.8 (I/II) | 48 | = Summilux-M 24mm f/1.4 ASPH.
> 11 | = Summaron-M 28mm f/5.6 | 49 | = Noctilux-M 50mm f/0.95 ASPH.
> 12 | = Thambar-M 90mm f/2.2 | 50 | = Elmar-M 24mm f/3.8 ASPH.
> 16 | = Tri-Elmar-M 16-18-21mm f/4 ASPH. | 51 | = Super-Elmar-M 21mm f/3.4 Asph
> 23 | = Summicron-M 50mm f/2 (III) | 52 | = Apo-Telyt-M 18mm f/3.8 ASPH.
> 24 | = Elmarit-M 21mm f/2.8 ASPH. | 53 | = Apo-Telyt-M 135mm f/3.4
> 25 | = Elmarit-M 24mm f/2.8 ASPH. | 58 | = Noctilux-M 75mm f/1.25 ASPH.
> 26 | = Summicron-M 28mm f/2 ASPH. | '0 0' | = Uncoded lens
> 27 | = Elmarit-M 28mm f/2.8 (IV) | '6 0' | = Summilux-M 35mm f/1.4
> 28 | = Elmarit-M 28mm f/2.8 ASPH. | '9 0' | = Apo-Telyt-M 135mm f/3.4
> 29 | = Summilux-M 35mm f/1.4 ASPH. | '16 1' | = Tri-Elmar-M 16-18-21mm f/4 ASPH. (at 16mm)
> 30 | = Summicron-M 35mm f/2 ASPH. | '16 2' | = Tri-Elmar-M 16-18-21mm f/4 ASPH. (at 18mm)
> 31 | = Noctilux-M 50mm f/1 | '16 3' | = Tri-Elmar-M 16-18-21mm f/4 ASPH. (at 21mm)
> 32 | = Summilux-M 50mm f/1.4 ASPH. | '29 0' | = Summilux-M 35mm f/1.4 ASPHERICAL
> 33 | = Summicron-M 50mm f/2 (IV, V) | '31 0' | = Noctilux-M 50mm f/1.2
> 34 | = Elmar-M 50mm f/2.8 | '39 0' | = Tele-Elmar-M 135mm f/4 (II)
> 35 | = Summilux-M 75mm f/1.4 | '41 3' | = Apo-Summicron-M 50mm f/2 ASPH.
> 36 | = Apo-Summicron-M 75mm f/2 ASPH. | '42 1' | = Tri-Elmar-M 28-35-50mm f/4 ASPH. (at 28mm)
> 37 | = Apo-Summicron-M 90mm f/2 ASPH. | '42 2' | = Tri-Elmar-M 28-35-50mm f/4 ASPH. (at 35mm)
> 38 | = Elmarit-M 90mm f/2.8 | '42 3' | = Tri-Elmar-M 28-35-50mm f/4 ASPH. (at 50mm)
> 39 | = Macro-Elmar-M 90mm f/4 | '51 2' | = Super-Elmar-M 14mm f/3.8 Asph
> 40 | = Macro-Adapter M | '53 2' | = Apo-Telyt-M 135mm f/3.4
> 41 | = Apo-Summicron-M 50mm f/2 ASPH. | '53 3' | = Apo-Summicron-M 50mm f/2 (VI)

## Panasonic Leica3 Tags

These tags are used by the Leica R8 and R9 digital backs.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x000b | SerialInfo | - | --> Panasonic SerialInfo Tags
> 0x000d | WB_RGBLevels | int16u[3] |

## Panasonic SerialInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | SerialNumber | no |

## Panasonic Leica4 Tags

This information is written by the M9.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x3000 | Subdir3000 | - | --> Panasonic Subdir Tags
> 0x3100 | Subdir3100 | - | --> Panasonic Subdir Tags
> 0x3400 | Subdir3400 | - | --> Panasonic Subdir Tags
> 0x3900 | Subdir3900 | - | --> Panasonic Subdir Tags

## Panasonic Subdir Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x300a | Contrast | int32u | 0 = Low 1 = Medium Low 2 = Normal 3 = Medium High 4 = High
> 0x300b | Sharpening | int32u | 0 = Off 1 = Low 2 = Normal 3 = Medium High 4 = High
> 0x300d | Saturation | int32u |
> 0 = Low 1 = Medium Low 2 = Normal 3 = Medium High |  | 4 = High 5 = Black & White 6 = Vintage B&W
> 0x3033 | WhiteBalance | int32u |
> 0 = Auto 1 = Tungsten 2 = Fluorescent 3 = Daylight Fluorescent 4 = Daylight 5 = Flash 6 = Cloudy 7 = Shade 8 = Manual 9 = Kelvin
> 0x3034 | JPEGQuality | int32u | 94 = Basic 97 = Fine
> 0x3036 | WB_RGBLevels | rational64u[3] |
> 0x3038 | UserProfile | string |
> 0x303a | JPEGSize | int32u | 0 = 5216x3472 1 = 3840x2592 2 = 2592x1728 3 = 1728x1152 4 = 1280x864
> 0x3103 | SerialNumber | string |
> 0x3109 | FirmwareVersion | string |
> 0x312a | BaseISO | int32u |
> 0x312b | SensorWidth | int32u |
> 0x312c | SensorHeight | int32u |
> 0x312d | SensorBitDepth | int32u |
> 0x3402 | CameraTemperature | int32s |
> 0x3405 | LensType | int32u | --> Panasonic LensType Values
> 0x3406 | ApproximateFNumber | rational64u |
> 0x3407 | MeasuredLV | int32s | (imaging sensor or TTL exposure meter measurement)
> 0x3408 | ExternalSensorBrightnessValue | int32s | ("blue dot" measurement)
> 0x3901 | Data1 | - | --> Panasonic Data1 Tags
> 0x3902 | Data2 | - | --> Panasonic Data2 Tags

## Panasonic Data1 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 22 | LensType | int32u | --> Panasonic LensType Values

## Panasonic Data2 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Panasonic Leica5 Tags

This information is written by the X1, X2, X VARIO and T.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0303 | LensType | string | (Leica T only)
> 0x0305 | SerialNumber | int32u |
> 0x0407 | OriginalFileName | string |
> 0x0408 | OriginalDirectory | string |
> 0x040a | FocusInfo | - | --> Panasonic FocusInfo Tags
> 0x040d | ExposureMode | int8u[4] | '0 0 0 0' = Program AE '1 0 0 0' = Aperture-priority AE '1 1 0 0' = Aperture-priority AE (1) '2 0 0 0' = Shutter speed priority AE '3 0 0 0' = Manual
> 0x0410 | ShotInfo | - | --> Panasonic ShotInfo Tags
> 0x0412 | FilmMode | string |
> 0x0413 | WB_RGBLevels | rational64u[3] |
> 0x0500 | InternalSerialNumber | undef |
> 0x05ff | CameraIFD | - | --> PanasonicRaw CameraIFD Tags

## Panasonic FocusInfo Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FocusDistance | int16u |
> 1 | FocalLength | int16u |

## Panasonic ShotInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FileIndex | int16u |

## Panasonic Leica6 Tags

This information is written by the S2 and M (Typ 240), as a trailer in JPEG images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0300 | PreviewImage | undef | (S2 and M (Typ 240))
> 0x0301 | UnknownBlock? | no | (unknown 320kB block, not copied to JPEG images)
> 0x0303 | LensType | string |
> 0x0304 | FocusDistance | int32u | (focus distance in mm for most models, but cm for others)
> 0x0311 | ExternalSensorBrightnessValue | rational64s | (Leica S only)
> 0x0312 | MeasuredLV | rational64s | (Leica S only)
> 0x0320 | FirmwareVersion | int8u[4] | (Leica S only)
> 0x0321 | LensSerialNumber | int32u | (Leica S only)

## Panasonic Leica9 Tags

This information is written by the Leica S (Typ 007) and M10 models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0304 | FocusDistance | int32u | (focus distance in mm for most models, but cm for others)
> 0x0311 | ExternalSensorBrightnessValue | rational64s |
> 0x0312 | MeasuredLV | rational64s |
> 0x034c | UserProfile | string |
> 0x0359 | ISOSelected | int32s | 0 = Auto
> 0x035a | FNumber | int32s |
> 0x035b | CorrelatedColorTemp | int16u |
> 0x035c | ColorTint | int16s |
> 0x035d | WhitePoint | rational64u[2] |
> 0x0370 | LensProfileName | string |

## Panasonic Type2 Tags

This type of maker notes is used by models such as the NV-DS65, PV-D2002, PV-DC3000, PV-DV203, PV-DV401, PV-DV702, PV-L2001, PV-SD4090, PV-SD5000 and iPalm.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteType | no |
> 3 | Gain | no |

## Panasonic PANA Tags

Tags extracted from the PANA and LEIC user data found in MP4 videos from various Panasonic and Leica models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | no |
> 4 | Model | no |
> 12 | Model | no |
> 16 | JPEG-likeData | - | --> EXIF Tags
> 22 | Model | no |
> 52 | Version1 | no |
> 62 | Version2 | no |
> 80 | MakerNoteLeica5 | - | --> Panasonic Leica5 Tags
> 88 | ThumbnailWidth | no | (Panasonic models)
> 90 | ThumbnailHeight | no |
> 92 | ThumbnailImage | no |
> 1334 | ThumbnailWidth | no | (Leica X Vario)
> 1338 | ThumbnailHeight | no |
> 1342 | ThumbnailLength | no |
> 1350 | ThumbnailImage | no |
> 1358 | ThumbnailWidth | no | (Leica X Vario)
> 1362 | ThumbnailHeight | no |
> 1366 | ThumbnailLength | no |
> 1374 | ThumbnailImage | no |
> 16488 | ExifData | - | --> EXIF Tags
> 16512 | ExifData | - | --> EXIF Tags
> 0x00200080 | ExifData | - | --> EXIF Tags

## Panasonic AdvancedSceneMode Values

A Composite tag derived from Model, SceneMode and AdvancedSceneType.

> Value | AdvancedSceneMode | Value | AdvancedSceneMode
> --- | --- | --- | ---
> '0 1' | = Off | '59 1' | = Expressive
> '2 2' | = Outdoor Portrait | '59 2' | = Retro
> '2 3' | = Indoor Portrait | '59 3' | = High Key
> '2 4' | = Creative Portrait | '59 4' | = Sepia
> '3 2' | = Nature | '59 5' | = High Dynamic
> '3 3' | = Architecture | '59 6' | = Miniature
> '3 4' | = Creative Scenery | '59 9' | = Low Key
> '4 2' | = Outdoor Sports | '59 10' | = Toy Effect
> '4 3' | = Indoor Sports | '59 11' | = Dynamic Monochrome
> '4 4' | = Creative Sports | '59 12' | = Soft
> '9 2' | = Flower | '66 1' | = Impressive Art
> '9 3' | = Objects | '66 2' | = Cross Process
> '9 4' | = Creative Macro | '66 3' | = Color Select
> '18 1' | = High Sensitivity | '66 4' | = Star
> '20 1' | = Fireworks | '90 3' | = Old Days
> '21 2' | = Illuminations | '90 4' | = Sunshine
> '21 4' | = Creative Night Scenery | '90 5' | = Bleach Bypass
> '26 1' | = High-speed Burst (shot 1) | '90 6' | = Toy Pop
> '27 1' | = High-speed Burst (shot 2) | '90 7' | = Fantasy
> '29 1' | = Snow | '90 8' | = Monochrome
> '30 1' | = Starry Sky | '90 9' | = Rough Monochrome
> '31 1' | = Beach | '90 10' | = Silky Monochrome
> '36 1' | = High-speed Burst (shot 3) | '92 1' | = Handheld Night Shot
> '39 1' | = Aerial Photo / Underwater / Multi-aspect | 'DMC-TZ40 90 1' | = Expressive
> '45 2' | = Cinema | 'DMC-TZ40 90 2' | = Retro
> '45 7' | = Expressive | 'DMC-TZ40 90 3' | = High Key
> '45 8' | = Retro | 'DMC-TZ40 90 4' | = Sepia
> '45 9' | = Pure | 'DMC-TZ40 90 5' | = High Dynamic
> '45 10' | = Elegant | 'DMC-TZ40 90 6' | = Miniature
> '45 12' | = Monochrome | 'DMC-TZ40 90 9' | = Low Key
> '45 13' | = Dynamic Art | 'DMC-TZ40 90 10' | = Toy Effect
> '45 14' | = Silhouette | 'DMC-TZ40 90 11' | = Dynamic Monochrome
> '51 2' | = HDR Art | 'DMC-TZ40 90 12' | = Soft
> '51 3' | = HDR B&W |  |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Dec 10, 2025

<-- ExifTool Tag Names