## FujiFilm Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | Version | undef |
> 0x0010 | InternalSerialNumber | string | (this number is unique for most models, and contains the camera model ID and the date of manufacture)
> 0x1000 | Quality | string |
> 0x1001 | Sharpness | int16u |
> 0x0 = -4 (softest) 0x1 = -3 (very soft) 0x2 = -2 (soft) 0x3 = 0 (normal) 0x4 = +2 (hard) 0x5 = +3 (very hard) 0x6 = +4 (hardest) 0x82 = -1 (medium soft) 0x84 = +1 (medium hard) 0x8000 = Film Simulation 0xffff = n/a
> 0x1002 | WhiteBalance | int16u |
> 0x0 = Auto 0x1 = Auto (white priority) 0x2 = Auto (ambiance priority) 0x100 = Daylight 0x200 = Cloudy 0x300 = Daylight Fluorescent 0x301 = Day White Fluorescent 0x302 = White Fluorescent 0x303 = Warm White Fluorescent 0x304 = Living Room Warm White Fluorescent 0x400 = Incandescent 0x500 = Flash 0x600 = Underwater 0xf00 = Custom 0xf01 = Custom2 0xf02 = Custom3 0xf03 = Custom4 0xf04 = Custom5 0xff0 = Kelvin
> 0x1003 | Saturation | int16u |
> 0x0 = 0 (normal) 0x80 = +1 (medium high) 0xc0 = +3 (very high) 0xe0 = +4 (highest) 0x100 = +2 (high) 0x180 = -1 (medium low) 0x200 = Low 0x300 = None (B&W) 0x301 = B&W Red Filter 0x302 = B&W Yellow Filter 0x303 = B&W Green Filter 0x310 = B&W Sepia 0x400 = -2 (low) 0x4c0 = -3 (very low) 0x4e0 = -4 (lowest) 0x500 = Acros 0x501 = Acros Red Filter 0x502 = Acros Yellow Filter 0x503 = Acros Green Filter 0x8000 = Film Simulation
> 0x1004 | Contrast | int16u |
> 0x0 = Normal 0x80 = Medium High 0x100 = High 0x180 = Medium Low 0x200 = Low 0x8000 = Film Simulation
> 0x1005 | ColorTemperature | int16u |
> 0x1006 | Contrast | int16u | 0x0 = Normal 0x100 = High 0x300 = Low
> 0x100a | WhiteBalanceFineTune | int32s[2] | (newer cameras should divide these values by 20)
> 0x100b | NoiseReduction | int16u | 0x40 = Low 0x80 = Normal 0x100 = n/a
> 0x100e | NoiseReduction | int16u |
> 0x0 = 0 (normal) 0x100 = +2 (strong) 0x180 = +1 (medium strong) 0x1c0 = +3 (very strong) 0x1e0 = +4 (strongest) 0x200 = -2 (weak) 0x280 = -1 (medium weak) 0x2c0 = -3 (very weak) 0x2e0 = -4 (weakest)
> 0x100f | Clarity | int32s |
> -5000 = -5 -4000 = -4 -3000 = -3 -2000 = -2 |  | -1000 = -1 0 = 0 1000 = 1 2000 = 2 |  | 3000 = 3 4000 = 4 5000 = 5
> 0x1010 | FujiFlashMode | int16u | 0x0 = Auto 0x1 = On 0x2 = Off 0x3 = Red-eye reduction 0x4 = External 0x10 = Commander 0x8000 = Not Attached 0x8120 = TTL 0x8320 = TTL Auto - Did not fire 0x9840 = Manual 0x9860 = Flash Commander 0x9880 = Multi-flash 0xa920 = 1st Curtain (front) 0xaa20 = TTL Slow - 1st Curtain (front) 0xab20 = TTL Auto - 1st Curtain (front) 0xad20 = TTL - Red-eye Flash - 1st Curtain (front) 0xae20 = TTL Slow - Red-eye Flash - 1st Curtain (front) 0xaf20 = TTL Auto - Red-eye Flash - 1st Curtain (front) 0xc920 = 2nd Curtain (rear) 0xca20 = TTL Slow - 2nd Curtain (rear) 0xcb20 = TTL Auto - 2nd Curtain (rear) 0xcd20 = TTL - Red-eye Flash - 2nd Curtain (rear) 0xce20 = TTL Slow - Red-eye Flash - 2nd Curtain (rear) 0xcf20 = TTL Auto - Red-eye Flash - 2nd Curtain (rear) 0xe920 = High Speed Sync (HSS)
> 0x1011 | FlashExposureComp | rational64s |
> 0x1020 | Macro | int16u | 0 = Off 1 = On
> 0x1021 | FocusMode | int16u | 0 = Auto 1 = Manual 65535 = Movie
> 0x1022 | AFMode | int16u | ("No" for manual and some AF-multi focus modes) 0 = No 1 = Single Point 256 = Zone 512 = Wide/Tracking
> 0x1023 | FocusPixel | int16u[2] |
> 0x102b | PrioritySettings | - | --> FujiFilm PrioritySettings Tags
> 0x102d | FocusSettings | - | --> FujiFilm FocusSettings Tags
> 0x102e | AFCSettings | - | --> FujiFilm AFCSettings Tags
> 0x1030 | SlowSync | int16u | 0 = Off 1 = On
> 0x1031 | PictureMode | int16u |
> 0x0 = Auto 0x1 = Portrait 0x2 = Landscape 0x3 = Macro 0x4 = Sports 0x5 = Night Scene 0x6 = Program AE 0x7 = Natural Light 0x8 = Anti-blur 0x9 = Beach & Snow 0xa = Sunset 0xb = Museum 0xc = Party 0xd = Flower 0xe = Text 0xf = Natural Light & Flash 0x10 = Beach 0x11 = Snow 0x12 = Fireworks 0x13 = Underwater 0x14 = Portrait with Skin Correction 0x16 = Panorama 0x17 = Night (tripod) 0x18 = Pro Low-light 0x19 = Pro Focus 0x1a = Portrait 2 0x1b = Dog Face Detection 0x1c = Cat Face Detection 0x30 = HDR 0x40 = Advanced Filter 0x100 = Aperture-priority AE 0x200 = Shutter speed priority AE 0x300 = Manual
> 0x1032 | ExposureCount | int16u | (number of exposures used for this image)
> 0x1033 | EXRAuto | int16u | 0 = Auto 1 = Manual
> 0x1034 | EXRMode | int16u | 0x100 = HR (High Resolution) 0x200 = SN (Signal to Noise priority) 0x300 = DR (Dynamic Range priority)
> 0x1037 | MultipleExposure | int16u | 1 = Additive 2 = Average 3 = Light 4 = Dark
> 0x1040 | ShadowTone | int32s |
> -64 = +4 (hardest) -48 = +3 (very hard) -32 = +2 (hard) -16 = +1 (medium hard) |  | 0 = 0 (normal) 16 = -1 (medium soft) 32 = -2 (soft)
> 0x1041 | HighlightTone | int32s |
> -64 = +4 (hardest) -48 = +3 (very hard) -32 = +2 (hard) -16 = +1 (medium hard) |  | 0 = 0 (normal) 16 = -1 (medium soft) 32 = -2 (soft)
> 0x1044 | DigitalZoom | int32u |
> 0x1045 | LensModulationOptimizer | int32u | 0 = Off 1 = On
> 0x1047 | GrainEffectRoughness | int32s | 0 = Off 32 = Weak 64 = Strong
> 0x1048 | ColorChromeEffect | int32s | 0 = Off 32 = Weak 64 = Strong
> 0x1049 | BWAdjustment | int8s | (positive values are warm, negative values are cool)
> 0x104b | BWMagentaGreen | int8s | (positive values are green, negative values are magenta)
> 0x104c | GrainEffectSize | int16u | 0 = Off 16 = Small 32 = Large
> 0x104d | CropMode | int16u | 0 = n/a 1 = Full-frame on GFX 2 = Sports Finder Mode 4 = Electronic Shutter 1.25x Crop 8 = Digital Tele-Conv
> 0x104e | ColorChromeFXBlue | int32s | 0 = Off 32 = Weak 64 = Strong
> 0x1050 | ShutterType | int16u | 0 = Mechanical 1 = Electronic 2 = Electronic (long shutter speed) 3 = Electronic Front Curtain
> 0x1051 | CropFlag | int8u | (this tag exists only if the image was cropped, and is 0 for cropped JPG image or 1 for a cropped RAF)
> 0x1052 | CropTopLeft | int32u |
> 0x1053 | CropSize | int32u |
> 0x1100 | AutoBracketing | int16u | (X-T3 only) 0 = Off 1 = On 2 = Pre-shot (other models) 0 = Off 1 = On 2 = No flash & flash 6 = Pixel Shift
> 0x1101 | SequenceNumber | int16u |
> 0x1102 | WhiteBalanceBracketing | int16u | 0x1ff = +/- 1 0x2ff = +/- 2 0x3ff = +/- 3
> 0x1103 | DriveSettings | - | --> FujiFilm DriveSettings Tags
> 0x1105 | PixelShiftShots | int16u |
> 0x1106 | PixelShiftOffset | rational64s[2] |
> 0x1150 | CompositeImageMode | int32u |
> 0 = n/a 1 = Pro Low-light 2 = Pro Focus |  | 32 = Panorama 128 = HDR 1024 = Multi-exposure
> 0x1151 | CompositeImageCount1 | int16u |
> 0x1152 | CompositeImageCount2 | int16u |
> 0x1153 | PanoramaAngle | int16u |
> 0x1154 | PanoramaDirection | int16u | 1 = Right 2 = Left 3 = Up 4 = Down
> 0x1201 | AdvancedFilter | int32u |
> 0x10000 = Pop Color 0x20000 = Hi Key 0x30000 = Toy Camera 0x40000 = Miniature 0x50000 = Dynamic Tone 0x60001 = Partial Color Red 0x60002 = Partial Color Yellow 0x60003 = Partial Color Green 0x60004 = Partial Color Blue 0x60005 = Partial Color Orange 0x60006 = Partial Color Purple 0x70000 = Soft Focus 0x90000 = Low Key 0x100000 = Light Leak 0x130000 = Expired Film Green 0x130001 = Expired Film Red 0x130002 = Expired Film Neutral
> 0x1210 | ColorMode | int16u | 0x0 = Standard 0x10 = Chrome 0x30 = B & W
> 0x1300 | BlurWarning | int16u | 0 = None 1 = Blur Warning
> 0x1301 | FocusWarning | int16u | 0 = Good 1 = Out of focus
> 0x1302 | ExposureWarning | int16u | 0 = Good 1 = Bad exposure
> 0x1304 | GEImageSize | string | (GE models only)
> 0x1400 | DynamicRange | int16u | 1 = Standard 3 = Wide
> 0x1401 | FilmMode | int16u | 0x0 = F0/Standard (Provia) 0x100 = F1/Studio Portrait 0x110 = F1a/Studio Portrait Enhanced Saturation 0x120 = F1b/Studio Portrait Smooth Skin Tone (Astia) 0x130 = F1c/Studio Portrait Increased Sharpness 0x200 = F2/Fujichrome (Velvia) 0x300 = F3/Studio Portrait Ex 0x400 = F4/Velvia 0x500 = Pro Neg. Std 0x501 = Pro Neg. Hi 0x600 = Classic Chrome 0x700 = Eterna 0x800 = Classic Negative 0x900 = Bleach Bypass 0xa00 = Nostalgic Neg 0xb00 = Reala ACE
> 0x1402 | DynamicRangeSetting | int16u |
> 0x0 = Auto 0x1 = Manual 0x100 = Standard (100%) 0x200 = Wide1 (230%) 0x201 = Wide2 (400%) 0x8000 = Film Simulation
> 0x1403 | DevelopmentDynamicRange | int16u |
> 0x1404 | MinFocalLength | rational64s |
> 0x1405 | MaxFocalLength | rational64s |
> 0x1406 | MaxApertureAtMinFocal | rational64s |
> 0x1407 | MaxApertureAtMaxFocal | rational64s |
> 0x140b | AutoDynamicRange | int16u |
> 0x1422 | ImageStabilization | int16u[3] | [Value 0]
> 0 = None 1 = Optical 2 = Sensor-shift |  | 3 = OIS Lens 258 = IBIS/OIS + DIS 512 = Digital
> [Value 1] 0 = Off 1 = On (mode 1, continuous) 2 = On (mode 2, shooting only)
> 0x1425 | SceneRecognition | int16u |
> 0x0 = Unrecognized 0x100 = Portrait Image 0x103 = Night Portrait 0x105 = Backlit Portrait 0x200 = Landscape Image 0x300 = Night Scene 0x400 = Macro
> 0x1431 | Rating | int32u |
> 0x1436 | ImageGeneration | int16u | 0 = Original Image 1 = Re-developed from RAW
> 0x1438 | ImageCount | int16u | (may reset to 0 when new firmware is installed)
> 0x1443 | DRangePriority | int16u | 0 = Auto 1 = Fixed
> 0x1444 | DRangePriorityAuto | int16u | 1 = Weak 2 = Strong 3 = Plus
> 0x1445 | DRangePriorityFixed | int16u | 1 = Weak 2 = Strong
> 0x1446 | FlickerReduction | int32u |
> 0x1447 | FujiModel | string |
> 0x1448 | FujiModel2 | string |
> 0x144a | WBRed | int16u |
> 0x144b | WBGreen | int16u |
> 0x144c | WBBlue | int16u |
> 0x144d | RollAngle | rational64s |
> 0x3803 | VideoRecordingMode | int32u | 0x0 = Normal 0x10 = F-log 0x20 = HLG 0x30 = F-log2
> 0x3804 | PeripheralLighting | int16u | 0 = Off 1 = On
> 0x3806 | VideoCompression | int16u | 1 = Log GOP 2 = All Intra
> 0x3820 | FrameRate | int16u |
> 0x3821 | FrameWidth | int16u |
> 0x3822 | FrameHeight | int16u |
> 0x3824 | FullHDHighSpeedRec | int32u | 1 = Off 2 = On
> 0x4005 | FaceElementSelected | int16u[4] |
> 0x4100 | FacesDetected | int16u |
> 0x4103 | FacePositions | int16u[n] | (left, top, right and bottom coordinates in full-sized image for each face detected)
> 0x4200 | NumFaceElements | int16u |
> 0x4201 | FaceElementTypes | int8u[n] | [Values 0-N]
> 1 = Face 2 = Left Eye 3 = Right Eye 7 = Body 8 = Head 9 = Both Eyes 11 = Bike 12 = Body of Car 13 = Front of Car 14 = Animal Body 15 = Animal Head 16 = Animal Face |  | 17 = Animal Left Eye 18 = Animal Right Eye 19 = Bird Body 20 = Bird Head 21 = Bird Left Eye 22 = Bird Right Eye 23 = Aircraft Body 25 = Aircraft Cockpit 26 = Train Front 27 = Train Cockpit 28 = Animal Head (28) 29 = Animal Body (29)
> 0x4203 | FaceElementPositions | int16u[n] | (left, top, right and bottom coordinates in full-sized image for each face element)
> 0x4282 | FaceRecInfo | - | --> FujiFilm FaceRecInfo Tags
> 0x8000 | FileSource | string |
> 0x8002 | OrderNumber | int32u |
> 0x8003 | FrameNumber | int16u |
> 0xb211 | Parallax | rational64s | (only found in MPImage2 of .MPO images)

## FujiFilm PrioritySettings Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | AF-SPriority | int16u | [val & 0xf] 1 = Release 2 = Focus
> 0.2 | AF-CPriority | int16u | [val >> 4 & 0xf] 1 = Release 2 = Focus

## FujiFilm FocusSettings Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | FocusMode2 | int32u | [val & 0xf] 0 = AF-M 1 = AF-S 2 = AF-C
> 0.2 | PreAF | int32u | [val >> 4 & 0xf] 0 = Off 1 = On
> 0.3 | AFAreaMode | int32u | [val >> 8 & 0xf] 0 = Single Point 1 = Zone 2 = Wide/Tracking
> 0.4 | AFAreaPointSize | int32u | [val >> 12 & 0xf] 0 = n/a
> 0.5 | AFAreaZoneSize | int32u | [val >> 16 & 0xff] 0 = n/a

## FujiFilm AFCSettings Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AF-CSetting | int32u | 0x102 = Set 1 (multi-purpose) 0x203 = Set 2 (ignore obstacles) 0x122 = Set 3 (accelerating subject) 0x010 = Set 4 (suddenly appearing subject) 0x123 = Set 5 (erratic motion)
> 0.1 | AF-CTrackingSensitivity | int32u | [val & 0xf]
> 0.2 | AF-CSpeedTrackingSensitivity | int32u | [val >> 4 & 0xf]
> 0.3 | AF-CZoneAreaSwitching | int32u | [val >> 8 & 0xf] 0 = Front 1 = Auto 2 = Center

## FujiFilm DriveSettings Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0.1 | DriveMode | int32u | [val & 0xff] 0 = Single 1 = Continuous Low 2 = Continuous High
> 0.2 | DriveSpeed | int32u | [val >> 24 & 0xff] 0 = n/a

## FujiFilm FaceRecInfo Tags

Face recognition information.

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> Face1Birthday | no |
> Face1Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face1Name | no |
> Face2Birthday | no |
> Face2Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face2Name | no |
> Face3Birthday | no |
> Face3Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face3Name | no |
> Face4Birthday | no |
> Face4Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face4Name | no |
> Face5Birthday | no |
> Face5Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face5Name | no |
> Face6Birthday | no |
> Face6Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face6Name | no |
> Face7Birthday | no |
> Face7Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face7Name | no |
> Face8Birthday | no |
> Face8Category | no | Bit 1 = Partner Bit 2 = Family Bit 3 = Friend
> Face8Name | no |

## FujiFilm RAFHeader Tags

Tags extracted from the header of RAF images.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 60 | FirmwareVersion | no |
> 108 | RAFCompression | no | 0 = Uncompressed 2 = Lossless 3 = Lossy

## FujiFilm RAF Tags

FujiFilm RAF images contain meta information stored in a proprietary FujiFilm RAF format, as well as EXIF information stored inside an embedded JPEG preview image. The table below lists tags currently decoded from the RAF-format information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0100 | RawImageFullSize | no | (including borders)
> 0x0110 | RawImageCropTopLeft | no | (top margin first, then left margin)
> 0x0111 | RawImageCroppedSize | no | (including borders)
> 0x0115 | RawImageAspectRatio | no |
> 0x0117 | RawZoomActive | no | 0 = No 1 = Yes
> 0x0118 | RawZoomTopLeft | no | (relative to RawCroppedImageSize)
> 0x0119 | RawZoomSize | no | (relative to RawCroppedImageSize)
> 0x0121 | RawImageSize | no |
> 0x0130 | FujiLayout | no |
> 0x0131 | XTransLayout | no |
> 0x2000 | WB_GRGBLevelsAuto | no |
> 0x2100 | WB_GRGBLevelsDaylight | no |
> 0x2200 | WB_GRGBLevelsCloudy | no |
> 0x2300 | WB_GRGBLevelsDaylightFluor | no |
> 0x2301 | WB_GRGBLevelsDayWhiteFluor | no |
> 0x2302 | WB_GRGBLevelsWhiteFluorescent | no |
> 0x2310 | WB_GRGBLevelsWarmWhiteFluor | no |
> 0x2311 | WB_GRGBLevelsLivingRoomWarmWhiteFluor | no |
> 0x2400 | WB_GRGBLevelsTungsten | no |
> 0x2ff0 | WB_GRGBLevels | no |
> 0x9200 | RelativeExposure | no |
> 0x9650 | RawExposureBias | no |
> 0xc000 | RAFData | - | --> FujiFilm RAFData Tags

## FujiFilm RAFData Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | RawImageWidth | no |
> 4 | RawImageWidth RawImageHeight | no no |
> 8 | RawImageWidth RawImageHeight | no no |
> 12 | RawImageHeight | no |

## FujiFilm IFD Tags

Tags found in the FujiIFD information of RAF images from some models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0xf000 | FujiIFD | - | --> FujiFilm IFD Tags
> 0xf001 | RawImageFullWidth | no |
> 0xf002 | RawImageFullHeight | no |
> 0xf003 | BitsPerSample | no |
> 0xf007 | StripOffsets | no |
> 0xf008 | StripByteCounts | no |
> 0xf00a | BlackLevel | no |
> 0xf00b | GeometricDistortionParams | no |
> 0xf00c | WB_GRBLevelsStandard | no |
> 0xf00d | WB_GRBLevelsAuto | no |
> 0xf00e | WB_GRBLevels | no |
> 0xf00f | ChromaticAberrationParams | no |
> 0xf010 | VignettingParams | no |

## FujiFilm MRAW Tags

Tags extracted from the M-RAW header of multi-image RAF files. The family 1 group name for these tags is "M-RAW". Additional metadata may be extracted from the embedded RAW images with the ExtractEmbedded option.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x2001 | RawImageNumber | no |
> 0x2005 | ExposureTime | no |
> 0x2006 | FNumber | no |
> 0x2007 | ISO | no |

## FujiFilm FFMV Tags

Information found in the FFMV atom of MOV videos.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MovieStreamName | no |

## FujiFilm MOV Tags

This information is found in MOV videos from some FujiFilm cameras.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | no |
> 24 | Model | no |
> 46 | ExposureTime | no |
> 50 | FNumber | no |
> 58 | ExposureCompensation | no |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised May 1, 2026

<-- ExifTool Tag Names