## PanasonicRaw Tags

These tags are found in IFD0 of Panasonic/Leica RAW, RW2 and RWL images.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | PanasonicRawVersion | undef |
> 0x0002 | SensorWidth | no |
> 0x0003 | SensorHeight | no |
> 0x0004 | SensorTopBorder | no |
> 0x0005 | SensorLeftBorder | no |
> 0x0006 | SensorBottomBorder | no |
> 0x0007 | SensorRightBorder | no |
> 0x0008 | SamplesPerPixel | int16u! |
> 0x0009 | CFAPattern | int16u! | 0 = n/a 1 = [Red,Green][Green,Blue] 2 = [Green,Red][Blue,Green] 3 = [Green,Blue][Red,Green] 4 = [Blue,Green][Green,Red]
> 0x000a | BitsPerSample | int16u! |
> 0x000b | Compression | int16u! | 34316 = Panasonic RAW 1 34826 = Panasonic RAW 2 34828 = Panasonic RAW 3 34830 = Panasonic RAW 4
> 0x000e | LinearityLimitRed | int16u |
> 0x000f | LinearityLimitGreen | int16u |
> 0x0010 | LinearityLimitBlue | int16u |
> 0x0011 | RedBalance | int16u | (found in Digilux 2 RAW images)
> 0x0012 | BlueBalance | int16u |
> 0x0013 | WBInfo | - | --> PanasonicRaw WBInfo Tags
> 0x0017 | ISO | int16u |
> 0x0018 | HighISOMultiplierRed | int16u |
> 0x0019 | HighISOMultiplierGreen | int16u |
> 0x001a | HighISOMultiplierBlue | int16u |
> 0x001b | NoiseReductionParams | undef[n]! | (the camera's default noise reduction setup. The first number is the number of entries, then for each entry there are 4 numbers: an ISO speed, and noise-reduction strengths the R, G and B channels)
> 0x001c | BlackLevelRed | int16u |
> 0x001d | BlackLevelGreen | int16u |
> 0x001e | BlackLevelBlue | int16u |
> 0x0024 | WBRedLevel | int16u |
> 0x0025 | WBGreenLevel | int16u |
> 0x0026 | WBBlueLevel | int16u |
> 0x0027 | WBInfo2 | - | --> PanasonicRaw WBInfo2 Tags
> 0x002d | RawFormat | int16u! |
> 0x002e | JpgFromRaw | undef! | --> JPEG Tags (processed as an embedded document because it contains full EXIF)
> 0x002f | CropTop | int16u |
> 0x0030 | CropLeft | int16u |
> 0x0031 | CropBottom | int16u |
> 0x0032 | CropRight | int16u |
> 0x0037 | ISO | int32u |
> 0x010f | Make | string |
> 0x0110 | Model | string |
> 0x0111 | StripOffsets | no |
> 0x0112 | Orientation | int16u |
> 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW
> 0x0116 | RowsPerStrip | no |
> 0x0117 | StripByteCounts | no |
> 0x0118 | RawDataOffset | no |
> 0x0119 | DistortionInfo | - | --> PanasonicRaw DistortionInfo Tags
> 0x011c | Gamma | int16u |
> 0x0120 | CameraIFD | - | --> PanasonicRaw CameraIFD Tags
> 0x0121 | Multishot | int32u | 0 = Off 65536 = Pixel Shift
> 0x0127 | JpgFromRaw2 | no |
> 0x013b | Artist | string |
> 0x02bc | ApplicationNotes | int8u! | --> XMP Tags
> 0x8298 | Copyright | string |
> 0x83bb | IPTC-NAA | int32u! | --> IPTC Tags
> 0x8769 | ExifOffset | - | --> EXIF Tags
> 0x8825 | GPSInfo | - | --> GPS Tags

## PanasonicRaw CameraIFD Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x1001 | MultishotOn | no | 0 = No 1 = Yes
> 0x1100 | FocusStepNear | no |
> 0x1101 | FocusStepCount | no |
> 0x1102 | FlashFired | no | 0 = No 1 = Yes
> 0x1105 | ZoomPosition | no | (in the range 0-255 for most cameras)
> 0x1200 | LensAttached | no | (many CameraIFD tags are invalid if there is no lens attached) 0 = No 1 = Yes
> 0x1201 | LensTypeMake | no |
> 0x1202 | LensTypeModel | no |
> 0x1203 | FocalLengthIn35mmFormat | no |
> 0x1301 | ApertureValue | no |
> 0x1302 | ShutterSpeedValue | no |
> 0x1303 | SensitivityValue | no |
> 0x1305 | HighISOMode | no | 1 = On 2 = Off
> 0x1412 | FacesDetected | no | 0 = No 1 = Yes
> 0x3200 | WB_CFA0_LevelDaylight | no |
> 0x3201 | WB_CFA1_LevelDaylight | no |
> 0x3202 | WB_CFA2_LevelDaylight | no |
> 0x3203 | WB_CFA3_LevelDaylight | no |
> 0x3300 | WhiteBalanceSet | no | --> PanasonicRaw WhiteBalance Values
> 0x3420 | WB_RedLevelAuto | no |
> 0x3421 | WB_BlueLevelAuto | no |
> 0x3501 | Orientation | no |
> 1 = Horizontal (normal) 2 = Mirror horizontal 3 = Rotate 180 4 = Mirror vertical 5 = Mirror horizontal and rotate 270 CW 6 = Rotate 90 CW 7 = Mirror horizontal and rotate 90 CW 8 = Rotate 270 CW
> 0x3600 | WhiteBalanceDetected | no | --> PanasonicRaw WhiteBalance Values

## PanasonicRaw WhiteBalance Values

> Value | WhiteBalance | Value | WhiteBalance | Value | WhiteBalance
> --- | --- | --- | --- | --- | ---
> 0 | = Auto | 5 | = Flash | 10 | = Custom#3
> 1 | = Daylight | 6 | = n/a | 11 | = Custom#4
> 2 | = Cloudy | 7 | = n/a | 12 | = Shade
> 3 | = Tungsten | 8 | = Custom#1 | 13 | = Kelvin
> 4 | = n/a | 9 | = Custom#2 | 16 | = AWBc

## PanasonicRaw WBInfo Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | NumWBEntries | int16u |
> 1 | WBType1 | int16u | --> EXIF LightSource Values
> 2 | WB_RBLevels1 | int16u[2] |
> 4 | WBType2 | int16u | --> EXIF LightSource Values
> 5 | WB_RBLevels2 | int16u[2] |
> 7 | WBType3 | int16u | --> EXIF LightSource Values
> 8 | WB_RBLevels3 | int16u[2] |
> 10 | WBType4 | int16u | --> EXIF LightSource Values
> 11 | WB_RBLevels4 | int16u[2] |
> 13 | WBType5 | int16u | --> EXIF LightSource Values
> 14 | WB_RBLevels5 | int16u[2] |
> 16 | WBType6 | int16u | --> EXIF LightSource Values
> 17 | WB_RBLevels6 | int16u[2] |
> 19 | WBType7 | int16u | --> EXIF LightSource Values
> 20 | WB_RBLevels7 | int16u[2] |

## PanasonicRaw WBInfo2 Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | NumWBEntries | int16u |
> 1 | WBType1 | int16u | --> EXIF LightSource Values
> 2 | WB_RGBLevels1 | int16u[3] |
> 5 | WBType2 | int16u | --> EXIF LightSource Values
> 6 | WB_RGBLevels2 | int16u[3] |
> 9 | WBType3 | int16u | --> EXIF LightSource Values
> 10 | WB_RGBLevels3 | int16u[3] |
> 13 | WBType4 | int16u | --> EXIF LightSource Values
> 14 | WB_RGBLevels4 | int16u[3] |
> 17 | WBType5 | int16u | --> EXIF LightSource Values
> 18 | WB_RGBLevels5 | int16u[3] |
> 21 | WBType6 | int16u | --> EXIF LightSource Values
> 22 | WB_RGBLevels6 | int16u[3] |
> 25 | WBType7 | int16u | --> EXIF LightSource Values
> 26 | WB_RGBLevels7 | int16u[3] |

## PanasonicRaw DistortionInfo Tags

Lens distortion correction information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | DistortionParam02 | int16s |
> 0x0004 | DistortionParam04 | int16s |
> 0x0005 | DistortionScale | int16s |
> 7.1 | DistortionCorrection | int16s | [val & 0xf] 0 = Off 1 = On
> 0x0008 | DistortionParam08 | int16s |
> 0x0009 | DistortionParam09 | int16s |
> 0x000b | DistortionParam11 | int16s |
> 0x000c | DistortionN? | int16s |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Jul 11, 2024

<-- ExifTool Tag Names