## Samsung Tags

Tags found in the binary "STMN" format maker notes written by a number of Samsung models.

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MakerNoteVersion | undef[8] |
> 2 | PreviewImageStart | int32u* |
> 3 | PreviewImageLength | int32u* |
> 11 | SamsungIFD | - | --> Samsung IFD Tags

## Samsung IFD Tags

This is a standard-format IFD found in the maker notes of some Samsung models, except that the entry count is a 4-byte integer and the offsets are relative to the end of the IFD. Currently, no tags in this IFD are known, so the Unknown (-u) or Verbose (-v) option must be used to see this information.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Samsung Type2 Tags

Tags found in the EXIF-format maker notes of newer Samsung models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MakerNoteVersion | undef[4] |
> 0x0002 | DeviceType | int32u | 0x1000 = Compact Digital Camera 0x2000 = High-end NX Camera 0x3000 = HXM Video Camera 0x12000 = Cell Phone 0x300000 = SMX Video Camera
> 0x0003 | SamsungModelID | int32u | 0x100101c = NX10 0x1001226 = HMX-S15BP 0x1001233 = HMX-Q10 0x1001234 = HMX-H304 0x100130c = NX100 0x1001327 = NX11 0x170104b = ES65, ES67 / VLUU ES65, ES67 / SL50 0x170104e = ES70, ES71 / VLUU ES70, ES71 / SL600 0x1701052 = ES73 / VLUU ES73 / SL605 0x1701055 = ES25, ES27 / VLUU ES25, ES27 / SL45 0x1701300 = ES28 / VLUU ES28 0x1701303 = ES74,ES75,ES78 / VLUU ES75,ES78 0x2001046 = PL150 / VLUU PL150 / TL210 / PL151 0x2001048 = PL100 / TL205 / VLUU PL100 / PL101 0x2001311 = PL120,PL121 / VLUU PL120,PL121 0x2001315 = PL170,PL171 / VLUUPL170,PL171 0x200131e = PL210, PL211 / VLUU PL210, PL211 0x2701317 = PL20,PL21 / VLUU PL20,PL21 0x2a0001b = WP10 / VLUU WP10 / AQ100 0x3000000 = Various Models (0x3000000) 0x3a00018 = Various Models (0x3a00018) 0x400101f = ST1000 / ST1100 / VLUU ST1000 / CL65 0x4001022 = ST550 / VLUU ST550 / TL225 0x4001025 = Various Models (0x4001025) 0x400103e = VLUU ST5500, ST5500, CL80 0x4001041 = VLUU ST5000, ST5000, TL240 0x4001043 = ST70 / VLUU ST70 / ST71 0x400130a = Various Models (0x400130a) 0x400130e = ST90,ST91 / VLUU ST90,ST91 0x4001313 = VLUU ST95, ST95 0x4a00015 = VLUU ST60 0x4a0135b = ST30, ST65 / VLUU ST65 / ST67 0x5000000 = Various Models (0x5000000) 0x5001038 = Various Models (0x5001038) 0x500103a = WB650 / VLUU WB650 / WB660 0x500103c = WB600 / VLUU WB600 / WB610 0x500133e = WB150 / WB150F / WB152 / WB152F / WB151 0x5a0000f = WB5000 / HZ25W 0x5a0001e = WB5500 / VLUU WB5500 / HZ50W 0x6001036 = EX1 0x700131c = VLUU SH100, SH100 0x27127002 = SMX-C20N
> 0x0011 | OrientationInfo | - | --> Samsung OrientationInfo Tags
> 0x0020 | SmartAlbumColor | int16u[2] | '0 0' = n/a [Value 0]
> 0 = Red 1 = Yellow 2 = Green 3 = Blue |  | 4 = Magenta 5 = Black 6 = White 7 = Various
> 0x0021 | PictureWizard | int16u | --> Samsung PictureWizard Tags
> 0x0030 | LocalLocationName | string |
> 0x0031 | LocationName | string |
> 0x0035 | PreviewIFD | - | --> Nikon PreviewIFD Tags --> Nikon PreviewIFD Tags
> 0x0040 | RawDataByteOrder | yes | 0 = Little-endian (Intel, II) 1 = Big-endian (Motorola, MM)
> 0x0041 | WhiteBalanceSetup | int32u | 0 = Auto 1 = Manual
> 0x0043 | CameraTemperature | rational64s |
> 0x0050 | RawDataCFAPattern | yes | 0 = Unchanged 1 = Swap 65535 = Roll
> 0x0100 | FaceDetect | int16u | 0 = Off 1 = On
> 0x0120 | FaceRecognition | int32u | 0 = Off 1 = On
> 0x0123 | FaceName | string |
> 0xa001 | FirmwareName | string |
> 0xa002 | SerialNumber | string |
> 0xa003 | LensType | int16u[n] | [Value 0] 0 = Built-in or Manual Lens 1 = Samsung NX 30mm F2 Pancake 2 = Samsung NX 18-55mm F3.5-5.6 OIS 3 = Samsung NX 50-200mm F4-5.6 ED OIS 4 = Samsung NX 20-50mm F3.5-5.6 ED 5 = Samsung NX 20mm F2.8 Pancake 6 = Samsung NX 18-200mm F3.5-6.3 ED OIS 7 = Samsung NX 60mm F2.8 Macro ED OIS SSA 8 = Samsung NX 16mm F2.4 Pancake 9 = Samsung NX 85mm F1.4 ED SSA 10 = Samsung NX 45mm F1.8 11 = Samsung NX 45mm F1.8 2D/3D 12 = Samsung NX 12-24mm F4-5.6 ED 13 = Samsung NX 16-50mm F2-2.8 S ED OIS 14 = Samsung NX 10mm F3.5 Fisheye 15 = Samsung NX 16-50mm F3.5-5.6 Power Zoom ED OIS 20 = Samsung NX 50-150mm F2.8 S ED OIS 21 = Samsung NX 300mm F2.8 ED OIS
> 0xa004 | LensFirmware | string |
> 0xa005 | InternalLensSerialNumber | string |
> 0xa010 | SensorAreas | int32u[8] | (full and valid sensor areas)
> 0xa011 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB
> 0xa012 | SmartRange | int16u | 0 = Off 1 = On
> 0xa013 | ExposureCompensation | rational64s |
> 0xa014 | ISO | int32u |
> 0xa018 | ExposureTime | rational64u |
> 0xa019 | FNumber | rational64u |
> 0xa01a | FocalLengthIn35mmFormat | int32u |
> 0xa020 | EncryptionKey | int32u[11]! | (key used to decrypt the tags below)
> 0xa021 | WB_RGGBLevelsUncorrected | int32u[4] | (these tags not corrected for WB_RGGBLevelsBlack)
> 0xa022 | WB_RGGBLevelsAuto | int32u[4] |
> 0xa023 | WB_RGGBLevelsIlluminator1 | int32u[4] |
> 0xa024 | WB_RGGBLevelsIlluminator2 | int32u[4] |
> 0xa025 | HighlightLinearityLimit | int32u |
> 0xa028 | WB_RGGBLevelsBlack | int32s[4] |
> 0xa030 | ColorMatrix | int32s[9] |
> 0xa031 | ColorMatrixSRGB | int32s[9] |
> 0xa032 | ColorMatrixAdobeRGB | int32s[9] |
> 0xa033 | CbCrMatrixDefault | int32s[4] |
> 0xa034 | CbCrMatrix | int32s[4] |
> 0xa035 | CbCrGainDefault | int32u[2] |
> 0xa036 | CbCrGain | int32u[2] |
> 0xa040 | ToneCurveSRGBDefault | int32u[23] | (first value gives the number of tone curve entries. This is followed by an array of X coordinates then an array of Y coordinates)
> 0xa041 | ToneCurveAdobeRGBDefault | int32u[23] |
> 0xa042 | ToneCurveSRGB | int32u[23] |
> 0xa043 | ToneCurveAdobeRGB | int32u[23] |
> 0xa048 | RawData? | int32s[12] |
> 0xa050 | Distortion? | int32s[8] |
> 0xa051 | ChromaticAberration? | int16u[22] |
> 0xa052 | Vignetting? | int16u[15] |
> 0xa053 | VignettingCorrection? | int16u[15] |
> 0xa054 | VignettingSetting? | int16u[15] |

## Samsung OrientationInfo Tags

Camera orientation information written by the Gear 360 (SM-C200).

> Index8 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | YawAngle? | rational64s | (always zero)
> 1 | PitchAngle | rational64s | (upward tilt of rear camera in degrees)
> 2 | RollAngle | rational64s | (clockwise rotation of rear camera in degrees)

## Samsung PictureWizard Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | PictureWizardMode | int16u |
> 0 = Standard 1 = Vivid 2 = Portrait 3 = Landscape 4 = Forest |  | 5 = Retro 6 = Cool 7 = Calm 8 = Classic 9 = Custom1 |  | 10 = Custom2 11 = Custom3 255 = n/a
> 1 | PictureWizardColor | int16u |
> 2 | PictureWizardSaturation | int16u |
> 3 | PictureWizardSharpness | int16u |
> 4 | PictureWizardContrast | int16u |

## Samsung APP5 Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'ssuniqueid' | UniqueID | no |

## Samsung Trailer Tags

Tags extracted from the trailer of JPEG images written when using certain features (such as "Sound & Shot" or "Shot & More") from Samsung models such as the Galaxy S4 and Tab S, and from the 'sefd' atom in HEIC images from the Samsung S10+.

> Tag Name | Writable | Values / Notes
> --- | --- | ---
> DepthMapData DepthMapData2 | no no |
> DepthMapName | no |
> DualCameraImage | no |
> DualCameraImageName | no |
> DualShotExtra | - | --> Samsung DualShotExtra Tags
> EmbeddedAudioFile | no |
> EmbeddedAudioFileName | no |
> EmbeddedImage EmbeddedImage2 | no no |
> EmbeddedImageName | no |
> EmbeddedVideoFile | no |
> EmbeddedVideoType | no |
> MCCData | no | 202 = Greece 204 = Netherlands 206 = Belgium 208 = France 212 = Monaco 213 = Andorra 214 = Spain 216 = Hungary 218 = Bosnia & Herzegov. 219 = Croatia 220 = Serbia 221 = Kosovo 222 = Italy 226 = Romania 228 = Switzerland 230 = Czech Rep. 231 = Slovakia 232 = Austria 234 = United Kingdom 235 = United Kingdom 238 = Denmark 240 = Sweden 242 = Norway 244 = Finland 246 = Lithuania 247 = Latvia 248 = Estonia 250 = Russian Federation 255 = Ukraine 257 = Belarus 259 = Moldova 260 = Poland 262 = Germany 266 = Gibraltar 268 = Portugal 270 = Luxembourg 272 = Ireland 274 = Iceland 276 = Albania 278 = Malta 280 = Cyprus 282 = Georgia 283 = Armenia 284 = Bulgaria 286 = Turkey 288 = Faroe Islands 289 = Abkhazia 290 = Greenland 292 = San Marino 293 = Slovenia 294 = Macedonia 295 = Liechtenstein 297 = Montenegro 302 = Canada 308 = St. Pierre & Miquelon 310 = United States / Guam 311 = United States / Guam 312 = United States 316 = United States 330 = Puerto Rico 334 = Mexico 338 = Jamaica 340 = French Guiana / Guadeloupe / Martinique 342 = Barbados 344 = Antigua and Barbuda 346 = Cayman Islands 348 = British Virgin Islands 350 = Bermuda 352 = Grenada 354 = Montserrat 356 = Saint Kitts and Nevis 358 = Saint Lucia 360 = St. Vincent & Gren. 362 = Bonaire, Sint Eustatius and Saba / Curacao / Netherlands Antilles 363 = Aruba 364 = Bahamas 365 = Anguilla 366 = Dominica 368 = Cuba 370 = Dominican Republic 372 = Haiti 374 = Trinidad and Tobago 376 = Turks and Caicos Islands / US Virgin Islands 400 = Azerbaijan 401 = Kazakhstan 402 = Bhutan 404 = India 405 = India 410 = Pakistan 412 = Afghanistan 413 = Sri Lanka 414 = Myanmar (Burma) 415 = Lebanon 416 = Jordan 417 = Syrian Arab Republic 418 = Iraq 419 = Kuwait 420 = Saudi Arabia 421 = Yemen 422 = Oman 424 = United Arab Emirates 425 = Israel / Palestinian Territory 426 = Bahrain 427 = Qatar 428 = Mongolia 429 = Nepal 430 = United Arab Emirates 431 = United Arab Emirates 432 = Iran 434 = Uzbekistan 436 = Tajikistan 437 = Kyrgyzstan 438 = Turkmenistan 440 = Japan 441 = Japan 450 = South Korea 452 = Viet Nam 454 = Hongkong, China 455 = Macao, China 456 = Cambodia 457 = Laos P.D.R. 460 = China 466 = Taiwan 467 = North Korea 470 = Bangladesh 472 = Maldives 502 = Malaysia 505 = Australia 510 = Indonesia 514 = Timor-Leste 515 = Philippines 520 = Thailand 525 = Singapore 528 = Brunei Darussalam 530 = New Zealand 537 = Papua New Guinea 539 = Tonga 540 = Solomon Islands 541 = Vanuatu 542 = Fiji 544 = American Samoa 545 = Kiribati 546 = New Caledonia 547 = French Polynesia 548 = Cook Islands 549 = Samoa 550 = Micronesia 552 = Palau 553 = Tuvalu 555 = Niue 602 = Egypt 603 = Algeria 604 = Morocco 605 = Tunisia 606 = Libya 607 = Gambia 608 = Senegal 609 = Mauritania 610 = Mali 611 = Guinea 612 = Ivory Coast 613 = Burkina Faso 614 = Niger 615 = Togo 616 = Benin 617 = Mauritius 618 = Liberia 619 = Sierra Leone 620 = Ghana 621 = Nigeria 622 = Chad 623 = Central African Rep. 624 = Cameroon 625 = Cape Verde 626 = Sao Tome & Principe 627 = Equatorial Guinea 628 = Gabon 629 = Congo, Republic 630 = Congo, Dem. Rep. 631 = Angola 632 = Guinea-Bissau 633 = Seychelles 634 = Sudan 635 = Rwanda 636 = Ethiopia 637 = Somalia 638 = Djibouti 639 = Kenya 640 = Tanzania 641 = Uganda 642 = Burundi 643 = Mozambique 645 = Zambia 646 = Madagascar 647 = Reunion 648 = Zimbabwe 649 = Namibia 650 = Malawi 651 = Lesotho 652 = Botswana 653 = Swaziland 654 = Comoros 655 = South Africa 657 = Eritrea 659 = South Sudan 702 = Belize 704 = Guatemala 706 = El Salvador 708 = Honduras 710 = Nicaragua 712 = Costa Rica 714 = Panama 716 = Peru 722 = Argentina Republic 724 = Brazil 730 = Chile 732 = Colombia 734 = Venezuela 736 = Bolivia 738 = Guyana 740 = Ecuador 744 = Paraguay 746 = Suriname 748 = Uruguay 750 = Falkland Islands (Malvinas) 901 = International Networks / Satellite Networks
> SingleShotDepthMap | no |
> SingleShotMeta | - | --> Samsung SingleShotMeta Tags
> SurroundShotVideo | no |
> SurroundShotVideoName | no |
> TimeStamp | no |

## Samsung DualShotExtra Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 16 | DepthMapWidth | no | (index varies depending on model)
> 17 | DepthMapHeight | no | (index varies depending on model)

## Samsung SingleShotMeta Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'beautyColorLevel' | BeautyColorLevel | no |
> 'beautyRetouchLevel' | BeautyRetouchLevel | no |
> 'blurStrength' | BlurStrength | no |
> 'bokehShape' | BokehShape | no |
> 'colorpopStrength' | ColorpopStrength | no |
> 'depthHWHeight' | DepthHWHeight | no |
> 'depthHWWidth' | DepthHWWidth | no |
> 'depthSWHeight' | DepthSWHeight | no |
> 'depthSWWidth' | DepthSWWidth | no |
> 'deviceOrientation' | DeviceOrientation | no |
> 'effectStrength' | EffectStrength | no |
> 'effectType' | EffectType | no |
> 'flipStatus' | FlipStatus | no |
> 'inputHeight' | InputHeight | no |
> 'inputWidth' | InputWidth | no |
> 'isArtBokeh' | IsArtBokeh | no |
> 'lensFacing' | LensFacing | no |
> 'monoStrength' | MonoStrength | no |
> 'objectOrientation' | ObjectOrientation | no |
> 'outputHeight' | OutputHeight | no |
> 'outputWidth' | OutputWidth | no |
> 'perfMode' | PerfMode | no |
> 'segHeight' | SegHeight | no |
> 'segWidth' | SegWidth | no |
> 'sidelightStrength' | SidelightStrength | no |
> 'spinStrength' | SpinStrength | no |
> 'vintageStrength' | VintageStrength | no |
> 'zoomStrength' | ZoomStrength | no |

## Samsung sec Tags

This information is found in the @sec atom of Samsung MP4 videos from models such as the WB30F.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | no |
> 32 | Model | no |
> 512 | ThumbnailWidth | no |
> 516 | ThumbnailHeight | no |
> 520 | ThumbnailLength | no |
> 524 | ThumbnailImage | no | (the THM image, embedded metadata is extracted as the first sub-document)

## Samsung INFO Tags

This information is found in MP4 videos from Samsung models such as the SMX-C20N.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'EFCT' | Effect | no |
> 'QLTY' | Quality | no |

## Samsung MP4 Tags

This information is found in Samsung MP4 videos from models such as the WP10.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Make | no |
> 24 | Model | no |
> 46 | ExposureTime | no |
> 50 | FNumber | no |
> 58 | ExposureCompensation | no |
> 106 | ISO | no |
> 125 | Software | no |
> 244 | Thumbnail | - | --> Samsung Thumbnail Tags

## Samsung Thumbnail Tags

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | ThumbnailWidth | no |
> 2 | ThumbnailHeight | no |
> 3 | ThumbnailLength | no |
> 4 | ThumbnailOffset | no |

## Samsung smta Tags

This information is found in the smta atom of Samsung MP4 videos from models such as the Galaxy S4.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'svss' | SamsungSvss | - | --> Samsung svss Tags

## Samsung svss Tags

This information is found in the svss atom of Samsung MP4 videos from models such as the Galaxy S4.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Jun 1, 2022

<-- ExifTool Tag Names