## Sony Tags

The following information has been decoded from the MakerNotes of Sony cameras. Some of these tags have been inherited from the Minolta MakerNotes.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0010 | CameraInfo CameraInfo2 CameraInfo3 CameraInfoUnknown | - - - - | --> Sony CameraInfo Tags --> Sony CameraInfo2 Tags --> Sony CameraInfo3 Tags --> Sony CameraInfoUnknown Tags
> 0x0020 | FocusInfo MoreInfo | - - | --> Sony FocusInfo Tags --> Sony MoreInfo Tags
> 0x0102 | Quality | int32u |
> 0 = RAW 1 = Super Fine 2 = Fine 3 = Standard 4 = Economy 5 = Extra Fine 6 = RAW + JPEG/HEIF 7 = Compressed RAW 8 = Compressed RAW + JPEG 9 = Light 4294967295 = n/a
> 0x0104 | FlashExposureComp | rational64s |
> 0x0105 | Teleconverter | int32u |
> 0x0 = None 0x4 = Minolta/Sony AF 1.4x APO (D) (0x04) 0x5 = Minolta/Sony AF 2x APO (D) (0x05) 0x48 = Minolta/Sony AF 2x APO (D) 0x50 = Minolta AF 2x APO II 0x60 = Minolta AF 2x APO 0x88 = Minolta/Sony AF 1.4x APO (D) 0x90 = Minolta AF 1.4x APO II 0xa0 = Minolta AF 1.4x APO
> 0x0112 | WhiteBalanceFineTune | int32u |
> 0x0114 | CameraSettings CameraSettings2 CameraSettings3 CameraSettingsUnknown | - - - - | --> Sony CameraSettings Tags --> Sony CameraSettings2 Tags --> Sony CameraSettings3 Tags --> Sony CameraSettingsUnknown Tags
> 0x0115 | WhiteBalance | int32u |
> 0x0 = Auto 0x1 = Color Temperature/Color Filter 0x10 = Daylight 0x20 = Cloudy 0x30 = Shade 0x40 = Tungsten 0x50 = Flash 0x60 = Fluorescent 0x70 = Custom 0x80 = Underwater
> 0x0116 | ExtraInfo ExtraInfo2 ExtraInfo3 | - - - | --> Sony ExtraInfo Tags --> Sony ExtraInfo2 Tags --> Sony ExtraInfo3 Tags
> 0x0e00 | PrintIM | - | --> PrintIM Tags
> 0x1000 | MultiBurstMode | undef | (MultiBurst tags valid only for models with this feature, like the F88) 0 = Off 1 = On
> 0x1001 | MultiBurstImageWidth | int16u |
> 0x1002 | MultiBurstImageHeight | int16u |
> 0x1003 | Panorama | - | --> Sony Panorama Tags
> 0x2001 | PreviewImage | undef | (HD-size preview in JPEG images from almost all DSLR/SLT/ILCA/NEX/ILCE.)
> 0x2002 | Rating | int32u |
> 0x2004 | Contrast | int32s |
> 0x2005 | Saturation | int32s |
> 0x2006 | Sharpness | int32s |
> 0x2007 | Brightness | int32s |
> 0x2008 | LongExposureNoiseReduction | int32u |
> 0x0 = Off 0x1 = On (unused) 0x10001 = On (dark subtracted) 0xffff0000 = Off (65535) 0xffff0001 = On (65535) 0xffffffff = n/a
> 0x2009 | HighISONoiseReduction | int16u |
> 0 = Off 1 = Low 2 = Normal |  | 3 = High 256 = Auto 65535 = n/a
> 0x200a | HDR | int32u | (stored as a 32-bit integer, but read as two 16-bit integers) [Value 0]
> 0x0 = Off 0x1 = Auto 0x10 = 1.0 EV 0x11 = 1.5 EV 0x12 = 2.0 EV |  | 0x13 = 2.5 EV 0x14 = 3.0 EV 0x15 = 3.5 EV 0x16 = 4.0 EV 0x17 = 4.5 EV |  | 0x18 = 5.0 EV 0x19 = 5.5 EV 0x1a = 6.0 EV
> [Value 1] 0x0 = Uncorrected image 0x1 = HDR image (good) 0x2 = HDR image (fail 1) 0x3 = HDR image (fail 2)
> 0x200b | MultiFrameNoiseReduction | int32u | (may not be valid for RS100) 0 = Off 1 = On 255 = n/a
> 0x200e | PictureEffect | int16u |
> 0 = Off 1 = Toy Camera 2 = Pop Color 3 = Posterization 4 = Posterization B/W 5 = Retro Photo 6 = Soft High Key 7 = Partial Color (red) 8 = Partial Color (green) 9 = Partial Color (blue) 10 = Partial Color (yellow) 13 = High Contrast Monochrome 16 = Toy Camera (normal) 17 = Toy Camera (cool) 18 = Toy Camera (warm) 19 = Toy Camera (green) 20 = Toy Camera (magenta) 32 = Soft Focus (low) 33 = Soft Focus 34 = Soft Focus (high) 48 = Miniature (auto) 49 = Miniature (top) 50 = Miniature (middle horizontal) 51 = Miniature (bottom) 52 = Miniature (left) 53 = Miniature (middle vertical) 54 = Miniature (right) 64 = HDR Painting (low) 65 = HDR Painting 66 = HDR Painting (high) 80 = Rich-tone Monochrome 97 = Water Color 98 = Water Color 2 112 = Illustration (low) 113 = Illustration 114 = Illustration (high)
> 0x200f | SoftSkinEffect | int32u | 0 = Off 1 = Low 2 = Mid 3 = High 4294967295 = n/a
> 0x2010 | Tag2010a Tag2010b Tag2010c Tag2010d Tag2010e Tag2010f Tag2010g Tag2010h Tag2010i | - - - - - - - - - | --> Sony Tag2010a Tags --> Sony Tag2010b Tags --> Sony Tag2010c Tags --> Sony Tag2010d Tags --> Sony Tag2010e Tags --> Sony Tag2010f Tags --> Sony Tag2010g Tags --> Sony Tag2010h Tags --> Sony Tag2010i Tags
> 0x2011 | VignettingCorrection | int32u | 0 = Off 2 = Auto 4294967295 = n/a
> 0x2012 | LateralChromaticAberration | int32u | 0 = Off 2 = Auto 4294967295 = n/a
> 0x2013 | DistortionCorrectionSetting | int32u | 0 = Off 2 = Auto 4294967295 = n/a
> 0x2014 | WBShiftAB_GM | int32s[2] | (2 numbers: 1. positive is a shift toward amber, 2. positive is a shift toward magenta)
> 0x2016 | AutoPortraitFramed | int16u | ("Yes" if this image was created by the Auto Portrait Framing feature) 0 = No 1 = Yes
> 0x2017 | FlashAction | int32u | 0 = Did not fire 1 = Flash Fired 2 = External Flash Fired 3 = Wireless Controlled Flash Fired
> 0x201a | ElectronicFrontCurtainShutter | int32u | 0 = Off 1 = On
> 0x201b | FocusMode | int8u |
> 0 = Manual 2 = AF-S 3 = AF-C |  | 4 = AF-A 6 = DMF 7 = AF-D
> 0x201c | AFAreaModeSetting | int8u | (SLT models) 0 = Wide 4 = Local 8 = Zone 9 = Spot (NEX, ILCE and some DSC models)
> 0 = Wide 1 = Center 3 = Flexible Spot 4 = Flexible Spot (LA-EA4) 9 = Center (LA-EA4) 11 = Zone 12 = Expanded Flexible Spot
> (ILCA models) 0 = Wide 4 = Flexible Spot 8 = Zone 9 = Center 12 = Expanded Flexible Spot
> 0x201d | FlexibleSpotPosition | int16u[2] | (X and Y coordinates of the AF point, valid only when AFAreaMode is Flexible Spot)
> 0x201e | AFPointSelected | int8u | (SLT models or ILCE with LA-EA2/EA4)
> 0 = Auto 1 = Center 2 = Top 3 = Upper-right 4 = Right 5 = Lower-right 6 = Bottom 7 = Lower-left 8 = Left 9 = Upper-left |  | 10 = Far Right 11 = Far Left 12 = Upper-middle 13 = Near Right 14 = Lower-middle 15 = Near Left 16 = Upper Far Right 17 = Lower Far Right 18 = Lower Far Left 19 = Upper Far Left
> (ILCA-68 and ILCA-77M2)
> -1 = Auto 0 = A5 1 = A6 2 = A7 3 = B2 4 = B3 5 = B4 6 = B5 7 = B6 8 = B7 9 = B8 10 = B9 11 = B10 12 = C1 13 = C2 14 = C3 |  | 15 = C4 16 = C5 17 = C6 18 = C7 19 = C8 20 = C9 21 = C10 22 = C11 23 = D1 24 = D2 25 = D3 26 = D4 27 = D5 28 = D6 29 = D7 30 = D8 |  | 31 = D9 32 = D10 33 = D11 34 = E1 35 = E2 36 = E3 37 = E4 38 = E5 39 = E6 (Center) 40 = E7 41 = E8 42 = E9 43 = E10 44 = E11 45 = F1 46 = F2 |  | 47 = F3 48 = F4 49 = F5 50 = F6 51 = F7 52 = F8 53 = F9 54 = F10 55 = F11 56 = G1 57 = G2 58 = G3 59 = G4 60 = G5 61 = G6 62 = G7 |  | 63 = G8 64 = G9 65 = G10 66 = G11 67 = H2 68 = H3 69 = H4 70 = H5 71 = H6 72 = H7 73 = H8 74 = H9 75 = H10 76 = I5 77 = I6 78 = I7
> (ILCA-99M2 when AFAreaModeSetting is not Zone)
> 0 = Auto 93 = A5 (93) 94 = A6 (94) 95 = A7 (95) 106 = B2 (106) 107 = B3 (107) 108 = B4 (108) 110 = B5 (110) 111 = B6 (111) 112 = B7 (112) 114 = B8 (114) 115 = B9 (115) 116 = B10 (116) 122 = C1 (122) 123 = C2 (123) 124 = C3 (124) 125 = C4 (125) 127 = C5 (127) 128 = C6 (128) 129 = C7 (129) |  | 131 = C8 (131) 132 = C9 (132) 133 = C10 (133) 134 = C11 (134) 139 = D1 (139) 140 = D2 (140) 141 = D3 (141) 142 = D4 (142) 144 = D5 (144) 145 = D6 (145) 146 = D7 (146) 148 = D8 (148) 149 = D9 (149) 150 = D10 (150) 151 = D11 (151) 156 = E1 (156) 157 = E2 (157) 158 = E3 (158) 159 = E4 (159) 161 = E5 (161) |  | 162 = E6 (162, Center) 163 = E7 (163) 165 = E8 (165) 166 = E9 (166) 167 = E10 (167) 168 = E11 (168) 173 = F1 (173) 174 = F2 (174) 175 = F3 (175) 176 = F4 (176) 178 = F5 (178) 179 = F6 (179) 180 = F7 (180) 182 = F8 (182) 183 = F9 (183) 184 = F10 (184) 185 = F11 (185) 190 = G1 (190) 191 = G2 (191) 192 = G3 (192) |  | 193 = G4 (193) 195 = G5 (195) 196 = G6 (196) 197 = G7 (197) 199 = G8 (199) 200 = G9 (200) 201 = G10 (201) 202 = G11 (202) 208 = H2 (208) 209 = H3 (209) 210 = H4 (210) 212 = H5 (212) 213 = H6 (213) 214 = H7 (214) 216 = H8 (216) 217 = H9 (217) 218 = H10 (218) 229 = I5 (229) 230 = I6 (230) 231 = I7 (231)
> (ILCA models when AFAreaModeSetting is set to Zone)
> 0 = n/a 1 = Top Left Zone 2 = Top Zone 3 = Top Right Zone 4 = Left Zone |  | 5 = Center Zone 6 = Right Zone 7 = Bottom Left Zone 8 = Bottom Zone 9 = Bottom Right Zone
> (NEX and ILCE models)
> 0 = n/a 1 = Center Zone 2 = Top Zone 3 = Right Zone 4 = Left Zone |  | 5 = Bottom Zone 6 = Bottom Right Zone 7 = Bottom Left Zone 8 = Top Left Zone 9 = Top Right Zone
> 0x2020 | AFPointsUsed | no | (SLT models, or NEX/ILCE with A-mount lenses)
> 0x0 = (none) Bit 0 = Center Bit 1 = Top Bit 2 = Upper-right Bit 3 = Right Bit 4 = Lower-right Bit 5 = Bottom Bit 6 = Lower-left Bit 7 = Left Bit 8 = Upper-left |  | Bit 9 = Far Right Bit 10 = Far Left Bit 11 = Upper-middle Bit 12 = Near Right Bit 13 = Lower-middle Bit 14 = Near Left Bit 15 = Upper Far Right Bit 16 = Lower Far Right Bit 17 = Lower Far Left Bit 18 = Upper Far Left
> (ILCA models)
> 0x0 = (none) Bit 0 = A5 Bit 1 = A6 Bit 2 = A7 Bit 3 = B2 Bit 4 = B3 Bit 5 = B4 Bit 6 = B5 Bit 7 = B6 Bit 8 = B7 Bit 9 = B8 Bit 10 = B9 Bit 11 = B10 Bit 12 = C1 Bit 13 = C2 Bit 14 = C3 Bit 15 = C4 Bit 16 = C5 Bit 17 = C6 Bit 18 = C7 |  | Bit 19 = C8 Bit 20 = C9 Bit 21 = C10 Bit 22 = C11 Bit 23 = D1 Bit 24 = D2 Bit 25 = D3 Bit 26 = D4 Bit 27 = D5 Bit 28 = D6 Bit 29 = D7 Bit 30 = D8 Bit 31 = D9 Bit 32 = D10 Bit 33 = D11 Bit 34 = E1 Bit 35 = E2 Bit 36 = E3 Bit 37 = E4 Bit 38 = E5 |  | Bit 39 = E6 Bit 40 = E7 Bit 41 = E8 Bit 42 = E9 Bit 43 = E10 Bit 44 = E11 Bit 45 = F1 Bit 46 = F2 Bit 47 = F3 Bit 48 = F4 Bit 49 = F5 Bit 50 = F6 Bit 51 = F7 Bit 52 = F8 Bit 53 = F9 Bit 54 = F10 Bit 55 = F11 Bit 56 = G1 Bit 57 = G2 Bit 58 = G3 |  | Bit 59 = G4 Bit 60 = G5 Bit 61 = G6 Bit 62 = G7 Bit 63 = G8 Bit 64 = G9 Bit 65 = G10 Bit 66 = G11 Bit 67 = H2 Bit 68 = H3 Bit 69 = H4 Bit 70 = H5 Bit 71 = H6 Bit 72 = H7 Bit 73 = H8 Bit 74 = H9 Bit 75 = H10 Bit 76 = I5 Bit 77 = I6 Bit 78 = I7
> 0x2021 | AFTracking | int8u | 0 = Off 1 = Face tracking 2 = Lock On AF
> 0x2022 | FocalPlaneAFPointsUsed | no | (On-sensor/focal-plane phase AF points for ILCE with hybrid AF) 0x0 = (none) 0x0 = (none)
> 0x2023 | MultiFrameNREffect | int32u | 0 = Normal 1 = High
> 0x2026 | WBShiftAB_GM_Precise | int32s[2]~ | (2 numbers: 1. positive is a shift toward amber, 2. positive is a shift toward magenta)
> 0x2027 | FocusLocation | int16u[4] |
> 0x2028 | VariableLowPassFilter | int16u[2] | '0 0' = n/a '1 0' = Off '1 1' = Standard '1 2' = High '65535 65535' = n/a
> 0x2029 | RAWFileType | int16u | 0 = Compressed RAW 1 = Uncompressed RAW 2 = Lossless Compressed RAW 65535 = n/a
> 0x202a | Tag202a | - | --> Sony Tag202a Tags
> 0x202b | PrioritySetInAWB | int8u | 0 = Standard 1 = Ambience 2 = White
> 0x202c | MeteringMode2 | int16u |
> 0x100 = Multi-segment 0x200 = Center-weighted average 0x301 = Spot (Standard) 0x302 = Spot (Large) 0x400 = Average 0x500 = Highlight
> 0x202d | ExposureStandardAdjustment | rational64s |
> 0x202e | Quality | int16u[2] |
> '0 0' = n/a '0 1' = Standard '0 2' = Fine '0 3' = Extra Fine '0 4' = Light '1 0' = RAW '1 1' = RAW + Standard '1 2' = RAW + Fine '1 3' = RAW + Extra Fine '1 4' = RAW + Light
> 0x202f | PixelShiftInfo | undef | '00000000 0 0 0x0' = n/a
> 0x2031 | SerialNumber | string |
> 0x2032 | Shadows | int32s |
> 0x2033 | Highlights | int32s |
> 0x2034 | Fade | int32s |
> 0x2035 | SharpnessRange | int32s |
> 0x2036 | Clarity | int32s |
> 0x2037 | FocusFrameSize | no | (width and height of FocusFrame, centered on FocusLocation)
> 0x2039 | JPEG-HEIFSwitch | int16u | 0 = JPEG 1 = HEIF 65535 = n/a
> 0x3000 | ShotInfo | - | --> Sony ShotInfo Tags
> 0x900b | Tag900b | - | --> Sony Tag900b Tags
> 0x9050 | Tag9050a Tag9050b Tag9050c | - - - | --> Sony Tag9050a Tags --> Sony Tag9050b Tags --> Sony Tag9050c Tags
> 0x9400 | Tag9400a Tag9400b Tag9400c | - - - | --> Sony Tag9400a Tags --> Sony Tag9400b Tags --> Sony Tag9400c Tags
> 0x9401 | Tag9401 | - | --> Sony Tag9401 Tags
> 0x9402 | Tag9402 | - | --> Sony Tag9402 Tags
> 0x9403 | Tag9403 | - | --> Sony Tag9403 Tags
> 0x9404 | Tag9404a Tag9404b Tag9404c | - - - | --> Sony Tag9404a Tags --> Sony Tag9404b Tags --> Sony Tag9404c Tags
> 0x9405 | Tag9405a Tag9405b | - - | --> Sony Tag9405a Tags --> Sony Tag9405b Tags
> 0x9406 | Tag9406 | - | --> Sony Tag9406 Tags
> 0x940a | Tag940a | - | --> Sony Tag940a Tags
> 0x940c | Tag940c | - | --> Sony Tag940c Tags
> 0x940e | AFInfo Tag940e | - - | --> Sony AFInfo Tags --> Sony Tag940e Tags
> 0x9416 | Sony_0x9416 | - | --> Sony Tag9416 Tags
> 0xb000 | FileFormat | int8u[4] |
> '0 0 0 2' = JPEG '1 0 0 0' = SR2 '2 0 0 0' = ARW 1.0 '3 0 0 0' = ARW 2.0 '3 1 0 0' = ARW 2.1 '3 2 0 0' = ARW 2.2 |  | '3 3 0 0' = ARW 2.3 '3 3 1 0' = ARW 2.3.1 '3 3 2 0' = ARW 2.3.2 '3 3 3 0' = ARW 2.3.3 '3 3 5 0' = ARW 2.3.5 '4 0 0 0' = ARW 4.0
> 0xb001 | SonyModelID | int16u |
> 2 = DSC-R1 256 = DSLR-A100 257 = DSLR-A900 258 = DSLR-A700 259 = DSLR-A200 260 = DSLR-A350 261 = DSLR-A300 262 = DSLR-A900 (APS-C mode) 263 = DSLR-A380/A390 264 = DSLR-A330 265 = DSLR-A230 266 = DSLR-A290 269 = DSLR-A850 270 = DSLR-A850 (APS-C mode) 273 = DSLR-A550 274 = DSLR-A500 275 = DSLR-A450 278 = NEX-5 279 = NEX-3 280 = SLT-A33 281 = SLT-A55 / SLT-A55V 282 = DSLR-A560 283 = DSLR-A580 284 = NEX-C3 285 = SLT-A35 286 = SLT-A65 / SLT-A65V 287 = SLT-A77 / SLT-A77V 288 = NEX-5N 289 = NEX-7 290 = NEX-VG20E 291 = SLT-A37 292 = SLT-A57 293 = NEX-F3 294 = SLT-A99 / SLT-A99V 295 = NEX-6 296 = NEX-5R 297 = DSC-RX100 298 = DSC-RX1 299 = NEX-VG900 300 = NEX-VG30E 302 = ILCE-3000 / ILCE-3500 303 = SLT-A58 305 = NEX-3N 306 = ILCE-7 307 = NEX-5T 308 = DSC-RX100M2 309 = DSC-RX10 |  | 310 = DSC-RX1R 311 = ILCE-7R 312 = ILCE-6000 313 = ILCE-5000 317 = DSC-RX100M3 318 = ILCE-7S 319 = ILCA-77M2 339 = ILCE-5100 340 = ILCE-7M2 341 = DSC-RX100M4 342 = DSC-RX10M2 344 = DSC-RX1RM2 346 = ILCE-QX1 347 = ILCE-7RM2 350 = ILCE-7SM2 353 = ILCA-68 354 = ILCA-99M2 355 = DSC-RX10M3 356 = DSC-RX100M5 357 = ILCE-6300 358 = ILCE-9 360 = ILCE-6500 362 = ILCE-7RM3 363 = ILCE-7M3 364 = DSC-RX0 365 = DSC-RX10M4 366 = DSC-RX100M6 367 = DSC-HX99 369 = DSC-RX100M5A 371 = ILCE-6400 372 = DSC-RX0M2 374 = DSC-RX100M7 375 = ILCE-7RM4 376 = ILCE-9M2 378 = ILCE-6600 379 = ILCE-6100 380 = ZV-1 381 = ILCE-7C 382 = ZV-E10 383 = ILCE-7SM3 384 = ILCE-1 385 = ILME-FX3 386 = ILCE-7RM3A 387 = ILCE-7RM4A 388 = ILCE-7M4 389 = ZV-1F 391 = ILME-FX30
> 0xb020 | CreativeStyle | string |
> 'AdobeRGB' = Adobe RGB 'Autumnleaves' = Autumn Leaves 'BW' = B&W 'Clear' = Clear 'Deep' = Deep 'FL' = FL 'IN' = IN 'Landscape' = Landscape 'Light' = Light 'Neutral' = Neutral 'Nightview' = Night View/Portrait 'None' = None 'Portrait' = Portrait 'Real' = Real 'SH' = SH 'Sepia' = Sepia 'Standard' = Standard 'Sunset' = Sunset 'VV2' = Vivid 2 'Vivid' = Vivid
> 0xb021 | ColorTemperature | int32u |
> 0xb022 | ColorCompensationFilter | int32u | (negative is green, positive is magenta)
> 0xb023 | SceneMode | int32u |
> 0 = Standard 1 = Portrait 2 = Text 3 = Night Scene 4 = Sunset 5 = Sports 6 = Landscape 7 = Night Portrait 8 = Macro 9 = Super Macro 16 = Auto 17 = Night View/Portrait 18 = Sweep Panorama |  | 19 = Handheld Night Shot 20 = Anti Motion Blur 21 = Cont. Priority AE 22 = Auto+ 23 = 3D Sweep Panorama 24 = Superior Auto 25 = High Sensitivity 26 = Fireworks 27 = Food 28 = Pet 33 = HDR 65535 = n/a
> 0xb024 | ZoneMatching | int32u | 0 = ISO Setting Used 1 = High Key 2 = Low Key
> 0xb025 | DynamicRangeOptimizer | int32u |
> 0 = Off 1 = Standard 2 = Advanced Auto 3 = Auto 8 = Advanced Lv1 9 = Advanced Lv2 10 = Advanced Lv3 |  | 11 = Advanced Lv4 12 = Advanced Lv5 16 = Lv1 17 = Lv2 18 = Lv3 19 = Lv4 20 = Lv5
> 0xb026 | ImageStabilization | int32u | 0 = Off 1 = On 4294967295 = n/a
> 0xb027 | LensType | int32u | --> Sony LensType Values
> 0xb028 | MinoltaMakerNote | - | --> Minolta Tags
> 0xb029 | ColorMode | int32u |
> 0 = Standard 1 = Vivid 2 = Portrait 3 = Landscape 4 = Sunset 5 = Night View/Portrait 6 = B&W 7 = Adobe RGB 12 = Neutral 13 = Clear 14 = Deep 15 = Light 16 = Autumn Leaves |  | 17 = Sepia 18 = FL 19 = Vivid 2 20 = IN 21 = SH 100 = Neutral 101 = Clear 102 = Deep 103 = Light 104 = Night View 105 = Autumn Leaves 255 = Off 4294967295 = n/a
> 0xb02a | LensSpec | int8u[8] | (like LensInfo, but also specifies lens features: DT, E, ZA, G, SSM, SAM, OSS, STF, Reflex, Macro and Fisheye)
> 0xb02b | FullImageSize | int32u[2] |
> 0xb02c | PreviewImageSize | int32u[2] |
> 0xb040 | Macro | int16u | 0 = Off 1 = On 2 = Close Focus 65535 = n/a
> 0xb041 | ExposureMode | int16u |
> 0 = Program AE 1 = Portrait 2 = Beach 3 = Sports 4 = Snow 5 = Landscape 6 = Auto 7 = Aperture-priority AE 8 = Shutter speed priority AE 9 = Night Scene / Twilight 10 = Hi-Speed Shutter 11 = Twilight Portrait 12 = Soft Snap/Portrait 13 = Fireworks 14 = Smile Shutter 15 = Manual |  | 18 = High Sensitivity 19 = Macro 20 = Advanced Sports Shooting 29 = Underwater 33 = Food 34 = Sweep Panorama 35 = Handheld Night Shot 36 = Anti Motion Blur 37 = Pet 38 = Backlight Correction HDR 39 = Superior Auto 40 = Background Defocus 41 = Soft Skin 42 = 3D Image 65535 = n/a
> 0xb042 | FocusMode | int16u | (not valid for all models) 1 = AF-S 2 = AF-C 4 = Permanent-AF 65535 = n/a
> 0xb043 | AFAreaMode | int16u | (older models)
> 0 = Default 1 = Multi 2 = Center 3 = Spot 4 = Flexible Spot |  | 6 = Touch 14 = Tracking 15 = Face Tracking 65535 = n/a
> (DSC-HX9V generation cameras)
> 0 = Multi 1 = Center 2 = Spot 3 = Flexible Spot 10 = Selective (for Miniature effect) 14 = Tracking 15 = Face Tracking 255 = Manual
> 0xb044 | AFIlluminator | int16u | 0 = Off 1 = Auto 65535 = n/a
> 0xb047 | JPEGQuality | int16u | 0 = Standard 1 = Fine 2 = Extra Fine 65535 = n/a
> 0xb048 | FlashLevel | int16s |
> -32768 = Low -9 = -9/3 -6 = -6/3 -5 = -5/3 -4 = -4/3 -3 = -3/3 |  | -2 = -2/3 -1 = -1/3 0 = Normal 1 = +1/3 2 = +2/3 3 = +3/3 |  | 4 = +4/3 5 = +5/3 6 = +6/3 9 = +9/3 128 = n/a 32767 = High
> 0xb049 | ReleaseMode | int16u |
> 0 = Normal 2 = Continuous 5 = Exposure Bracketing 6 = White Balance Bracketing 8 = DRO Bracketing 65535 = n/a
> 0xb04a | SequenceNumber | int16u | (shot number in continuous burst) 0 = Single 65535 = n/a
> 0xb04b | Anti-Blur | int16u | 0 = Off 1 = On (Continuous) 2 = On (Shooting) 65535 = n/a
> 0xb04e | FocusMode | int16u | (valid for DSC-HX9V generation and newer) 0 = Manual 2 = AF-S 3 = AF-C 5 = Semi-manual 6 = DMF
> 0xb04f | DynamicRangeOptimizer | int16u | 0 = Off 1 = Standard 2 = Plus
> 0xb050 | HighISONoiseReduction2 | int16u | (DSC models only) 0 = Normal 1 = High 2 = Low 3 = Off 65535 = n/a
> 0xb052 | IntelligentAuto | int16u | 0 = Off 1 = On 2 = Advanced
> 0xb054 | WhiteBalance | int16u | (decoding of the Fluorescent settings matches the EXIF standard, which is different than the names used by Sony for some models)
> 0 = Auto 4 = Custom 5 = Daylight 6 = Cloudy 7 = Cool White Fluorescent 8 = Day White Fluorescent 9 = Daylight Fluorescent 10 = Incandescent2 11 = Warm White Fluorescent 14 = Incandescent 15 = Flash 17 = Underwater 1 (Blue Water) 18 = Underwater 2 (Green Water) 19 = Underwater Auto

## Sony LensType Values

Decimal values have been added to differentiate lenses which would otherwise have the same LensType, and are used by the Composite LensID tag when attempting to identify the specific lens model. "New" or "II" appear in brackets if the original version of the lens has the same LensType. Special logic is employed to identify the attached lens when a Metabones Canon EF adapter is used.

> Value | LensType
> --- | ---
> 0 | = Minolta AF 28-85mm F3.5-4.5 New
> 1 | = Minolta AF 80-200mm F2.8 HS-APO G
> 2 | = Minolta AF 28-70mm F2.8 G
> 3 | = Minolta AF 28-80mm F4-5.6
> 4 | = Minolta AF 85mm F1.4G
> 5 | = Minolta AF 35-70mm F3.5-4.5 [II]
> 6 | = Minolta AF 24-85mm F3.5-4.5 [New]
> 7 | = Minolta AF 100-300mm F4.5-5.6 APO [New] or 100-400mm or Sigma Lens
> 7.1 | = Minolta AF 100-400mm F4.5-6.7 APO
> 7.2 | = Sigma AF 100-300mm F4 EX DG IF
> 8 | = Minolta AF 70-210mm F4.5-5.6 [II]
> 9 | = Minolta AF 50mm F3.5 Macro
> 10 | = Minolta AF 28-105mm F3.5-4.5 [New]
> 11 | = Minolta AF 300mm F4 HS-APO G
> 12 | = Minolta AF 100mm F2.8 Soft Focus
> 13 | = Minolta AF 75-300mm F4.5-5.6 (New or II)
> 14 | = Minolta AF 100-400mm F4.5-6.7 APO
> 15 | = Minolta AF 400mm F4.5 HS-APO G
> 16 | = Minolta AF 17-35mm F3.5 G
> 17 | = Minolta AF 20-35mm F3.5-4.5
> 18 | = Minolta AF 28-80mm F3.5-5.6 II
> 19 | = Minolta AF 35mm F1.4 G
> 20 | = Minolta/Sony 135mm F2.8 [T4.5] STF
> 22 | = Minolta AF 35-80mm F4-5.6 II
> 23 | = Minolta AF 200mm F4 Macro APO G
> 24 | = Minolta/Sony AF 24-105mm F3.5-4.5 (D) or Sigma or Tamron Lens
> 24.1 | = Sigma 18-50mm F2.8
> 24.2 | = Sigma 17-70mm F2.8-4.5 DC Macro
> 24.3 | = Sigma 20-40mm F2.8 EX DG Aspherical IF
> 24.4 | = Sigma 18-200mm F3.5-6.3 DC
> 24.5 | = Sigma DC 18-125mm F4-5,6 D
> 24.6 | = Tamron SP AF 28-75mm F2.8 XR Di LD Aspherical [IF] Macro
> 24.7 | = Sigma 15-30mm F3.5-4.5 EX DG Aspherical
> 25 | = Minolta AF 100-300mm F4.5-5.6 APO (D) or Sigma Lens
> 25.1 | = Sigma 100-300mm F4 EX (APO (D) or D IF)
> 25.2 | = Sigma 70mm F2.8 EX DG Macro
> 25.3 | = Sigma 20mm F1.8 EX DG Aspherical RF
> 25.4 | = Sigma 30mm F1.4 EX DC
> 25.5 | = Sigma 24mm F1.8 EX DG ASP Macro
> 27 | = Minolta AF 85mm F1.4 G (D)
> 28 | = Minolta/Sony AF 100mm F2.8 Macro (D) or Tamron Lens
> 28.1 | = Tamron SP AF 90mm F2.8 Di Macro
> 28.2 | = Tamron SP AF 180mm F3.5 Di LD [IF] Macro
> 29 | = Minolta/Sony AF 75-300mm F4.5-5.6 (D)
> 30 | = Minolta AF 28-80mm F3.5-5.6 (D) or Sigma Lens
> 30.1 | = Sigma AF 10-20mm F4-5.6 EX DC
> 30.2 | = Sigma AF 12-24mm F4.5-5.6 EX DG
> 30.3 | = Sigma 28-70mm EX DG F2.8
> 30.4 | = Sigma 55-200mm F4-5.6 DC
> 31 | = Minolta/Sony AF 50mm F2.8 Macro (D) or F3.5
> 31.1 | = Minolta/Sony AF 50mm F3.5 Macro
> 32 | = Minolta/Sony AF 300mm F2.8 G or 1.5x Teleconverter
> 33 | = Minolta/Sony AF 70-200mm F2.8 G
> 35 | = Minolta AF 85mm F1.4 G (D) Limited
> 36 | = Minolta AF 28-100mm F3.5-5.6 (D)
> 38 | = Minolta AF 17-35mm F2.8-4 (D)
> 39 | = Minolta AF 28-75mm F2.8 (D)
> 40 | = Minolta/Sony AF DT 18-70mm F3.5-5.6 (D)
> 41 | = Minolta/Sony AF DT 11-18mm F4.5-5.6 (D) or Tamron Lens
> 41.1 | = Tamron SP AF 11-18mm F4.5-5.6 Di II LD Aspherical IF
> 42 | = Minolta/Sony AF DT 18-200mm F3.5-6.3 (D)
> 43 | = Sony 35mm F1.4 G (SAL35F14G)
> 44 | = Sony 50mm F1.4 (SAL50F14)
> 45 | = Carl Zeiss Planar T* 85mm F1.4 ZA (SAL85F14Z)
> 46 | = Carl Zeiss Vario-Sonnar T* DT 16-80mm F3.5-4.5 ZA (SAL1680Z)
> 47 | = Carl Zeiss Sonnar T* 135mm F1.8 ZA (SAL135F18Z)
> 48 | = Carl Zeiss Vario-Sonnar T* 24-70mm F2.8 ZA SSM (SAL2470Z) or Other Lens
> 48.1 | = Carl Zeiss Vario-Sonnar T* 24-70mm F2.8 ZA SSM II (SAL2470Z2)
> 48.2 | = Tamron SP 24-70mm F2.8 Di USD
> 49 | = Sony DT 55-200mm F4-5.6 (SAL55200)
> 50 | = Sony DT 18-250mm F3.5-6.3 (SAL18250)
> 51 | = Sony DT 16-105mm F3.5-5.6 (SAL16105)
> 52 | = Sony 70-300mm F4.5-5.6 G SSM (SAL70300G) or G SSM II or Tamron Lens
> 52.1 | = Sony 70-300mm F4.5-5.6 G SSM II (SAL70300G2)
> 52.2 | = Tamron SP 70-300mm F4-5.6 Di USD
> 53 | = Sony 70-400mm F4-5.6 G SSM (SAL70400G)
> 54 | = Carl Zeiss Vario-Sonnar T* 16-35mm F2.8 ZA SSM (SAL1635Z) or ZA SSM II
> 54.1 | = Carl Zeiss Vario-Sonnar T* 16-35mm F2.8 ZA SSM II (SAL1635Z2)
> 55 | = Sony DT 18-55mm F3.5-5.6 SAM (SAL1855) or SAM II
> 55.1 | = Sony DT 18-55mm F3.5-5.6 SAM II (SAL18552)
> 56 | = Sony DT 55-200mm F4-5.6 SAM (SAL55200-2)
> 57 | = Sony DT 50mm F1.8 SAM (SAL50F18) or Tamron Lens or Commlite CM-EF-NEX adapter
> 57.1 | = Tamron SP AF 60mm F2 Di II LD [IF] Macro 1:1
> 57.2 | = Tamron 18-270mm F3.5-6.3 Di II PZD
> 58 | = Sony DT 30mm F2.8 Macro SAM (SAL30M28)
> 59 | = Sony 28-75mm F2.8 SAM (SAL2875)
> 60 | = Carl Zeiss Distagon T* 24mm F2 ZA SSM (SAL24F20Z)
> 61 | = Sony 85mm F2.8 SAM (SAL85F28)
> 62 | = Sony DT 35mm F1.8 SAM (SAL35F18)
> 63 | = Sony DT 16-50mm F2.8 SSM (SAL1650)
> 64 | = Sony 500mm F4 G SSM (SAL500F40G)
> 65 | = Sony DT 18-135mm F3.5-5.6 SAM (SAL18135)
> 66 | = Sony 300mm F2.8 G SSM II (SAL300F28G2)
> 67 | = Sony 70-200mm F2.8 G SSM II (SAL70200G2)
> 68 | = Sony DT 55-300mm F4.5-5.6 SAM (SAL55300)
> 69 | = Sony 70-400mm F4-5.6 G SSM II (SAL70400G2)
> 70 | = Carl Zeiss Planar T* 50mm F1.4 ZA SSM (SAL50F14Z)
> 128 | = Tamron or Sigma Lens (128)
> 128.1 | = Tamron AF 18-200mm F3.5-6.3 XR Di II LD Aspherical [IF] Macro
> 128.2 | = Tamron AF 28-300mm F3.5-6.3 XR Di LD Aspherical [IF] Macro
> 128.3 | = Tamron AF 28-200mm F3.8-5.6 XR Di Aspherical [IF] Macro
> 128.4 | = Tamron SP AF 17-35mm F2.8-4 Di LD Aspherical IF
> 128.5 | = Sigma AF 50-150mm F2.8 EX DC APO HSM II
> 128.6 | = Sigma 10-20mm F3.5 EX DC HSM
> 128.7 | = Sigma 70-200mm F2.8 II EX DG APO MACRO HSM
> 128.8 | = Sigma 10mm F2.8 EX DC HSM Fisheye
> 128.9 | = Sigma 50mm F1.4 EX DG HSM
> 128.10 | = Sigma 85mm F1.4 EX DG HSM
> 128.11 | = Sigma 24-70mm F2.8 IF EX DG HSM
> 128.12 | = Sigma 18-250mm F3.5-6.3 DC OS HSM
> 128.13 | = Sigma 17-50mm F2.8 EX DC HSM
> 128.14 | = Sigma 17-70mm F2.8-4 DC Macro HSM
> 128.15 | = Sigma 150mm F2.8 EX DG OS HSM APO Macro
> 128.16 | = Sigma 150-500mm F5-6.3 APO DG OS HSM
> 128.17 | = Tamron AF 28-105mm F4-5.6 [IF]
> 128.18 | = Sigma 35mm F1.4 DG HSM
> 128.19 | = Sigma 18-35mm F1.8 DC HSM
> 128.20 | = Sigma 50-500mm F4.5-6.3 APO DG OS HSM
> 128.21 | = Sigma 24-105mm F4 DG HSM | A
> 128.22 | = Sigma 30mm F1.4
> 128.23 | = Sigma 35mm F1.4 DG HSM | A
> 128.24 | = Sigma 105mm F2.8 EX DG OS HSM Macro
> 128.25 | = Sigma 180mm F2.8 EX DG OS HSM APO Macro
> 128.26 | = Sigma 18-300mm F3.5-6.3 DC Macro HSM | C
> 128.27 | = Sigma 18-50mm F2.8-4.5 DC HSM
> 129 | = Tamron Lens (129)
> 129.1 | = Tamron 200-400mm F5.6 LD
> 129.2 | = Tamron 70-300mm F4-5.6 LD
> 131 | = Tamron 20-40mm F2.7-3.5 SP Aspherical IF
> 135 | = Vivitar 28-210mm F3.5-5.6
> 136 | = Tokina EMZ M100 AF 100mm F3.5
> 137 | = Cosina 70-210mm F2.8-4 AF
> 138 | = Soligor 19-35mm F3.5-4.5
> 139 | = Tokina AF 28-300mm F4-6.3
> 142 | = Cosina AF 70-300mm F4.5-5.6 MC
> 146 | = Voigtlander Macro APO-Lanthar 125mm F2.5 SL
> 194 | = Tamron SP AF 17-50mm F2.8 XR Di II LD Aspherical [IF]
> 202 | = Tamron SP AF 70-200mm F2.8 Di LD [IF] Macro
> 203 | = Tamron SP 70-200mm F2.8 Di USD
> 204 | = Tamron SP 24-70mm F2.8 Di USD
> 212 | = Tamron 28-300mm F3.5-6.3 Di PZD
> 213 | = Tamron 16-300mm F3.5-6.3 Di II PZD Macro
> 214 | = Tamron SP 150-600mm F5-6.3 Di USD
> 215 | = Tamron SP 15-30mm F2.8 Di USD
> 216 | = Tamron SP 45mm F1.8 Di USD
> 217 | = Tamron SP 35mm F1.8 Di USD
> 218 | = Tamron SP 90mm F2.8 Di Macro 1:1 USD (F017)
> 220 | = Tamron SP 150-600mm F5-6.3 Di USD G2
> 224 | = Tamron SP 90mm F2.8 Di Macro 1:1 USD (F004)
> 255 | = Tamron Lens (255)
> 255.1 | = Tamron SP AF 17-50mm F2.8 XR Di II LD Aspherical
> 255.2 | = Tamron AF 18-250mm F3.5-6.3 XR Di II LD
> 255.3 | = Tamron AF 55-200mm F4-5.6 Di II LD Macro
> 255.4 | = Tamron AF 70-300mm F4-5.6 Di LD Macro 1:2
> 255.5 | = Tamron SP AF 200-500mm F5.0-6.3 Di LD IF
> 255.6 | = Tamron SP AF 10-24mm F3.5-4.5 Di II LD Aspherical IF
> 255.7 | = Tamron SP AF 70-200mm F2.8 Di LD IF Macro
> 255.8 | = Tamron SP AF 28-75mm F2.8 XR Di LD Aspherical IF
> 255.9 | = Tamron AF 90-300mm F4.5-5.6 Telemacro
> 1868 | = Sigma MC-11 SA-E Mount Converter with not-supported Sigma lens
> 2550 | = Minolta AF 50mm F1.7
> 2551 | = Minolta AF 35-70mm F4 or Other Lens
> 2551.1 | = Sigma UC AF 28-70mm F3.5-4.5
> 2551.2 | = Sigma AF 28-70mm F2.8
> 2551.3 | = Sigma M-AF 70-200mm F2.8 EX Aspherical
> 2551.4 | = Quantaray M-AF 35-80mm F4-5.6
> 2551.5 | = Tokina 28-70mm F2.8-4.5 AF
> 2552 | = Minolta AF 28-85mm F3.5-4.5 or Other Lens
> 2552.1 | = Tokina 19-35mm F3.5-4.5
> 2552.2 | = Tokina 28-70mm F2.8 AT-X
> 2552.3 | = Tokina 80-400mm F4.5-5.6 AT-X AF II 840
> 2552.4 | = Tokina AF PRO 28-80mm F2.8 AT-X 280
> 2552.5 | = Tokina AT-X PRO [II] AF 28-70mm F2.6-2.8 270
> 2552.6 | = Tamron AF 19-35mm F3.5-4.5
> 2552.7 | = Angenieux AF 28-70mm F2.6
> 2552.8 | = Tokina AT-X 17 AF 17mm F3.5
> 2552.9 | = Tokina 20-35mm F3.5-4.5 II AF
> 2553 | = Minolta AF 28-135mm F4-4.5 or Other Lens
> 2553.1 | = Sigma ZOOM-alpha 35-135mm F3.5-4.5
> 2553.2 | = Sigma 28-105mm F2.8-4 Aspherical
> 2553.3 | = Sigma 28-105mm F4-5.6 UC
> 2553.4 | = Tokina AT-X 242 AF 24-200mm F3.5-5.6
> 2554 | = Minolta AF 35-105mm F3.5-4.5
> 2555 | = Minolta AF 70-210mm F4 Macro or Sigma Lens
> 2555.1 | = Sigma 70-210mm F4-5.6 APO
> 2555.2 | = Sigma M-AF 70-200mm F2.8 EX APO
> 2555.3 | = Sigma 75-200mm F2.8-3.5
> 2556 | = Minolta AF 135mm F2.8
> 2557 | = Minolta/Sony AF 28mm F2.8
> 2558 | = Minolta AF 24-50mm F4
> 2560 | = Minolta AF 100-200mm F4.5
> 2561 | = Minolta AF 75-300mm F4.5-5.6 or Sigma Lens
> 2561.1 | = Sigma 70-300mm F4-5.6 DL Macro
> 2561.2 | = Sigma 300mm F4 APO Macro
> 2561.3 | = Sigma AF 500mm F4.5 APO
> 2561.4 | = Sigma AF 170-500mm F5-6.3 APO Aspherical
> 2561.5 | = Tokina AT-X AF 300mm F4
> 2561.6 | = Tokina AT-X AF 400mm F5.6 SD
> 2561.7 | = Tokina AF 730 II 75-300mm F4.5-5.6
> 2561.8 | = Sigma 800mm F5.6 APO
> 2561.9 | = Sigma AF 400mm F5.6 APO Macro
> 2561.10 | = Sigma 1000mm F8 APO
> 2562 | = Minolta AF 50mm F1.4 [New]
> 2563 | = Minolta AF 300mm F2.8 APO or Sigma Lens
> 2563.1 | = Sigma AF 50-500mm F4-6.3 EX DG APO
> 2563.2 | = Sigma AF 170-500mm F5-6.3 APO Aspherical
> 2563.3 | = Sigma AF 500mm F4.5 EX DG APO
> 2563.4 | = Sigma 400mm F5.6 APO
> 2564 | = Minolta AF 50mm F2.8 Macro or Sigma Lens
> 2564.1 | = Sigma 50mm F2.8 EX Macro
> 2565 | = Minolta AF 600mm F4 APO
> 2566 | = Minolta AF 24mm F2.8 or Sigma Lens
> 2566.1 | = Sigma 17-35mm F2.8-4 EX Aspherical
> 2572 | = Minolta/Sony AF 500mm F8 Reflex
> 2578 | = Minolta/Sony AF 16mm F2.8 Fisheye or Sigma Lens
> 2578.1 | = Sigma 8mm F4 EX [DG] Fisheye
> 2578.2 | = Sigma 14mm F3.5
> 2578.3 | = Sigma 15mm F2.8 Fisheye
> 2579 | = Minolta/Sony AF 20mm F2.8 or Tokina Lens
> 2579.1 | = Tokina AT-X Pro DX 11-16mm F2.8
> 2581 | = Minolta AF 100mm F2.8 Macro [New] or Sigma or Tamron Lens
> 2581.1 | = Sigma AF 90mm F2.8 Macro
> 2581.2 | = Sigma AF 105mm F2.8 EX [DG] Macro
> 2581.3 | = Sigma 180mm F5.6 Macro
> 2581.4 | = Sigma 180mm F3.5 EX DG Macro
> 2581.5 | = Tamron 90mm F2.8 Macro
> 2585 | = Minolta AF 35-105mm F3.5-4.5 New or Tamron Lens
> 2585.1 | = Beroflex 35-135mm F3.5-4.5
> 2585.2 | = Tamron 24-135mm F3.5-5.6
> 2588 | = Minolta AF 70-210mm F3.5-4.5
> 2589 | = Minolta AF 80-200mm F2.8 APO or Tokina Lens
> 2589.1 | = Tokina 80-200mm F2.8
> 2590 | = Minolta AF 200mm F2.8 G APO + Minolta AF 1.4x APO or Other Lens + 1.4x
> 2590.1 | = Minolta AF 600mm F4 HS-APO G + Minolta AF 1.4x APO
> 2591 | = Minolta AF 35mm F1.4
> 2592 | = Minolta AF 85mm F1.4 G (D)
> 2593 | = Minolta AF 200mm F2.8 APO
> 2594 | = Minolta AF 3x-1x F1.7-2.8 Macro
> 2596 | = Minolta AF 28mm F2
> 2597 | = Minolta AF 35mm F2 [New]
> 2598 | = Minolta AF 100mm F2
> 2601 | = Minolta AF 200mm F2.8 G APO + Minolta AF 2x APO or Other Lens + 2x
> 2601.1 | = Minolta AF 600mm F4 HS-APO G + Minolta AF 2x APO
> 2604 | = Minolta AF 80-200mm F4.5-5.6
> 2605 | = Minolta AF 35-80mm F4-5.6
> 2606 | = Minolta AF 100-300mm F4.5-5.6
> 2607 | = Minolta AF 35-80mm F4-5.6
> 2608 | = Minolta AF 300mm F2.8 HS-APO G
> 2609 | = Minolta AF 600mm F4 HS-APO G
> 2612 | = Minolta AF 200mm F2.8 HS-APO G
> 2613 | = Minolta AF 50mm F1.7 New
> 2615 | = Minolta AF 28-105mm F3.5-4.5 xi
> 2616 | = Minolta AF 35-200mm F4.5-5.6 xi
> 2618 | = Minolta AF 28-80mm F4-5.6 xi
> 2619 | = Minolta AF 80-200mm F4.5-5.6 xi
> 2620 | = Minolta AF 28-70mm F2.8 G
> 2621 | = Minolta AF 100-300mm F4.5-5.6 xi
> 2624 | = Minolta AF 35-80mm F4-5.6 Power Zoom
> 2628 | = Minolta AF 80-200mm F2.8 HS-APO G
> 2629 | = Minolta AF 85mm F1.4 New
> 2631 | = Minolta AF 100-300mm F4.5-5.6 APO
> 2632 | = Minolta AF 24-50mm F4 New
> 2638 | = Minolta AF 50mm F2.8 Macro New
> 2639 | = Minolta AF 100mm F2.8 Macro
> 2641 | = Minolta/Sony AF 20mm F2.8 New
> 2642 | = Minolta AF 24mm F2.8 New
> 2644 | = Minolta AF 100-400mm F4.5-6.7 APO
> 2662 | = Minolta AF 50mm F1.4 New
> 2667 | = Minolta AF 35mm F2 New
> 2668 | = Minolta AF 28mm F2 New
> 2672 | = Minolta AF 24-105mm F3.5-4.5 (D)
> 3046 | = Metabones Canon EF Speed Booster
> 4567 | = Tokina 70-210mm F4-5.6
> 4568 | = Tokina AF 35-200mm F4-5.6 Zoom SD
> 4570 | = Tamron AF 35-135mm F3.5-4.5
> 4571 | = Vivitar 70-210mm F4.5-5.6
> 4574 | = 2x Teleconverter or Tamron or Tokina Lens
> 4574.1 | = Tamron SP AF 90mm F2.5
> 4574.2 | = Tokina RF 500mm F8.0 x2
> 4574.3 | = Tokina 300mm F2.8 x2
> 4575 | = 1.4x Teleconverter
> 4585 | = Tamron SP AF 300mm F2.8 LD IF
> 4586 | = Tamron SP AF 35-105mm F2.8 LD Aspherical IF
> 4587 | = Tamron AF 70-210mm F2.8 SP LD
> 4812 | = Metabones Canon EF Speed Booster Ultra
> 6118 | = Canon EF Adapter
> 6528 | = Sigma 16mm F2.8 Filtermatic Fisheye
> 6553 | = E-Mount, T-Mount, Other Lens or no lens
> 6553.1 | = Arax MC 35mm F2.8 Tilt+Shift
> 6553.2 | = Arax MC 80mm F2.8 Tilt+Shift
> 6553.3 | = Zenitar MF 16mm F2.8 Fisheye M42
> 6553.4 | = Samyang 500mm Mirror F8.0
> 6553.5 | = Pentacon Auto 135mm F2.8
> 6553.6 | = Pentacon Auto 29mm F2.8
> 6553.7 | = Helios 44-2 58mm F2.0
> 18688 | = Sigma MC-11 SA-E Mount Converter with not-supported Sigma lens
> 25501 | = Minolta AF 50mm F1.7
> 25511 | = Minolta AF 35-70mm F4 or Other Lens
> 25511.1 | = Sigma UC AF 28-70mm F3.5-4.5
> 25511.2 | = Sigma AF 28-70mm F2.8
> 25511.3 | = Sigma M-AF 70-200mm F2.8 EX Aspherical
> 25511.4 | = Quantaray M-AF 35-80mm F4-5.6
> 25511.5 | = Tokina 28-70mm F2.8-4.5 AF
> 25521 | = Minolta AF 28-85mm F3.5-4.5 or Other Lens
> 25521.1 | = Tokina 19-35mm F3.5-4.5
> 25521.2 | = Tokina 28-70mm F2.8 AT-X
> 25521.3 | = Tokina 80-400mm F4.5-5.6 AT-X AF II 840
> 25521.4 | = Tokina AF PRO 28-80mm F2.8 AT-X 280
> 25521.5 | = Tokina AT-X PRO [II] AF 28-70mm F2.6-2.8 270
> 25521.6 | = Tamron AF 19-35mm F3.5-4.5
> 25521.7 | = Angenieux AF 28-70mm F2.6
> 25521.8 | = Tokina AT-X 17 AF 17mm F3.5
> 25521.9 | = Tokina 20-35mm F3.5-4.5 II AF
> 25531 | = Minolta AF 28-135mm F4-4.5 or Other Lens
> 25531.1 | = Sigma ZOOM-alpha 35-135mm F3.5-4.5
> 25531.2 | = Sigma 28-105mm F2.8-4 Aspherical
> 25531.3 | = Sigma 28-105mm F4-5.6 UC
> 25531.4 | = Tokina AT-X 242 AF 24-200mm F3.5-5.6
> 25541 | = Minolta AF 35-105mm F3.5-4.5
> 25551 | = Minolta AF 70-210mm F4 Macro or Sigma Lens
> 25551.1 | = Sigma 70-210mm F4-5.6 APO
> 25551.2 | = Sigma M-AF 70-200mm F2.8 EX APO
> 25551.3 | = Sigma 75-200mm F2.8-3.5
> 25561 | = Minolta AF 135mm F2.8
> 25571 | = Minolta/Sony AF 28mm F2.8
> 25581 | = Minolta AF 24-50mm F4
> 25601 | = Minolta AF 100-200mm F4.5
> 25611 | = Minolta AF 75-300mm F4.5-5.6 or Sigma Lens
> 25611.1 | = Sigma 70-300mm F4-5.6 DL Macro
> 25611.2 | = Sigma 300mm F4 APO Macro
> 25611.3 | = Sigma AF 500mm F4.5 APO
> 25611.4 | = Sigma AF 170-500mm F5-6.3 APO Aspherical
> 25611.5 | = Tokina AT-X AF 300mm F4
> 25611.6 | = Tokina AT-X AF 400mm F5.6 SD
> 25611.7 | = Tokina AF 730 II 75-300mm F4.5-5.6
> 25611.8 | = Sigma 800mm F5.6 APO
> 25611.9 | = Sigma AF 400mm F5.6 APO Macro
> 25611.10 | = Sigma 1000mm F8 APO
> 25621 | = Minolta AF 50mm F1.4 [New]
> 25631 | = Minolta AF 300mm F2.8 APO or Sigma Lens
> 25631.1 | = Sigma AF 50-500mm F4-6.3 EX DG APO
> 25631.2 | = Sigma AF 170-500mm F5-6.3 APO Aspherical
> 25631.3 | = Sigma AF 500mm F4.5 EX DG APO
> 25631.4 | = Sigma 400mm F5.6 APO
> 25641 | = Minolta AF 50mm F2.8 Macro or Sigma Lens
> 25641.1 | = Sigma 50mm F2.8 EX Macro
> 25651 | = Minolta AF 600mm F4 APO
> 25661 | = Minolta AF 24mm F2.8 or Sigma Lens
> 25661.1 | = Sigma 17-35mm F2.8-4 EX Aspherical
> 25721 | = Minolta/Sony AF 500mm F8 Reflex
> 25781 | = Minolta/Sony AF 16mm F2.8 Fisheye or Sigma Lens
> 25781.1 | = Sigma 8mm F4 EX [DG] Fisheye
> 25781.2 | = Sigma 14mm F3.5
> 25781.3 | = Sigma 15mm F2.8 Fisheye
> 25791 | = Minolta/Sony AF 20mm F2.8 or Tokina Lens
> 25791.1 | = Tokina AT-X Pro DX 11-16mm F2.8
> 25811 | = Minolta AF 100mm F2.8 Macro [New] or Sigma or Tamron Lens
> 25811.1 | = Sigma AF 90mm F2.8 Macro
> 25811.2 | = Sigma AF 105mm F2.8 EX [DG] Macro
> 25811.3 | = Sigma 180mm F5.6 Macro
> 25811.4 | = Sigma 180mm F3.5 EX DG Macro
> 25811.5 | = Tamron 90mm F2.8 Macro
> 25851 | = Beroflex 35-135mm F3.5-4.5
> 25858 | = Minolta AF 35-105mm F3.5-4.5 New or Tamron Lens
> 25858.1 | = Tamron 24-135mm F3.5-5.6
> 25881 | = Minolta AF 70-210mm F3.5-4.5
> 25891 | = Minolta AF 80-200mm F2.8 APO or Tokina Lens
> 25891.1 | = Tokina 80-200mm F2.8
> 25901 | = Minolta AF 200mm F2.8 G APO + Minolta AF 1.4x APO or Other Lens + 1.4x
> 25901.1 | = Minolta AF 600mm F4 HS-APO G + Minolta AF 1.4x APO
> 25911 | = Minolta AF 35mm F1.4
> 25921 | = Minolta AF 85mm F1.4 G (D)
> 25931 | = Minolta AF 200mm F2.8 APO
> 25941 | = Minolta AF 3x-1x F1.7-2.8 Macro
> 25961 | = Minolta AF 28mm F2
> 25971 | = Minolta AF 35mm F2 [New]
> 25981 | = Minolta AF 100mm F2
> 26011 | = Minolta AF 200mm F2.8 G APO + Minolta AF 2x APO or Other Lens + 2x
> 26011.1 | = Minolta AF 600mm F4 HS-APO G + Minolta AF 2x APO
> 26041 | = Minolta AF 80-200mm F4.5-5.6
> 26051 | = Minolta AF 35-80mm F4-5.6
> 26061 | = Minolta AF 100-300mm F4.5-5.6
> 26071 | = Minolta AF 35-80mm F4-5.6
> 26081 | = Minolta AF 300mm F2.8 HS-APO G
> 26091 | = Minolta AF 600mm F4 HS-APO G
> 26121 | = Minolta AF 200mm F2.8 HS-APO G
> 26131 | = Minolta AF 50mm F1.7 New
> 26151 | = Minolta AF 28-105mm F3.5-4.5 xi
> 26161 | = Minolta AF 35-200mm F4.5-5.6 xi
> 26181 | = Minolta AF 28-80mm F4-5.6 xi
> 26191 | = Minolta AF 80-200mm F4.5-5.6 xi
> 26201 | = Minolta AF 28-70mm F2.8 G
> 26211 | = Minolta AF 100-300mm F4.5-5.6 xi
> 26241 | = Minolta AF 35-80mm F4-5.6 Power Zoom
> 26281 | = Minolta AF 80-200mm F2.8 HS-APO G
> 26291 | = Minolta AF 85mm F1.4 New
> 26311 | = Minolta AF 100-300mm F4.5-5.6 APO
> 26321 | = Minolta AF 24-50mm F4 New
> 26381 | = Minolta AF 50mm F2.8 Macro New
> 26391 | = Minolta AF 100mm F2.8 Macro
> 26411 | = Minolta/Sony AF 20mm F2.8 New
> 26421 | = Minolta AF 24mm F2.8 New
> 26441 | = Minolta AF 100-400mm F4.5-6.7 APO
> 26621 | = Minolta AF 50mm F1.4 New
> 26671 | = Minolta AF 35mm F2 New
> 26681 | = Minolta AF 28mm F2 New
> 26721 | = Minolta AF 24-105mm F3.5-4.5 (D)
> 30464 | = Metabones Canon EF Speed Booster
> 45671 | = Tokina 70-210mm F4-5.6
> 45681 | = Tokina AF 35-200mm F4-5.6 Zoom SD
> 45701 | = Tamron AF 35-135mm F3.5-4.5
> 45711 | = Vivitar 70-210mm F4.5-5.6
> 45741 | = 2x Teleconverter or Tamron or Tokina Lens
> 45741.1 | = Tamron SP AF 90mm F2.5
> 45741.2 | = Tokina RF 500mm F8.0 x2
> 45741.3 | = Tokina 300mm F2.8 x2
> 45751 | = 1.4x Teleconverter
> 45851 | = Tamron SP AF 300mm F2.8 LD IF
> 45861 | = Tamron SP AF 35-105mm F2.8 LD Aspherical IF
> 45871 | = Tamron AF 70-210mm F2.8 SP LD
> 48128 | = Metabones Canon EF Speed Booster Ultra
> 61184 | = Canon EF Adapter
> 65280 | = Sigma 16mm F2.8 Filtermatic Fisheye
> 65535 | = E-Mount, T-Mount, Other Lens or no lens
> 65535.1 | = Arax MC 35mm F2.8 Tilt+Shift
> 65535.2 | = Arax MC 80mm F2.8 Tilt+Shift
> 65535.3 | = Zenitar MF 16mm F2.8 Fisheye M42
> 65535.4 | = Samyang 500mm Mirror F8.0
> 65535.5 | = Pentacon Auto 135mm F2.8
> 65535.6 | = Pentacon Auto 29mm F2.8
> 65535.7 | = Helios 44-2 58mm F2.0

## Sony CameraInfo Tags

Camera information for the A700, A850 and A900.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensSpec | undef[8] |
> 20 | FocusModeSetting | int8u | (FocusModeSetting for the A700, A850 and A900) 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A 4 = DMF
> 21 | AFPointSelected | int8u |
> 0 = Auto 1 = Center 2 = Top 3 = Upper-right 4 = Right 5 = Lower-right |  | 6 = Bottom 7 = Lower-left 8 = Left 9 = Upper-left 10 = Far Right 11 = Far Left
> 25 | AFPoint | int8u |
> 0 = Upper-left 1 = Left 2 = Lower-left 3 = Far Left 4 = Bottom Assist-left 5 = Bottom 6 = Bottom Assist-right 7 = Center (7) 8 = Center (horizontal) 9 = Center (9) 10 = Center (10) 11 = Center (11) |  | 12 = Center (12) 13 = Center (vertical) 14 = Center (14) 15 = Top Assist-left 16 = Top 17 = Top Assist-right 18 = Far Right 19 = Upper-right 20 = Right 21 = Lower-right 22 = Center F2.8
> 30 | AFStatusActiveSensor | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 32 | AFStatusUpper-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 34 | AFStatusLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 36 | AFStatusLower-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 38 | AFStatusFarLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 40 | AFStatusBottomAssist-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 42 | AFStatusBottom | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 44 | AFStatusBottomAssist-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 46 | AFStatusCenter-7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 48 | AFStatusCenter-horizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 50 | AFStatusCenter-9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 52 | AFStatusCenter-10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 54 | AFStatusCenter-11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 56 | AFStatusCenter-12 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 58 | AFStatusCenter-vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 60 | AFStatusCenter-14 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 62 | AFStatusTopAssist-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 64 | AFStatusTop | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 66 | AFStatusTopAssist-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 68 | AFStatusFarRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 70 | AFStatusUpper-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 72 | AFStatusRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 74 | AFStatusLower-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 76 | AFStatusCenterF2-8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 304 | AFMicroAdjValue | int8u |
> 305 | AFMicroAdjMode | int8u | [val >> 7 & 0x1] 0 = Off 1 = On
> 305.1 | AFMicroAdjRegisteredLenses | int8u | (number of registered lenses with a non-zero AFMicroAdjValue) [val & 0x7f]

## Sony CameraInfo2 Tags

Camera information for the DSLR-A200, A230, A290, A300, A330, A350, A380 and A390.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensSpec | undef[8] |
> 20 | AFPointSelected | int8u |
> 0 = Auto 1 = Center 2 = Top 3 = Upper-right 4 = Right |  | 5 = Lower-right 6 = Bottom 7 = Lower-left 8 = Left 9 = Upper-left
> 21 | FocusModeSetting | int8u | (FocusModeSetting for other models) 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A 4 = DMF
> 24 | AFPoint | int8u |
> 0 = Top-right 1 = Bottom-right 2 = Bottom 3 = Middle Horizontal |  | 4 = Center Vertical 5 = Top 6 = Top-left 7 = Bottom-left
> 27 | AFStatusActiveSensor | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 29 | AFStatusTop-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 31 | AFStatusBottom-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 33 | AFStatusBottom | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 35 | AFStatusMiddleHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 37 | AFStatusCenterVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 39 | AFStatusTop | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 41 | AFStatusTop-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 43 | AFStatusBottom-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 45 | AFStatusLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 47 | AFStatusCenterHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 49 | AFStatusRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus

## Sony CameraInfo3 Tags

Camera information stored by the A33, A35, A55, A450, A500, A550, A560, A580, NEX-3/5/5C/C3 and VG10E. Some tags are valid only for some of these models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | LensSpec | undef[8] |
> 14 | FocalLength | int16u |
> 16 | FocalLengthTeleZoom | int16u |
> 20 | AFPointSelected | int8u |
> 0 = Auto 1 = Center 2 = Top 3 = Upper-right 4 = Right |  | 5 = Lower-right 6 = Bottom 7 = Lower-left 8 = Left 9 = Upper-left
> 21 | FocusMode | int8u | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A
> 24 | AFPoint | int8u |
> 0 = Top-right 1 = Bottom-right 2 = Bottom 3 = Middle Horizontal |  | 4 = Center Vertical 5 = Top 6 = Top-left 7 = Bottom-left
> 25 | FocusStatus | int8u | (not valid with Contrast AF or for NEX models) 0 = Manual - Not confirmed (0) 4 = Manual - Not confirmed (4) 16 = AF-C - Confirmed 24 = AF-C - Not Confirmed 64 = AF-S - Confirmed
> 27 | AFStatusActiveSensor | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 28 | AFPointSelected | int8u | (not valid for Contrast AF)
> 0 = Auto 1 = Center 2 = Top 3 = Upper-right 4 = Right 5 = Lower-right 6 = Bottom 7 = Lower-left |  | 8 = Left 9 = Upper-left 10 = Far Right 11 = Far Left 12 = Upper-middle 13 = Near Right 14 = Lower-middle 15 = Near Left
> 29 | FocusMode AFStatusTop-right | int8u int16s | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A
> -32768 = Out of Focus |  | 0 = In Focus
> 31 | AFStatusBottom-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 32 | AFPoint | int8u | (the AF sensor used for focusing. Not valid for Contrast AF)
> 0 = Upper-left 1 = Left 2 = Lower-left 3 = Far Left 4 = Top (horizontal) 5 = Near Right 6 = Center (horizontal) 7 = Near Left 8 = Bottom (horizontal) 9 = Top (vertical) |  | 10 = Center (vertical) 11 = Bottom (vertical) 12 = Far Right 13 = Upper-right 14 = Right 15 = Lower-right 16 = Upper-middle 17 = Lower-middle 255 = (none)
> 33 | AFStatusActiveSensor AFStatusBottom | int16s int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> -32768 = Out of Focus |  | 0 = In Focus
> 35 | AFStatus15 AFStatusMiddleHorizontal | - int16s | --> Sony AFStatus15 Tags
> -32768 = Out of Focus |  | 0 = In Focus
> 37 | AFStatusCenterVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 39 | AFStatusTop | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 41 | AFStatusTop-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 43 | AFStatusBottom-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 45 | AFStatusLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 47 | AFStatusCenterHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 49 | AFStatusRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus

## Sony AFStatus15 Tags

AF Status information for models with 15-point AF.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFStatusUpper-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 2 | AFStatusLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 4 | AFStatusLower-left | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 6 | AFStatusFarLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 8 | AFStatusTopHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 10 | AFStatusNearRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 12 | AFStatusCenterHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 14 | AFStatusNearLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 16 | AFStatusBottomHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 18 | AFStatusTopVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 20 | AFStatusCenterVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 22 | AFStatusBottomVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 24 | AFStatusFarRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 26 | AFStatusUpper-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 28 | AFStatusRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 30 | AFStatusLower-right | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 32 | AFStatusUpper-middle | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 34 | AFStatusLower-middle | int16s |
> -32768 = Out of Focus |  | 0 = In Focus

## Sony CameraInfoUnknown Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Sony FocusInfo Tags

More camera settings and focus information decoded for models such as the A200, A230, A290, A300, A330, A350, A380, A390, A700, A850 and A900.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 14 | DriveMode2 | int8u | (A230, A290, A330, A380 and A390)
> 0x1 = Single Frame 0x2 = Continuous High 0x4 = Self-timer 10 sec 0x5 = Self-timer 2 sec, Mirror Lock-up 0x7 = Continuous Bracketing 0xa = Remote Commander 0xb = Continuous Self-timer
> (A200, A300, A350, A700, A850 and A900)
> 0x1 = Single Frame 0x2 = Continuous High 0x4 = Self-timer 10 sec 0x5 = Self-timer 2 sec, Mirror Lock-up 0x6 = Single-frame Bracketing 0x7 = Continuous Bracketing 0xa = Remote Commander 0xb = Mirror Lock-up 0x12 = Continuous Low 0x18 = White Balance Bracketing Low 0x19 = D-Range Optimizer Bracketing Low 0x28 = White Balance Bracketing High 0x29 = D-Range Optimizer Bracketing High
> 16 | Rotation | int8u | 0 = Horizontal (normal) 1 = Rotate 270 CW 2 = Rotate 90 CW
> 20 | ImageStabilizationSetting | int8u | 0 = Off 1 = On
> 21 | DynamicRangeOptimizerMode | int8u | 0 = Off 1 = Standard 2 = Advanced Auto 3 = Advanced Level
> 43 | BracketShotNumber | int8u | (WB and DRO bracketing)
> 44 | WhiteBalanceBracketing | int8u | 0 = Off 1 = Low 2 = High
> 45 | BracketShotNumber2 | int8u |
> 46 | DynamicRangeOptimizerBracket | int8u | 0 = Off 1 = Low 2 = High
> 47 | ExposureBracketShotNumber | int8u |
> 63 | ExposureProgram | int8u | --> Sony ExposureProgram Values
> 65 | CreativeStyle | int8u |
> 1 = Standard 2 = Vivid 3 = Portrait 4 = Landscape 5 = Sunset 6 = Night View/Portrait 8 = B&W |  | 9 = Adobe RGB 11 = Neutral 12 = Clear 13 = Deep 14 = Light 15 = Autumn Leaves 16 = Sepia
> 109 | ISOSetting | int8u |
> 111 | ISO | int8u |
> 119 | DynamicRangeOptimizerMode | int8u | 0 = Off 1 = Standard 2 = Advanced Auto 3 = Advanced Level
> 121 | DynamicRangeOptimizerLevel | int8u |
> 2118 | ShutterCount | int32u | (only valid for some DSLR models)
> 2491 | FocusPosition | int8u | (only valid for some DSLR models)
> 4368 | TiffMeteringImage | no | (13-bit RBGG (?) 40x30 pixels, presumably metering info, extracted as a 16-bit TIFF image;)

## Sony ExposureProgram Values

> Value | ExposureProgram | Value | ExposureProgram | Value | ExposureProgram
> --- | --- | --- | --- | --- | ---
> 0 | = Auto | 8 | = Program Shift A | 19 | = Night Portrait
> 1 | = Manual | 9 | = Program Shift S | 20 | = Landscape
> 2 | = Program AE | 16 | = Portrait | 21 | = Macro
> 3 | = Aperture-priority AE | 17 | = Sports | 35 | = Auto No Flash
> 4 | = Shutter speed priority AE | 18 | = Sunset |  |

## Sony MoreInfo Tags

More camera settings information decoded for the A450, A500, A550, A560, A580, A33, A35, A55, NEX-3/5/C3 and VG10E.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0001 | MoreSettings | - | --> Sony MoreSettings Tags
> 0x0002 | FaceInfo FaceInfoA | - - | --> Sony FaceInfo Tags --> Sony FaceInfoA Tags
> 0x0107 | TiffMeteringImage | no | (10-bit RGB data from the 1200 AE metering segments, extracted as a 16-bit TIFF image)
> 0x0201 | MoreInfo0201 | - | --> Sony MoreInfo0201 Tags
> 0x0401 | MoreInfo0401 | - | --> Sony MoreInfo0401 Tags

## Sony MoreSettings Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | DriveMode2 | int8u |
> 0x10 = Single Frame 0x21 = Continuous High 0x22 = Continuous Low 0x30 = Speed Priority Continuous 0x51 = Self-timer 10 sec 0x52 = Self-timer 2 sec, Mirror Lock-up 0x71 = Continuous Bracketing 0.3 EV 0x75 = Continuous Bracketing 0.7 EV 0x91 = White Balance Bracketing Low 0x92 = White Balance Bracketing High 0xc0 = Remote Commander
> 2 | ExposureProgram | int8u | --> Sony ExposureProgram2 Values
> 3 | MeteringMode | int8u | 1 = Multi-segment 2 = Center-weighted average 3 = Spot
> 4 | DynamicRangeOptimizerSetting | int8u | 1 = Off 16 = On (Auto) 17 = On (Manual)
> 5 | DynamicRangeOptimizerLevel | int8u |
> 6 | ColorSpace | int8u | 1 = sRGB 2 = Adobe RGB
> 7 | CreativeStyleSetting | int8u |
> 16 = Standard 32 = Vivid 64 = Portrait |  | 80 = Landscape 96 = B&W 160 = Sunset
> 8 | ContrastSetting | int8s |
> 9 | SaturationSetting | int8s |
> 10 | SharpnessSetting | int8s |
> 13 | WhiteBalanceSetting | int8u | --> Sony WhiteBalanceSetting Values
> 14 | ColorTemperatureSetting | int8u |
> 15 | ColorCompensationFilterSet | int8s | (negative is green, positive is magenta)
> 16 | FlashMode | int8u |
> 1 = Flash Off 16 = Autoflash 17 = Fill-flash |  | 18 = Slow Sync 19 = Rear Sync 20 = Wireless
> 17 | LongExposureNoiseReduction | int8u | 1 = Off 16 = On
> 18 | HighISONoiseReduction | int8u | 16 = Low 17 = High 19 = Auto
> 19 | FocusMode | int8u | 17 = AF-S 18 = AF-C 19 = AF-A 32 = Manual 48 = DMF
> 21 | MultiFrameNoiseReduction | int8u | 0 = n/a 1 = Off 16 = On 255 = None
> 22 | HDRSetting | int8u | 1 = Off 16 = On (Auto) 17 = On (Manual)
> 23 | HDRLevel | int8u |
> 33 = 1 EV 34 = 1.5 EV 35 = 2 EV |  | 36 = 2.5 EV 37 = 3 EV 38 = 3.5 EV |  | 39 = 4 EV 40 = 5 EV 41 = 6 EV
> 24 | ViewingMode | int8u | 16 = ViewFinder 33 = Focus Check Live View 34 = Quick AF Live View
> 25 | FaceDetection | int8u | 1 = Off 16 = On
> 26 | CustomWB_RBLevels | int16uRev[2] |
> 30 | BrightnessValue ExposureCompensationSet | int8u int8u | (A450, A500 and A550) (other models)
> 31 | ISO FlashExposureCompSet | int8u int8u | (A450, A500 and A550) (other models)
> 32 | FNumber LiveViewAFMethod | int8u int8u | (A450, A500 and A550) (other models except the NEX-3/5/5C) 0 = n/a 1 = Phase-detect AF 2 = Contrast AF
> 33 | ExposureTime ISO | int8u int8u | (A450, A500 and A550) (NEX-3/5/5C)
> 34 | FNumber | int8u | (NEX-3/5/5C only)
> 35 | FocalLength2 ExposureTime | int8u int8u | (A450, A500 and A550) (NEX-3/5/5C)
> 36 | ExposureCompensation2 | int16s | (A450, A500 and A550)
> 37 | FocalLength2 ISO | int8u int8u | (NEX-3/5/5C) (other models except the A450, A500 and A550)
> 38 | FlashExposureCompSet2 ExposureCompensation2 FNumber | int16s int16s int8u | (A450, A500 and A550) (NEX-3/5/5C) (other models)
> 39 | ExposureTime | int8u | (models other than the A450, A500, A550 and NEX-3/5/5C)
> 40 | Orientation2 | int8u | (A450, A500 and A550) 1 = Horizontal (normal) 2 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 41 | FocusPosition2 FocalLength2 | int8u int8u | (A450, A500 and A550) (other models except the NEX-3/5/5C)
> 42 | FlashAction ExposureCompensation2 | int8u int16s | (A450, A500 and A550) 0 = Did not fire 1 = Fired (other models except the NEX-3/5/5C)
> 43 | FocusPosition2 | int8u | (NEX-3/5/5C only)
> 44 | FocusMode2 FlashAction FlashExposureCompSet2 | int8u int8u int16s | (A450, A500 and A550) 0 = AF 1 = MF (NEX-3/5/5C FlashAction2) 0 = Did not fire 1 = Fired (other models FlashExposureCompSet2)
> 46 | FocusMode2 Orientation2 | int8u int8u | (NEX-3/5/5C) 0 = AF 1 = MF (other models except the A450, A500 and A550) 1 = Horizontal (normal) 2 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 47 | FocusPosition2 | int8u | (models other than the A450, A500, A550 and NEX-3/5/5C)
> 48 | FlashAction | int8u | (models other than the A450, A500, A550 and NEX-3/5/5C) 0 = Did not fire 1 = Fired
> 50 | FocusMode2 | int8u | (models other than the A450, A500, A550 and NEX-3/5/5C) 0 = AF 1 = MF
> 119 | FlashAction2 | int8u | 0 = Did not fire 2 = External Flash fired (2) 3 = Built-in Flash fired 4 = External Flash fired (4)
> 120 | FlashActionExternal | int8u | 121 = Fired 122 = Fired 136 = Did not fire
> 124 | FlashActionExternal | int8u | 136 = Did not fire 167 = Fired 182 = Fired, HSS
> 130 | FlashStatus | int8u | 0 = None 2 = External
> 134 | FlashStatus | int8u | 0 = None 1 = Built-in 2 = External

## Sony ExposureProgram2 Values

> Value | ExposureProgram2 | Value | ExposureProgram2 | Value | ExposureProgram2
> --- | --- | --- | --- | --- | ---
> 1 | = Program AE | 52 | = Sports | 129 | = Pop Color
> 2 | = Aperture-priority AE | 53 | = Sunset | 130 | = Posterization
> 3 | = Shutter speed priority AE | 54 | = Night view | 131 | = Posterization B/W
> 4 | = Manual | 55 | = Night view/portrait | 132 | = Retro Photo
> 5 | = Cont. Priority AE | 56 | = Handheld Night Shot | 133 | = High-key
> 16 | = Auto | 57 | = 3D Sweep Panorama | 134 | = Partial Color Red
> 17 | = Auto (no flash) | 64 | = Auto 2 | 135 | = Partial Color Green
> 18 | = Auto+ | 65 | = Auto 2 (no flash) | 136 | = Partial Color Blue
> 49 | = Portrait | 80 | = Sweep Panorama | 137 | = Partial Color Yellow
> 50 | = Landscape | 96 | = Anti Motion Blur | 138 | = High Contrast Monochrome
> 51 | = Macro | 128 | = Toy Camera |  |

## Sony WhiteBalanceSetting Values

> Value | WhiteBalanceSetting | Value | WhiteBalanceSetting
> --- | --- | --- | ---
> 0x10 | = Auto (-3) | 0x45 | = Cloudy (+2)
> 0x11 | = Auto (-2) | 0x46 | = Cloudy (+3)
> 0x12 | = Auto (-1) | 0x50 | = Tungsten (-3)
> 0x13 | = Auto (0) | 0x51 | = Tungsten (-2)
> 0x14 | = Auto (+1) | 0x52 | = Tungsten (-1)
> 0x15 | = Auto (+2) | 0x53 | = Tungsten (0)
> 0x16 | = Auto (+3) | 0x54 | = Tungsten (+1)
> 0x20 | = Daylight (-3) | 0x55 | = Tungsten (+2)
> 0x21 | = Daylight (-2) | 0x56 | = Tungsten (+3)
> 0x22 | = Daylight (-1) | 0x60 | = Fluorescent (-3)
> 0x23 | = Daylight (0) | 0x61 | = Fluorescent (-2)
> 0x24 | = Daylight (+1) | 0x62 | = Fluorescent (-1)
> 0x25 | = Daylight (+2) | 0x63 | = Fluorescent (0)
> 0x26 | = Daylight (+3) | 0x64 | = Fluorescent (+1)
> 0x30 | = Shade (-3) | 0x65 | = Fluorescent (+2)
> 0x31 | = Shade (-2) | 0x66 | = Fluorescent (+3)
> 0x32 | = Shade (-1) | 0x70 | = Flash (-3)
> 0x33 | = Shade (0) | 0x71 | = Flash (-2)
> 0x34 | = Shade (+1) | 0x72 | = Flash (-1)
> 0x35 | = Shade (+2) | 0x73 | = Flash (0)
> 0x36 | = Shade (+3) | 0x74 | = Flash (+1)
> 0x40 | = Cloudy (-3) | 0x75 | = Flash (+2)
> 0x41 | = Cloudy (-2) | 0x76 | = Flash (+3)
> 0x42 | = Cloudy (-1) | 0xa3 | = Custom
> 0x43 | = Cloudy (0) | 0xf3 | = Color Temperature/Color Filter
> 0x44 | = Cloudy (+1) |  |

## Sony FaceInfo Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | FacesDetected | int16s | -1 = n/a
> 1 | Face1Position | int16u[4] | (re-ordered and scaled to return the top, left, height and width of detected face, with coordinates relative to the full-sized unrotated image and increasing Y downwards)
> 6 | Face2Position | int16u[4] |
> 11 | Face3Position | int16u[4] |
> 16 | Face4Position | int16u[4] |
> 21 | Face5Position | int16u[4] |
> 26 | Face6Position | int16u[4] |
> 31 | Face7Position | int16u[4] |
> 36 | Face8Position | int16u[4] |

## Sony FaceInfoA Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 3 | FacesDetected | no |
> 11 | PotentialFace1Position | int16u[4] |
> 21 | PotentialFace2Position | int16u[4] |
> 31 | PotentialFace3Position | int16u[4] |
> 41 | PotentialFace4Position | int16u[4] |
> 51 | PotentialFace5Position | int16u[4] |
> 61 | PotentialFace6Position | int16u[4] |
> 71 | PotentialFace7Position | int16u[4] |
> 81 | PotentialFace8Position | int16u[4] |
> 91 | Face1Position | int16u[4] |
> 101 | Face2Position | int16u[4] |
> 111 | Face3Position | int16u[4] |
> 121 | Face4Position | int16u[4] |

## Sony MoreInfo0201 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 283 | ImageCount | int32u | (not valid for the A450, A500 or A550)
> 293 | ShutterCount | int32u | (not valid for the A450, A500 or A550)
> 330 | ShutterCount | int32u | (A450, A500 and A550 only)

## Sony MoreInfo0401 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1102 | ShotNumberSincePowerUp | int32u | (Not valid for the NEX-3 or NEX-5)

## Sony CameraSettings Tags

Camera settings for the A200, A300, A350, A700, A850 and A900.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ExposureTime | int16u |
> 1 | FNumber | int16u |
> 2 | HighSpeedSync | int16u | 0 = Off 1 = On
> 3 | ExposureCompensationSet | int16u |
> 4 | DriveMode | int16u | [val & 0xff]
> 0x1 = Single Frame 0x2 = Continuous High 0x4 = Self-timer 10 sec 0x5 = Self-timer 2 sec, Mirror Lock-up 0x6 = Single-frame Bracketing 0x7 = Continuous Bracketing 0xa = Remote Commander 0xb = Mirror Lock-up 0x12 = Continuous Low 0x18 = White Balance Bracketing Low 0x19 = D-Range Optimizer Bracketing Low 0x28 = White Balance Bracketing High 0x29 = D-Range Optimizer Bracketing High
> 5 | WhiteBalanceSetting | int16u |
> 2 = Auto 4 = Daylight 5 = Fluorescent 6 = Tungsten 7 = Flash 16 = Cloudy 17 = Shade 18 = Color Temperature/Color Filter 32 = Custom 1 33 = Custom 2 34 = Custom 3
> 6 | WhiteBalanceFineTune | int16u |
> 7 | ColorTemperatureSet | int16u |
> 8 | ColorCompensationFilterSet | int16u | (negative is green, positive is magenta)
> 12 | ColorTemperatureCustom | int16u |
> 13 | ColorCompensationFilterCustom | int16u | (negative is green, positive is magenta)
> 15 | WhiteBalance | int16u |
> 2 = Auto 4 = Daylight 5 = Fluorescent 6 = Tungsten 7 = Flash |  | 12 = Color Temperature 13 = Color Filter 14 = Custom 16 = Cloudy 17 = Shade
> 16 | FocusModeSetting | int16u | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A 4 = DMF
> 17 | AFAreaMode | int16u | 0 = Wide 1 = Local 2 = Spot
> 18 | AFPointSetting | int16u |
> 1 = Center 2 = Top 3 = Upper-right 4 = Right 5 = Lower-right 6 = Bottom |  | 7 = Lower-left 8 = Left 9 = Upper-left 10 = Far Right 11 = Far Left
> 19 | FlashMode | int16u |
> 0 = Autoflash 2 = Rear Sync 3 = Wireless |  | 4 = Fill-flash 5 = Flash Off 6 = Slow Sync
> 20 | FlashExposureCompSet | int16u |
> 21 | MeteringMode | int16u | 1 = Multi-segment 2 = Center-weighted average 4 = Spot
> 22 | ISOSetting | int16u |
> 24 | DynamicRangeOptimizerMode | int16u | 0 = Off 1 = Standard 2 = Advanced Auto 3 = Advanced Level
> 25 | DynamicRangeOptimizerLevel | int16u |
> 26 | CreativeStyle | int16u |
> 1 = Standard 2 = Vivid 3 = Portrait 4 = Landscape 5 = Sunset 6 = Night View/Portrait 8 = B&W |  | 9 = Adobe RGB 11 = Neutral 12 = Clear 13 = Deep 14 = Light 15 = Autumn Leaves 16 = Sepia
> 27 | ColorSpace | int16u | 0 = sRGB 1 = Adobe RGB 5 = Adobe RGB (A700)
> 28 | Sharpness | int16u |
> 29 | Contrast | int16u |
> 30 | Saturation | int16u |
> 31 | ZoneMatchingValue | int16u |
> 34 | Brightness | int16u |
> 35 | FlashControl | int16u | 0 = ADI 1 = Pre-flash TTL 2 = Manual
> 40 | PrioritySetupShutterRelease | int16u | 0 = AF 1 = Release
> 41 | AFIlluminator | int16u | 0 = Auto 1 = Off
> 42 | AFWithShutter | int16u | 0 = On 1 = Off
> 43 | LongExposureNoiseReduction | int16u | 0 = Off 1 = On
> 44 | HighISONoiseReduction | int16u | 0 = Normal 1 = Low 2 = High 3 = Off
> 45 | ImageStyle | int16u |
> 1 = Standard 2 = Vivid 3 = Portrait 4 = Landscape 5 = Sunset 7 = Night View/Portrait 8 = B&W 9 = Adobe RGB |  | 11 = Neutral 129 = StyleBox1 130 = StyleBox2 131 = StyleBox3 132 = StyleBox4 133 = StyleBox5 134 = StyleBox6
> 46 | FocusModeSwitch | int16u | 0 = AF 1 = Manual
> 47 | ShutterSpeedSetting | int16u | (used in M, S and Program Shift S modes)
> 48 | ApertureSetting | int16u | (used in M, A and Program Shift A modes)
> 60 | ExposureProgram | int16u | --> Sony ExposureProgram Values
> 61 | ImageStabilizationSetting | int16u | 0 = Off 1 = On
> 62 | FlashAction | int16u | 0 = Did not fire 1 = Fired 2 = External Flash, Did not fire 3 = External Flash, Fired
> 63 | Rotation | int16u | 0 = Horizontal (normal) 1 = Rotate 90 CW 2 = Rotate 270 CW
> 64 | AELock | int16u | 1 = Off 2 = On
> 76 | FlashAction2 | int16u |
> 1 = Fired, Autoflash 2 = Fired, Fill-flash 3 = Fired, Rear Sync 4 = Fired, Wireless 5 = Did not fire 6 = Fired, Slow Sync 17 = Fired, Autoflash, Red-eye reduction 18 = Fired, Fill-flash, Red-eye reduction 34 = Fired, Fill-flash, HSS
> 77 | FocusMode | int16u | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A 4 = DMF
> 80 | BatteryState | int16u | 2 = Empty 3 = Very Low 4 = Low 5 = Sufficient 6 = Full
> 81 | BatteryLevel | int16u |
> 83 | FocusStatus | int16u | 0x0 = Not confirmed 0x4 = Not confirmed, Tracking Bit 0 = Confirmed Bit 1 = Failed Bit 2 = Tracking
> 84 | SonyImageSize | int16u | 1 = Large 2 = Medium 3 = Small
> 85 | AspectRatio | int16u | 1 = 3:2 2 = 16:9
> 86 | Quality | int16u |
> 0 = RAW 2 = CRAW 16 = Extra Fine 32 = Fine |  | 34 = RAW + JPEG 35 = CRAW + JPEG 48 = Standard
> 88 | ExposureLevelIncrements | int16u | 33 = 1/3 EV 50 = 1/2 EV
> 106 | RedEyeReduction | int16u | 0 = Off 1 = On
> 154 | FolderNumber | int16u | [val & 0x3ff]
> 155 | ImageNumber | int16u | [val & 0x3fff]

## Sony CameraSettings2 Tags

Camera settings for the A230, A290, A330, A380 and A390.

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ExposureTime | int16u |
> 1 | FNumber | int16u |
> 2 | HighSpeedSync | int16u | 0 = Off 1 = On
> 3 | ExposureCompensationSet | int16u |
> 4 | WhiteBalanceSetting | int16u |
> 2 = Auto 4 = Daylight 5 = Fluorescent 6 = Tungsten 7 = Flash 16 = Cloudy 17 = Shade 18 = Color Temperature/Color Filter 32 = Custom 1 33 = Custom 2 34 = Custom 3
> 5 | WhiteBalanceFineTune | int16u |
> 6 | ColorTemperatureSet | int16u |
> 7 | ColorCompensationFilterSet | int16u | (negative is green, positive is magenta)
> 8 | CustomWB_RGBLevels | int16u[3] |
> 11 | ColorTemperatureCustom | int16u |
> 12 | ColorCompensationFilterCustom | int16u | (negative is green, positive is magenta)
> 14 | WhiteBalance | int16u |
> 2 = Auto 4 = Daylight 5 = Fluorescent 6 = Tungsten 7 = Flash |  | 12 = Color Temperature 13 = Color Filter 14 = Custom 16 = Cloudy 17 = Shade
> 15 | FocusModeSetting | int16u | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A
> 16 | AFAreaMode | int16u | 0 = Wide 1 = Local 2 = Spot
> 17 | AFPointSetting | int16u |
> 1 = Center 2 = Top 3 = Upper-right 4 = Right 5 = Lower-right |  | 6 = Bottom 7 = Lower-left 8 = Left 9 = Upper-left
> 18 | FlashExposureCompSet | int16u |
> 19 | MeteringMode | int16u | 1 = Multi-segment 2 = Center-weighted average 4 = Spot
> 20 | ISOSetting | int16u |
> 22 | DynamicRangeOptimizerMode | int16u | 0 = Off 1 = Standard 2 = Advanced Auto 3 = Advanced Level
> 23 | DynamicRangeOptimizerLevel | int16u |
> 24 | CreativeStyle | int16u |
> 1 = Standard 2 = Vivid 3 = Portrait 4 = Landscape |  | 5 = Sunset 6 = Night View/Portrait 8 = B&W
> 25 | Sharpness | int16u |
> 26 | Contrast | int16u |
> 27 | Saturation | int16u |
> 31 | FlashControl | int16u | 0 = ADI 1 = Pre-flash TTL 2 = Manual
> 37 | LongExposureNoiseReduction | int16u | 0 = Off 1 = On
> 38 | HighISONoiseReduction | int16u | 0 = Off 1 = Low 2 = Normal 3 = High
> 39 | ImageStyle | int16u |
> 1 = Standard 2 = Vivid 3 = Portrait 4 = Landscape |  | 5 = Sunset 7 = Night View/Portrait 8 = B&W
> 40 | ShutterSpeedSetting | int16u | (used in M, S and Program Shift S modes)
> 41 | ApertureSetting | int16u | (used in M, A and Program Shift A modes)
> 60 | ExposureProgram | int16u | --> Sony ExposureProgram Values
> 61 | ImageStabilizationSetting | int16u | 0 = Off 1 = On
> 62 | FlashAction | int16u | 0 = Did not fire 1 = Fired 2 = External Flash, Did not fire 3 = External Flash, Fired
> 63 | Rotation | int16u | 0 = Horizontal (normal) 1 = Rotate 90 CW 2 = Rotate 270 CW
> 64 | AELock | int16u | 1 = Off 2 = On
> 76 | FlashAction2 | int16u |
> 1 = Fired, Autoflash 2 = Fired, Fill-flash 3 = Fired, Rear Sync 4 = Fired, Wireless 5 = Did not fire 6 = Fired, Slow Sync 17 = Fired, Autoflash, Red-eye reduction 18 = Fired, Fill-flash, Red-eye reduction 34 = Fired, Fill-flash, HSS
> 77 | FocusMode | int16u | 0 = Manual 1 = AF-S 2 = AF-C 3 = AF-A
> 83 | FocusStatus | int16u | 0x0 = Not confirmed 0x4 = Not confirmed, Tracking Bit 0 = Confirmed Bit 1 = Failed Bit 2 = Tracking
> 84 | SonyImageSize | int16u | 1 = Large 2 = Medium 3 = Small
> 85 | AspectRatio | int16u | 1 = 3:2 2 = 16:9
> 86 | Quality | int16u |
> 0 = RAW 2 = CRAW 16 = Extra Fine 32 = Fine |  | 34 = RAW + JPEG 35 = CRAW + JPEG 48 = Standard
> 88 | ExposureLevelIncrements | int16u | 33 = 1/3 EV 50 = 1/2 EV
> 126 | DriveMode | int16u | [val & 0xff]
> 1 = Single Frame 2 = Continuous High 4 = Self-timer 10 sec 5 = Self-timer 2 sec, Mirror Lock-up 7 = Continuous Bracketing 10 = Remote Commander 11 = Continuous Self-timer
> 127 | FlashMode | int16u |
> 0 = Autoflash 2 = Rear Sync 3 = Wireless |  | 4 = Fill-flash 5 = Flash Off 6 = Slow Sync
> 131 | ColorSpace | int16u | 5 = Adobe RGB 6 = sRGB

## Sony CameraSettings3 Tags

Camera settings for models such as the A33, A35, A55, A450, A500, A550, A560, A580, NEX-3, NEX-5, NEX-C3 and NEX-VG10E.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ShutterSpeedSetting | int8u | (used only in M and S exposure modes)
> 1 | ApertureSetting | int8u | (used only in M and A exposure modes)
> 2 | ISOSetting | int8u | 0 = Auto 254 = n/a
> 3 | ExposureCompensationSet | int8u |
> 4 | DriveModeSetting | int8u |
> 0x10 = Single Frame 0x21 = Continuous High 0x22 = Continuous Low 0x30 = Speed Priority Continuous 0x51 = Self-timer 10 sec 0x52 = Self-timer 2 sec, Mirror Lock-up 0x71 = Continuous Bracketing 0.3 EV 0x75 = Continuous Bracketing 0.7 EV 0x91 = White Balance Bracketing Low 0x92 = White Balance Bracketing High 0xc0 = Remote Commander
> 5 | ExposureProgram | int8u | --> Sony ExposureProgram2 Values
> 6 | FocusModeSetting | int8u | 17 = AF-S 18 = AF-C 19 = AF-A 32 = Manual 48 = DMF
> 7 | MeteringMode | int8u | 1 = Multi-segment 2 = Center-weighted average 3 = Spot
> 9 | SonyImageSize | int8u |
> 21 = Large (3:2) 22 = Medium (3:2) 23 = Small (3:2) |  | 25 = Large (16:9) 26 = Medium (16:9) 27 = Small (16:9)
> 10 | AspectRatio | int8u | 4 = 3:2 8 = 16:9
> 11 | Quality | int8u | 2 = RAW 4 = RAW + JPEG 6 = Fine 7 = Standard
> 12 | DynamicRangeOptimizerSetting | int8u | 1 = Off 16 = On (Auto) 17 = On (Manual)
> 13 | DynamicRangeOptimizerLevel | int8u |
> 14 | ColorSpace | int8u | 1 = sRGB 2 = Adobe RGB
> 15 | CreativeStyleSetting | int8u |
> 16 = Standard 32 = Vivid 64 = Portrait |  | 80 = Landscape 96 = B&W 160 = Sunset
> 16 | ContrastSetting | int8s |
> 17 | SaturationSetting | int8s |
> 18 | SharpnessSetting | int8s |
> 22 | WhiteBalanceSetting | int8u | --> Sony WhiteBalanceSetting Values
> 23 | ColorTemperatureSetting | int8u |
> 24 | ColorCompensationFilterSet | int8s | (negative is green, positive is magenta)
> 25 | CustomWB_RGBLevels | int16uRev[3] |
> 32 | FlashMode | int8u |
> 1 = Flash Off 16 = Autoflash 17 = Fill-flash |  | 18 = Slow Sync 19 = Rear Sync 20 = Wireless
> 33 | FlashControl | int8u | 1 = ADI Flash 2 = Pre-flash TTL
> 35 | FlashExposureCompSet | int8u |
> 36 | AFAreaMode | int8u | 1 = Wide 2 = Spot 3 = Local 4 = Flexible
> 37 | LongExposureNoiseReduction | int8u | 1 = Off 16 = On
> 38 | HighISONoiseReduction | int8u | 16 = Low 17 = High 19 = Auto
> 39 | SmileShutterMode | int8u | 17 = Slight Smile 18 = Normal Smile 19 = Big Smile
> 40 | RedEyeReduction | int8u | 1 = Off 16 = On
> 45 | HDRSetting | int8u | 1 = Off 16 = On (Auto) 17 = On (Manual)
> 46 | HDRLevel | int8u |
> 33 = 1 EV 34 = 1.5 EV 35 = 2 EV |  | 36 = 2.5 EV 37 = 3 EV 38 = 3.5 EV |  | 39 = 4 EV 40 = 5 EV 41 = 6 EV
> 47 | ViewingMode | int8u | 16 = ViewFinder 33 = Focus Check Live View 34 = Quick AF Live View
> 48 | FaceDetection | int8u | 1 = Off 16 = On
> 49 | SmileShutter | int8u | 1 = Off 16 = On
> 50 | SweepPanoramaSize | int8u | 1 = Standard 2 = Wide
> 51 | SweepPanoramaDirection | int8u | 1 = Right 2 = Left 3 = Up 4 = Down
> 52 | DriveMode | int8u |
> 0x10 = Single Frame 0x21 = Continuous High 0x22 = Continuous Low 0x30 = Speed Priority Continuous 0x51 = Self-timer 10 sec 0x52 = Self-timer 2 sec, Mirror Lock-up 0x71 = Continuous Bracketing 0.3 EV 0x75 = Continuous Bracketing 0.7 EV 0x91 = White Balance Bracketing Low 0x92 = White Balance Bracketing High 0xc0 = Remote Commander 0xd1 = Continuous - HDR 0xd2 = Continuous - Multi Frame NR 0xd3 = Continuous - Handheld Night Shot 0xd4 = Continuous - Anti Motion Blur 0xd5 = Continuous - Sweep Panorama 0xd6 = Continuous - 3D Sweep Panorama
> 53 | MultiFrameNoiseReduction | int8u | 0 = n/a 1 = Off 16 = On 255 = None
> 54 | LiveViewAFSetting | int8u | 0 = n/a 1 = Phase-detect AF 2 = Contrast AF
> 56 | PanoramaSize3D | int8u | 0 = n/a 1 = Standard 2 = Wide 3 = 16:9
> 131 | AFButtonPressed | int8u | 1 = No 16 = Yes
> 132 | LiveViewMetering | int8u | 0 = n/a 16 = 40 Segment 32 = 1200-zone Evaluative
> 133 | ViewingMode2 | int8u | 0 = n/a 16 = Viewfinder 33 = Focus Check Live View 34 = Quick AF Live View
> 134 | AELock | int8u | 1 = On 2 = Off
> 135 | FlashStatusBuilt-in | int8u | 1 = Off 2 = On
> 136 | FlashStatusExternal | int8u | 1 = None 2 = Off 3 = On
> 139 | LiveViewFocusMode | int8u | 0 = n/a 1 = AF 16 = Manual
> 153 | LensMount | int8u | 1 = Unknown 16 = A-mount 17 = E-mount
> 268 | SequenceNumber | int8u | 0 = Single 255 = n/a
> 276 | FolderNumber | int32u | [val >> 14 & 0x3ff]
> 276.1 | ImageNumber | int32u | [val & 0x3fff]
> 512 | ShotNumberSincePowerUp2 | int32u | (same as ShotNumberSincePowerUp for single-shot images, but includes all shots of the current image in multi-shot modes like HDR, panorama, and multi-frame noise reduction)
> 643 | AFButtonPressed | int8u | 1 = No 16 = Yes
> 644 | LiveViewMetering | int8u | 0 = n/a 16 = 40 Segment 32 = 1200-zone Evaluative
> 645 | ViewingMode2 | int8u | 0 = n/a 16 = Viewfinder 33 = Focus Check Live View 34 = Quick AF Live View
> 646 | AELock | int8u | 1 = On 2 = Off
> 647 | FlashStatusBuilt-in | int8u | (A450, A500 and A550) 1 = Off 2 = On
> 648 | FlashStatusExternal | int8u | (A450, A500 and A550) 1 = None 2 = Off 3 = On
> 651 | LiveViewFocusMode | int8u | 0 = n/a 1 = AF 16 = Manual
> 780 | SequenceNumber | int8u | (A450, A500 and A550) 0 = Single 255 = n/a
> 788 | ImageNumber | int16u | (A450, A500 and A550) [val & 0x3fff]
> 790 | FolderNumber | int16u | (A450, A500 and A550) [val & 0x3ff]
> 1008 | LensE-mountVersion | int16u |
> 1011 | LensFirmwareVersion | int16u~ |
> 1015 | LensType2 | int16u | --> Sony LensType2 Values
> 1024 | ImageNumber | int16u | (A450, A500 and A550) [val & 0x3fff]
> 1026 | FolderNumber | int16u | (A450, A500 and A550) [val & 0x3ff]

## Sony LensType2 Values

Lens type numbers for Sony E-mount lenses used by NEX/ILCE models.

> Value | LensType2
> --- | ---
> 0 | = Unknown E-mount lens or other lens
> 0.1 | = Sigma 19mm F2.8 [EX] DN
> 0.2 | = Sigma 30mm F2.8 [EX] DN
> 0.3 | = Sigma 60mm F2.8 DN
> 0.4 | = Sony E 18-200mm F3.5-6.3 OSS LE
> 0.5 | = Tamron 18-200mm F3.5-6.3 Di III VC
> 0.6 | = Tokina FiRIN 20mm F2 FE AF
> 0.7 | = Tokina FiRIN 20mm F2 FE MF
> 0.8 | = Zeiss Touit 12mm F2.8
> 0.9 | = Zeiss Touit 32mm F1.8
> 0.10 | = Zeiss Touit 50mm F2.8 Macro
> 0.11 | = Zeiss Loxia 50mm F2
> 0.12 | = Zeiss Loxia 35mm F2
> 1 | = Sony LA-EA1 or Sigma MC-11 Adapter
> 2 | = Sony LA-EA2 Adapter
> 3 | = Sony LA-EA3 Adapter
> 6 | = Sony LA-EA4 Adapter
> 7 | = Sony LA-EA5 Adapter
> 44 | = Metabones Canon EF Smart Adapter
> 78 | = Metabones Canon EF Smart Adapter Mark III or Other Adapter
> 184 | = Metabones Canon EF Speed Booster Ultra
> 234 | = Metabones Canon EF Smart Adapter Mark IV
> 239 | = Metabones Canon EF Speed Booster
> 24593 | = LA-EA4r MonsterAdapter
> 32784 | = Sony E 16mm F2.8
> 32785 | = Sony E 18-55mm F3.5-5.6 OSS
> 32786 | = Sony E 55-210mm F4.5-6.3 OSS
> 32787 | = Sony E 18-200mm F3.5-6.3 OSS
> 32788 | = Sony E 30mm F3.5 Macro
> 32789 | = Sony E 24mm F1.8 ZA or Samyang AF 50mm F1.4
> 32789.1 | = Samyang AF 50mm F1.4
> 32790 | = Sony E 50mm F1.8 OSS or Samyang AF 14mm F2.8
> 32790.1 | = Samyang AF 14mm F2.8
> 32791 | = Sony E 16-70mm F4 ZA OSS
> 32792 | = Sony E 10-18mm F4 OSS
> 32793 | = Sony E PZ 16-50mm F3.5-5.6 OSS
> 32794 | = Sony FE 35mm F2.8 ZA or Samyang Lens
> 32794.1 | = Samyang AF 24mm F2.8
> 32794.2 | = Samyang AF 35mm F2.8
> 32795 | = Sony FE 24-70mm F4 ZA OSS
> 32796 | = Sony FE 85mm F1.8 or Viltrox PFU RBMH 85mm F1.8
> 32796.1 | = Viltrox PFU RBMH 85mm F1.8
> 32797 | = Sony E 18-200mm F3.5-6.3 OSS LE
> 32798 | = Sony E 20mm F2.8
> 32799 | = Sony E 35mm F1.8 OSS
> 32800 | = Sony E PZ 18-105mm F4 G OSS
> 32801 | = Sony FE 12-24mm F4 G
> 32802 | = Sony FE 90mm F2.8 Macro G OSS
> 32803 | = Sony E 18-50mm F4-5.6
> 32804 | = Sony FE 24mm F1.4 GM
> 32805 | = Sony FE 24-105mm F4 G OSS
> 32807 | = Sony E PZ 18-200mm F3.5-6.3 OSS
> 32808 | = Sony FE 55mm F1.8 ZA
> 32810 | = Sony FE 70-200mm F4 G OSS
> 32811 | = Sony FE 16-35mm F4 ZA OSS
> 32812 | = Sony FE 50mm F2.8 Macro
> 32813 | = Sony FE 28-70mm F3.5-5.6 OSS
> 32814 | = Sony FE 35mm F1.4 ZA
> 32815 | = Sony FE 24-240mm F3.5-6.3 OSS
> 32816 | = Sony FE 28mm F2
> 32817 | = Sony FE PZ 28-135mm F4 G OSS
> 32819 | = Sony FE 100mm F2.8 STF GM OSS
> 32820 | = Sony E PZ 18-110mm F4 G OSS
> 32821 | = Sony FE 24-70mm F2.8 GM
> 32822 | = Sony FE 50mm F1.4 ZA
> 32823 | = Sony FE 85mm F1.4 GM or Samyang AF 85mm F1.4
> 32823.1 | = Samyang AF 85mm F1.4
> 32824 | = Sony FE 50mm F1.8
> 32826 | = Sony FE 21mm F2.8 (SEL28F20 + SEL075UWC)
> 32827 | = Sony FE 16mm F3.5 Fisheye (SEL28F20 + SEL057FEC)
> 32828 | = Sony FE 70-300mm F4.5-5.6 G OSS
> 32829 | = Sony FE 100-400mm F4.5-5.6 GM OSS
> 32830 | = Sony FE 70-200mm F2.8 GM OSS
> 32831 | = Sony FE 16-35mm F2.8 GM
> 32848 | = Sony FE 400mm F2.8 GM OSS
> 32849 | = Sony E 18-135mm F3.5-5.6 OSS
> 32850 | = Sony FE 135mm F1.8 GM
> 32851 | = Sony FE 200-600mm F5.6-6.3 G OSS
> 32852 | = Sony FE 600mm F4 GM OSS
> 32853 | = Sony E 16-55mm F2.8 G
> 32854 | = Sony E 70-350mm F4.5-6.3 G OSS
> 32855 | = Sony FE C 16-35mm T3.1 G
> 32858 | = Sony FE 35mm F1.8
> 32859 | = Sony FE 20mm F1.8 G
> 32860 | = Sony FE 12-24mm F2.8 GM
> 32862 | = Sony FE 50mm F1.2 GM
> 32863 | = Sony FE 14mm F1.8 GM
> 32864 | = Sony FE 28-60mm F4-5.6
> 32865 | = Sony FE 35mm F1.4 GM
> 32866 | = Sony FE 24mm F2.8 G
> 32867 | = Sony FE 40mm F2.5 G
> 32868 | = Sony FE 50mm F2.5 G
> 32871 | = Sony FE PZ 16-35mm F4 G
> 32873 | = Sony E PZ 10-20mm F4 G
> 32874 | = Sony FE 70-200mm F2.8 GM OSS II
> 32875 | = Sony FE 24-70mm F2.8 GM II
> 32876 | = Sony E 11mm F1.8
> 32877 | = Sony E 15mm F1.4 G
> 33072 | = Sony FE 70-200mm F2.8 GM OSS + 1.4X Teleconverter
> 33073 | = Sony FE 70-200mm F2.8 GM OSS + 2X Teleconverter
> 33076 | = Sony FE 100mm F2.8 STF GM OSS (macro mode)
> 33077 | = Sony FE 100-400mm F4.5-5.6 GM OSS + 1.4X Teleconverter
> 33078 | = Sony FE 100-400mm F4.5-5.6 GM OSS + 2X Teleconverter
> 33079 | = Sony FE 400mm F2.8 GM OSS + 1.4X Teleconverter
> 33080 | = Sony FE 400mm F2.8 GM OSS + 2X Teleconverter
> 33081 | = Sony FE 200-600mm F5.6-6.3 G OSS + 1.4X Teleconverter
> 33082 | = Sony FE 200-600mm F5.6-6.3 G OSS + 2X Teleconverter
> 33083 | = Sony FE 600mm F4 GM OSS + 1.4X Teleconverter
> 33084 | = Sony FE 600mm F4 GM OSS + 2X Teleconverter
> 49201 | = Zeiss Touit 12mm F2.8
> 49202 | = Zeiss Touit 32mm F1.8
> 49203 | = Zeiss Touit 50mm F2.8 Macro
> 49216 | = Zeiss Batis 25mm F2
> 49217 | = Zeiss Batis 85mm F1.8
> 49218 | = Zeiss Batis 18mm F2.8
> 49219 | = Zeiss Batis 135mm F2.8
> 49220 | = Zeiss Batis 40mm F2 CF
> 49232 | = Zeiss Loxia 50mm F2
> 49233 | = Zeiss Loxia 35mm F2
> 49234 | = Zeiss Loxia 21mm F2.8
> 49235 | = Zeiss Loxia 85mm F2.4
> 49236 | = Zeiss Loxia 25mm F2.4
> 49457 | = Tamron 28-75mm F2.8 Di III RXD
> 49458 | = Tamron 17-28mm F2.8 Di III RXD
> 49459 | = Tamron 35mm F2.8 Di III OSD M1:2
> 49460 | = Tamron 24mm F2.8 Di III OSD M1:2
> 49461 | = Tamron 20mm F2.8 Di III OSD M1:2
> 49462 | = Tamron 70-180mm F2.8 Di III VXD
> 49463 | = Tamron 28-200mm F2.8-5.6 Di III RXD
> 49464 | = Tamron 70-300mm F4.5-6.3 Di III RXD
> 49465 | = Tamron 17-70mm F2.8 Di III-A VC RXD
> 49466 | = Tamron 150-500mm F5-6.7 Di III VC VXD
> 49467 | = Tamron 11-20mm F2.8 Di III-A RXD
> 49468 | = Tamron 18-300mm F3.5-6.3 Di III-A VC VXD
> 49469 | = Tamron 35-150mm F2-F2.8 Di III VXD
> 49470 | = Tamron 28-75mm F2.8 Di III VXD G2
> 49471 | = Tamron 50-400mm F4.5-6.3 Di III VC VXD
> 49473 | = Tokina atx-m 85mm F1.8 FE or Viltrox lens
> 49473.1 | = Viltrox 23mm F1.4 E
> 49473.2 | = Viltrox 56mm F1.4 E
> 49712 | = Tokina FiRIN 20mm F2 FE AF
> 49713 | = Tokina FiRIN 100mm F2.8 FE MACRO
> 49714 | = Tokina atx-m 11-18mm F2.8 E
> 50480 | = Sigma 30mm F1.4 DC DN | C
> 50481 | = Sigma 50mm F1.4 DG HSM | A
> 50482 | = Sigma 18-300mm F3.5-6.3 DC MACRO OS HSM | C + MC-11
> 50483 | = Sigma 18-35mm F1.8 DC HSM | A + MC-11
> 50484 | = Sigma 24-35mm F2 DG HSM | A + MC-11
> 50485 | = Sigma 24mm F1.4 DG HSM | A + MC-11
> 50486 | = Sigma 150-600mm F5-6.3 DG OS HSM | C + MC-11
> 50487 | = Sigma 20mm F1.4 DG HSM | A + MC-11
> 50488 | = Sigma 35mm F1.4 DG HSM | A
> 50489 | = Sigma 150-600mm F5-6.3 DG OS HSM | S + MC-11
> 50490 | = Sigma 120-300mm F2.8 DG OS HSM | S + MC-11
> 50492 | = Sigma 24-105mm F4 DG OS HSM | A + MC-11
> 50493 | = Sigma 17-70mm F2.8-4 DC MACRO OS HSM | C + MC-11
> 50495 | = Sigma 50-100mm F1.8 DC HSM | A + MC-11
> 50499 | = Sigma 85mm F1.4 DG HSM | A
> 50501 | = Sigma 100-400mm F5-6.3 DG OS HSM | C + MC-11
> 50503 | = Sigma 16mm F1.4 DC DN | C
> 50507 | = Sigma 105mm F1.4 DG HSM | A
> 50508 | = Sigma 56mm F1.4 DC DN | C
> 50512 | = Sigma 70-200mm F2.8 DG OS HSM | S + MC-11
> 50513 | = Sigma 70mm F2.8 DG MACRO | A
> 50514 | = Sigma 45mm F2.8 DG DN | C
> 50515 | = Sigma 35mm F1.2 DG DN | A
> 50516 | = Sigma 14-24mm F2.8 DG DN | A
> 50517 | = Sigma 24-70mm F2.8 DG DN | A
> 50518 | = Sigma 100-400mm F5-6.3 DG DN OS | C
> 50521 | = Sigma 85mm F1.4 DG DN | A
> 50522 | = Sigma 105mm F2.8 DG DN MACRO | A
> 50523 | = Sigma 65mm F2 DG DN | C
> 50524 | = Sigma 35mm F2 DG DN | C
> 50525 | = Sigma 24mm F3.5 DG DN | C
> 50526 | = Sigma 28-70mm F2.8 DG DN | C
> 50527 | = Sigma 150-600mm F5-6.3 DG DN OS | S
> 50528 | = Sigma 35mm F1.4 DG DN | A
> 50529 | = Sigma 90mm F2.8 DG DN | C
> 50530 | = Sigma 24mm F2 DG DN | C
> 50531 | = Sigma 18-50mm F2.8 DC DN | C
> 50532 | = Sigma 20mm F2 DG DN | C
> 50533 | = Sigma 16-28mm F2.8 DG DN | C
> 50992 | = Voigtlander SUPER WIDE-HELIAR 15mm F4.5 III
> 50993 | = Voigtlander HELIAR-HYPER WIDE 10mm F5.6
> 50994 | = Voigtlander ULTRA WIDE-HELIAR 12mm F5.6 III
> 50995 | = Voigtlander MACRO APO-LANTHAR 65mm F2 Aspherical
> 50996 | = Voigtlander NOKTON 40mm F1.2 Aspherical
> 50997 | = Voigtlander NOKTON classic 35mm F1.4
> 50998 | = Voigtlander MACRO APO-LANTHAR 110mm F2.5
> 50999 | = Voigtlander COLOR-SKOPAR 21mm F3.5 Aspherical
> 51000 | = Voigtlander NOKTON 50mm F1.2 Aspherical
> 51001 | = Voigtlander NOKTON 21mm F1.4 Aspherical
> 51002 | = Voigtlander APO-LANTHAR 50mm F2 Aspherical
> 51003 | = Voigtlander NOKTON 35mm F1.2 Aspherical SE
> 51006 | = Voigtlander APO-LANTHAR 35mm F2 Aspherical
> 51504 | = Samyang AF 50mm F1.4
> 51505 | = Samyang AF 14mm F2.8 or Samyang AF 35mm F2.8
> 51505.1 | = Samyang AF 35mm F2.8
> 51507 | = Samyang AF 35mm F1.4
> 51508 | = Samyang AF 45mm F1.8
> 51510 | = Samyang AF 18mm F2.8 or Samyang AF 35mm F1.8
> 51510.1 | = Samyang AF 35mm F1.8
> 51512 | = Samyang AF 75mm F1.8
> 51513 | = Samyang AF 35mm F1.8
> 51514 | = Samyang AF 24mm F1.8
> 51515 | = Samyang AF 12mm F2.0
> 51516 | = Samyang AF 24-70mm F2.8
> 51517 | = Samyang AF 50mm F1.4 II
> 51518 | = Samyang AF 135mm F1.8

## Sony CameraSettingsUnknown Tags

> Index2 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> [no tags known]

## Sony ExtraInfo Tags

Extra hardware information for the A850 and A900.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | BatteryTemperature | int8u |
> 2 | BatteryUnknown? | no |
> 8 | BatteryVoltage? | no |
> 10 | ImageStabilization2? | int8u | 191 = On (191) 207 = On (207) 210 = On (210) 213 = On 246 = Off
> 12 | BatteryLevel | int8u |
> 26 | ExtraInfoVersion | int8u[4] |

## Sony ExtraInfo2 Tags

Extra hardware information for the A230/290/330/380/390.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | BatteryLevel | int8u |
> 18 | ImageStabilization | int8u | 0 = Off 64 = On

## Sony ExtraInfo3 Tags

Extra hardware information for the A33, A35, A55, A450, A500, A550, A560, A580 and NEX-3/5/C3/VG10.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | BatteryUnknown? | int16u |
> 2 | BatteryTemperature | int8u |
> 4 | BatteryLevel | int8u |
> 6 | BatteryVoltage1 | int16u |
> 8 | BatteryVoltage2 | int16u |
> 17 | ImageStabilization | int8u | 0 = Off 64 = On
> 20 | BatteryState ExposureProgram ModeDialPosition | int8u int8u int8u | (BatteryState for SLT models) 1 = Empty 2 = Low 3 = Half full 4 = Almost full 5 = Full (ExposureProgram for the A450, A500 and A550)
> 241 = Landscape 243 = Aperture-priority AE 245 = Portrait 246 = Auto 247 = Program AE 249 = Macro 252 = Sunset 253 = Sports 255 = Manual
> (ModeDialPosition for other DSLR models)
> 248 = No Flash 249 = Aperture-priority AE 250 = SCN 251 = Shutter speed priority AE 252 = Auto 253 = Program AE 254 = Panorama 255 = Manual
> 22 | MemoryCardConfiguration CameraOrientation | int8u int8u | 244 = MemoryStick in use, SD card present 245 = MemoryStick in use, SD slot empty 252 = SD card in use, MemoryStick present 254 = SD card in use, MemoryStick slot empty [val >> 6 & 0x3] 0 = Horizontal (normal) 1 = Rotate 90 CW 2 = Rotate 270 CW 3 = Rotate 180
> 24 | CameraOrientation | int8u | [val >> 4 & 0x3] 0 = Horizontal (normal) 1 = Rotate 90 CW 2 = Rotate 270 CW 3 = Rotate 180

## Sony Panorama Tags

Tags found in panorama images from various Sony DSC, NEX, SLT and DSLR cameras. The width/height values of these tags are not affected by camera rotation -- the width is always the longer dimension.

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | PanoramaFullWidth | int32u |
> 2 | PanoramaFullHeight | int32u |
> 3 | PanoramaDirection | int32u | 0 = Left or Up 1 = Right or Down
> 4 | PanoramaCropLeft | int32u |
> 5 | PanoramaCropTop | int32u |
> 6 | PanoramaCropRight | int32u |
> 7 | PanoramaCropBottom | int32u |
> 8 | PanoramaFrameWidth | int32u |
> 9 | PanoramaFrameHeight | int32u |
> 10 | PanoramaSourceWidth | int32u |
> 11 | PanoramaSourceHeight | int32u |

## Sony Tag2010a Tags

Valid for NEX-5N.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1200 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4392 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4396 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4404 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4408 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4414 | StopsAboveBaseISO | int16u |
> 4416 | BrightnessValue | int16u |
> 4420 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4424 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4428 | ExposureCompensation | int16s |
> 4446 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4447 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4451 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4464 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 4468 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4469 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4476 | WB_RGBLevels | int16u[3] |

## Sony ReleaseMode2 Values

> Value | ReleaseMode2 | Value | ReleaseMode2
> --- | --- | --- | ---
> 0 | = Normal | 16 | = Continuous - 3D Image
> 1 | = Continuous | 17 | = Continuous - Burst 2
> 2 | = Continuous - Exposure Bracketing | 18 | = Normal - iAuto+
> 3 | = DRO or White Balance Bracketing | 19 | = Continuous - Speed/Advance Priority
> 5 | = Continuous - Burst | 20 | = Continuous - Multi Frame NR
> 6 | = Single Frame - Capture During Movie | 23 | = Single-frame - Exposure Bracketing
> 7 | = Continuous - Sweep Panorama | 26 | = Continuous Low
> 8 | = Continuous - Anti-Motion Blur, Hand-held Twilight | 27 | = Continuous - High Sensitivity
> 9 | = Continuous - HDR | 28 | = Smile Shutter
> 10 | = Continuous - Background defocus | 29 | = Continuous - Tele-zoom Advance Priority
> 13 | = Continuous - 3D Sweep Panorama | 146 | = Single Frame - Movie Capture
> 15 | = Continuous - High Resolution Sweep Panorama |  |

## Sony PictureEffect2 Values

> Value | PictureEffect2 | Value | PictureEffect2 | Value | PictureEffect2
> --- | --- | --- | --- | --- | ---
> 0 | = Off | 5 | = Soft High Key | 10 | = Rich-tone Monochrome
> 1 | = Toy Camera | 6 | = Partial Color | 11 | = Miniature
> 2 | = Pop Color | 7 | = High Contrast Monochrome | 12 | = Water Color
> 3 | = Posterization | 8 | = Soft Focus | 13 | = Illustration
> 4 | = Retro Photo | 9 | = HDR Painting |  |

## Sony ExposureProgram3 Values

> Value | ExposureProgram3 | Value | ExposureProgram3 | Value | ExposureProgram3
> --- | --- | --- | --- | --- | ---
> 0 | = Program AE | 11 | = Twilight Portrait | 27 | = Gourmet
> 1 | = Aperture-priority AE | 12 | = Sunset | 28 | = Pet
> 2 | = Shutter speed priority AE | 14 | = Action (High speed) | 29 | = Macro
> 3 | = Manual | 16 | = Sports | 30 | = Backlight Correction HDR
> 4 | = Auto | 17 | = Handheld Night Shot | 33 | = Sweep Panorama
> 5 | = iAuto | 18 | = Anti Motion Blur | 36 | = Background Defocus
> 6 | = Superior Auto | 19 | = High Sensitivity | 37 | = Soft Skin
> 7 | = iAuto+ | 21 | = Beach | 42 | = 3D Image
> 8 | = Portrait | 22 | = Snow | 43 | = Cont. Priority AE
> 9 | = Landscape | 23 | = Fireworks | 45 | = Document
> 10 | = Twilight | 26 | = Underwater | 46 | = Party

## Sony MeterInfo Tags

Information possibly related to metering. Extracted only if the Unknown option is used.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MeterInfo1Row1 | int32u[27] |
> 108 | MeterInfo1Row2 | int32u[27] |
> 216 | MeterInfo1Row3 | int32u[27] |
> 324 | MeterInfo1Row4 | int32u[27] |
> 432 | MeterInfo1Row5 | int32u[27] |
> 540 | MeterInfo1Row6 | int32u[27] |
> 648 | MeterInfo1Row7 | int32u[27] |
> 756 | MeterInfo2Row1 | int32u[33] |
> 888 | MeterInfo2Row2 | int32u[33] |
> 1020 | MeterInfo2Row3 | int32u[33] |
> 1152 | MeterInfo2Row4 | int32u[33] |
> 1284 | MeterInfo2Row5 | int32u[33] |
> 1416 | MeterInfo2Row6 | int32u[33] |
> 1548 | MeterInfo2Row7 | int32u[33] |
> 1680 | MeterInfo2Row8 | int32u[33] |
> 1812 | MeterInfo2Row9 | int32u[33] |

## Sony Tag2010b Tags

Valid for SLT-A65/A77, NEX-7/VG20E.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 4 | SequenceFileNumber | int32u | (file number in burst sequence)
> 8 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 438 | SonyDateTime | undef[7] |
> 804 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 1204 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4392 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4396 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4404 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4408 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4414 | StopsAboveBaseISO | int16u |
> 4416 | BrightnessValue | int16u |
> 4420 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4424 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4428 | ExposureCompensation | int16s |
> 4450 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4451 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4455 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4468 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 4472 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4473 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4480 | WB_RGBLevels | int16u[3] |
> 4632 | SonyISO | int16u |
> 6691 | DistortionCorrParams | int16s[16] |

## Sony Tag2010c Tags

Valid for SLT-A37/A57 and NEX-F3.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 4 | SequenceFileNumber | int32u | (file number in burst sequence)
> 8 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 512 | DigitalZoomRatio | int8u |
> 528 | SonyDateTime | undef[7] |
> 768 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 1168 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4356 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4360 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4368 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4372 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4378 | StopsAboveBaseISO | int16u |
> 4380 | BrightnessValue | int16u |
> 4384 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4388 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4392 | ExposureCompensation | int16s |
> 4414 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4415 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4419 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4432 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 4436 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4437 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4444 | WB_RGBLevels | int16u[3] |
> 4596 | SonyISO | int16u |

## Sony Tag2010d Tags

Valid for DSC-HX10V/HX20V/HX200V/TX66/TX200V/TX300V/WX50/WX100/WX150, but not valid for panorama images.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 4 | SequenceFileNumber | int32u | (file number in burst sequence)
> 8 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 510 | SonyDateTime | undef[7] |
> 892 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 1292 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4480 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4484 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4492 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4496 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4502 | StopsAboveBaseISO | int16u |
> 4504 | BrightnessValue | int16u |
> 4508 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4512 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4538 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4539 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4543 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4560 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4561 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4568 | WB_RGBLevels | int16u[3] |
> 4720 | SonyISO | int16u |

## Sony Tag2010e Tags

Valid for SLT-A58/A99, ILCE-3000/3500, NEX-3N/5R/5T/6/VG30E/VG900, DSC-RX100, DSC-RX1/RX1R. Also valid for DSC-HX300/HX50V/TX30/WX60/WX200/ WX300, but not for panorama images.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 4 | SequenceFileNumber | int32u | (file number in burst sequence)
> 8 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 540 | DigitalZoomRatio | int8u |
> 556 | SonyDateTime | undef[7] |
> 808 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 1208 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4444 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4448 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4456 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4460 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4466 | StopsAboveBaseISO | int16u |
> 4468 | BrightnessValue | int16u |
> 4472 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4476 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4480 | ExposureCompensation | int16s |
> 4502 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4503 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4507 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4520 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 4524 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4525 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4532 | WB_RGBLevels | int16u[3] |
> 4692 | SonyISO | int16u |
> 4696 | SonyISO | int16u |
> 4728 | FocalLength | int16u |
> 4730 | MinFocalLength | int16u |
> 4732 | MaxFocalLength | int16u |
> 4736 | SonyISO | int16u |
> 6256 | DistortionCorrParams | int16s[16] |
> 6289 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 6290 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 6291 | LensType2 | int16u | --> Sony LensType2 Values
> 6294 | LensType | int16u | --> Sony LensType Values
> 6296 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 6297 | DistortionCorrParamsNumber | int8u | 11 = 11 (APS-C) 16 = 16 (Full-frame)

## Sony Tag2010f Tags

Valid for DSC-RX100M2, DSC-QX10/QX100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 80 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 480 | MeterInfo? | - | --> Sony MeterInfo Tags
> 4116 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 4120 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 4128 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 4132 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 4138 | StopsAboveBaseISO | int16u |
> 4140 | BrightnessValue | int16u |
> 4144 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 4148 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 4152 | ExposureCompensation | int16s |
> 4174 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4175 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 4179 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 4192 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 4196 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 4197 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 4204 | WB_RGBLevels | int16u[3] |
> 4404 | FocalLength | int16u |
> 4406 | MinFocalLength | int16u |
> 4408 | MaxFocalLength | int16u |
> 4412 | SonyISO | int16u |

## Sony Tag2010g Tags

Valid for DSC-HX60V/HX350/HX400V/QX30/RX10/RX100M3/WX220/WX350, ILCE-7/7R/7S/7M2/5000/5100/6000/QX1, ILCA-68/77M2.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 80 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 524 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 528 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 536 | SelfTimer | int8u | 0 = Off 1 = Self-timer 10 s 2 = Self-timer 2 s
> 540 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 546 | StopsAboveBaseISO | int16u |
> 548 | BrightnessValue | int16u |
> 552 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 556 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 560 | ExposureCompensation | int16s |
> 582 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 583 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 587 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 600 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 604 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 605 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 612 | WB_RGBLevels | int16u[3] |
> 812 | FocalLength | int16u |
> 814 | MinFocalLength | int16u |
> 816 | MaxFocalLength | int16u |
> 836 | SonyISO | int16u |
> 904 | MeterInfo? | - | --> Sony MeterInfo Tags
> 6300 | DistortionCorrParams | int16s[16] |
> 6333 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 6334 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 6335 | LensType2 | int16u | --> Sony LensType2 Values
> 6338 | LensType | int16u | --> Sony LensType Values
> 6340 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 6341 | DistortionCorrParamsNumber | int8u | 11 = 11 (APS-C) 16 = 16 (Full-frame)

## Sony Tag2010h Tags

Valid for DSC-HX80/HX90V/RX0/RX1RM2/RX10M2/RX10M3/RX100M4/RX100M5/WX500, ILCE-6300/6500/7RM2/7SM2, ILCA-99M2.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 80 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 524 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 528 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 536 | SelfTimer | int8u | 0 = Off 1 = Self-timer 5 or 10 s 2 = Self-timer 2 s
> 540 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 546 | StopsAboveBaseISO | int16u |
> 548 | BrightnessValue | int16u |
> 552 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 556 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 560 | ExposureCompensation | int16s |
> 582 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 583 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 587 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 600 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 604 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 605 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 612 | WB_RGBLevels | int16u[3] |
> 812 | FocalLength | int16u |
> 814 | MinFocalLength | int16u |
> 816 | MaxFocalLength | int16u |
> 838 | SonyISO | int16u |
> 904 | MeterInfo? | - | --> Sony MeterInfo Tags
> 920 | MeterInfo? | - | --> Sony MeterInfo Tags
> 6348 | DistortionCorrParams | int16s[16] |
> 6381 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 6382 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 6383 | LensType2 | int16u | --> Sony LensType2 Values
> 6386 | LensType | int16u | --> Sony LensType Values
> 6388 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 6389 | DistortionCorrParamsNumber | int8u | 11 = 11 (APS-C) 16 = 16 (Full-frame)

## Sony Tag2010i Tags

Valid for ILCE-6100/6400/6600/7C/7M3/7RM3/7RM4/9/9M2, DSC-RX0M2/RX10M4/RX100M6/ RX100M5A/RX100M7/HX99.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | ReleaseMode2 | int32u | --> Sony ReleaseMode2 Values
> 78 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 516 | ReleaseMode3 | int8u |
> 0 = Normal 1 = Continuous 2 = Bracketing 4 = Continuous - Burst 5 = Continuous - Speed/Advance Priority 6 = Normal - Self-timer 9 = Single Burst Shooting
> 520 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 528 | SelfTimer | int8u | 0 = Off 1 = Self-timer 5 or 10 s 2 = Self-timer 2 s
> 529 | FlashMode | int8u |
> 0 = Autoflash 1 = Fill-flash 2 = Flash Off |  | 3 = Slow Sync 4 = Rear Sync 6 = Wireless
> 535 | StopsAboveBaseISO | int16u |
> 537 | BrightnessValue | int16u |
> 539 | DynamicRangeOptimizer | int8u |
> 0 = Off 1 = Auto 3 = Lv1 4 = Lv2 |  | 5 = Lv3 6 = Lv4 7 = Lv5 8 = n/a
> 543 | HDRSetting | int8u |
> 0 = Off 1 = HDR Auto 3 = HDR 1 EV 5 = HDR 2 EV |  | 7 = HDR 3 EV 9 = HDR 4 EV 11 = HDR 5 EV 13 = HDR 6 EV
> 547 | ExposureCompensation | int16s |
> 567 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 568 | PictureProfile | int8u |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 572 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 583 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG
> 587 | MeteringMode | int8u | 0 = Multi-segment 2 = Center-weighted average 3 = Spot 4 = Average 5 = Highlight
> 588 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 594 | WB_RGBLevels | int16u[3] |
> 778 | FocalLength | int16u |
> 780 | MinFocalLength | int16u |
> 782 | MaxFocalLength | int16u |
> 800 | SonyISO | int16u |
> 877 | MeterInfo? | - | --> Sony MeterInfo9 Tags
> 6096 | DistortionCorrParams | int16s[16] |
> 6129 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 6130 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 6131 | LensType2 | int16u | --> Sony LensType2 Values
> 6134 | LensType | int16u | --> Sony LensType Values
> 6136 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 6137 | DistortionCorrParamsNumber | int8u | 11 = 11 (APS-C) 16 = 16 (Full-frame)

## Sony MeterInfo9 Tags

Information possibly related to metering. Extracted only if the Unknown option is used.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | MeterInfo1Row1 | no |
> 90 | MeterInfo1Row2 | no |
> 180 | MeterInfo1Row3 | no |
> 270 | MeterInfo1Row4 | no |
> 360 | MeterInfo1Row5 | no |
> 450 | MeterInfo1Row6 | no |
> 540 | MeterInfo1Row7 | no |
> 630 | MeterInfo2Row1 | no |
> 740 | MeterInfo2Row2 | no |
> 850 | MeterInfo2Row3 | no |
> 960 | MeterInfo2Row4 | no |
> 1070 | MeterInfo2Row5 | no |
> 1180 | MeterInfo2Row6 | no |
> 1290 | MeterInfo2Row7 | no |
> 1400 | MeterInfo2Row8 | no |
> 1510 | MeterInfo2Row9 | no |

## Sony Tag202a Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1 | FocalPlaneAFPointsUsed | int8u |
> 2 | FocalPlaneAFPointArea | int16u[2] |
> 6 | FocalPlaneAFPointLocation1 | int16u[2] |
> 10 | FocalPlaneAFPointLocation2 | int16u[2] |
> 14 | FocalPlaneAFPointLocation3 | int16u[2] |
> 18 | FocalPlaneAFPointLocation4 | int16u[2] |
> 22 | FocalPlaneAFPointLocation5 | int16u[2] |
> 26 | FocalPlaneAFPointLocation6 | int16u[2] |
> 30 | FocalPlaneAFPointLocation7 | int16u[2] |
> 34 | FocalPlaneAFPointLocation8 | int16u[2] |
> 38 | FocalPlaneAFPointLocation9 | int16u[2] |
> 42 | FocalPlaneAFPointLocation10 | int16u[2] |
> 46 | FocalPlaneAFPointLocation11 | int16u[2] |
> 50 | FocalPlaneAFPointLocation12 | int16u[2] |
> 54 | FocalPlaneAFPointLocation13 | int16u[2] |
> 58 | FocalPlaneAFPointLocation14 | int16u[2] |
> 62 | FocalPlaneAFPointLocation15 | int16u[2] |

## Sony ShotInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | FaceInfoOffset | no |
> 6 | SonyDateTime | string[20] |
> 26 | SonyImageHeight | int16u |
> 28 | SonyImageWidth | int16u |
> 48 | FacesDetected | int16u |
> 50 | FaceInfoLength | no |
> 52 | MetaVersion | string[16] |
> 72 | FaceInfo1 | - | --> Sony FaceInfo1 Tags
> 94 | FaceInfo2 | - | --> Sony FaceInfo2 Tags

## Sony FaceInfo1 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Face1Position | int16u[4] | (top, left, height and width of detected face. Coordinates are relative to the full-sized unrotated image, with increasing Y downwards)
> 32 | Face2Position | int16u[4] |
> 64 | Face3Position | int16u[4] |
> 96 | Face4Position | int16u[4] |
> 128 | Face5Position | int16u[4] |
> 160 | Face6Position | int16u[4] |
> 192 | Face7Position | int16u[4] |
> 224 | Face8Position | int16u[4] |

## Sony FaceInfo2 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Face1Position | int16u[4] | (top, left, height and width of detected face. Coordinates are relative to the full-sized unrotated image, with increasing Y downwards)
> 37 | Face2Position | int16u[4] |
> 74 | Face3Position | int16u[4] |
> 111 | Face4Position | int16u[4] |
> 148 | Face5Position | int16u[4] |
> 185 | Face6Position | int16u[4] |
> 222 | Face7Position | int16u[4] |
> 259 | Face8Position | int16u[4] |

## Sony Tag900b Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | FacesDetected | no |
> 0 = 0 33 = 5 57 = 2 |  | 77 = 4 93 = 3 98 = 1 |  | 115 = 8 168 = 6 241 = 7
> 189 | FaceDetection | no | 0 = Off 98 = On

## Sony Tag9050a Tags

Data for tags 0x9050, 0x94xx and 0x2010 is encrypted by a simple substitution cipher, but the deciphered values are listed below.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SonyMaxAperture | int8u |
> 1 | SonyMinAperture | int8u |
> 32 | Shutter | int16u[3] | '0 0 0' = Silent / Electronic (0 0 0)
> 49 | FlashStatus | int8u |
> 0 = No Flash present 2 = Flash Inhibited 64 = Built-in Flash present 65 = Built-in Flash Fired 66 = Built-in Flash Inhibited 128 = External Flash present 129 = External Flash Fired
> 50 | ShutterCount | int32u | (total number of image exposures made by the camera, modulo 65536 for some models)
> 58 | SonyExposureTime | int16u |
> 60 | SonyFNumber | int16u |
> 63 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 76 | ShutterCount2 | int32u |
> 81 | SonyDateTime2 | undef[6] |
> 103 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 124 | InternalSerialNumber | int8u[4]~ |
> 240 | InternalSerialNumber | int8u[5] |
> 261 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 262 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 263 | LensType2 | int16u | --> Sony LensType2 Values
> 265 | LensType | int16u | --> Sony LensType Values (SLT models, and NEX with A-mount lenses)
> 267 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 276 | APS-CSizeCapture | int8u | 0 = Off 1 = On
> 277 | LensSpecFeatures | undef[2] |
> 278 | LensSpecFeatures | undef[2] |
> 416 | ShutterCount3 | int32u |
> 426 | ShutterCount3 | int32u |
> 445 | ShutterCount3 | int32u |

## Sony Tag9050b Tags

Valid from July 2015 for ILCE-6100/6300/6400/6500/6600/7C/7M3/7RM2/7RM3/7RM4/ 7SM2/9/9M2, ILCA-99M2.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | SonyMaxAperture | int8u |
> 1 | SonyMinAperture | int8u |
> 38 | Shutter | int16u[3] | '0 0 0' = Silent / Electronic (0 0 0)
> 57 | FlashStatus | int8u |
> 0 = No Flash present 2 = Flash Inhibited 64 = Built-in Flash present 65 = Built-in Flash Fired 66 = Built-in Flash Inhibited 128 = External Flash present 129 = External Flash Fired
> 58 | ShutterCount | int32u | (total number of image exposures made by the camera)
> 70 | SonyExposureTime | int16u |
> 72 | SonyFNumber | int16u |
> 75 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 80 | ShutterCount2 | int32u |
> 82 | ShutterCount2 | int32u |
> 88 | ShutterCount2 | int32u |
> 97 | SonyTimeMinSec | no |
> 107 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 109 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 115 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 136 | InternalSerialNumber | int8u[6]~ |
> 261 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 262 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 263 | LensType2 | int16u | --> Sony LensType2 Values
> 265 | LensType | int16u | --> Sony LensType Values (SLT models, and NEX with A-mount lenses)
> 267 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 276 | APS-CSizeCapture | int8u | 0 = Off 1 = On
> 278 | LensSpecFeatures | undef[2] |
> 415 | ShutterCount3 | int32u |
> 459 | ShutterCount3 | int32u |
> 461 | ShutterCount3 | int32u |
> 491 | APS-CSizeCapture | int8u | 0 = Off 1 = On
> 493 | LensSpecFeatures | undef[2] |
> 494 | APS-CSizeCapture | int8u | 0 = Off 1 = On
> 496 | LensSpecFeatures | undef[2] |
> 538 | APS-CSizeCapture | int8u | 0 = Off 1 = On
> 540 | LensSpecFeatures APS-CSizeCapture | undef[2] int8u | 0 = Off 1 = On
> 542 | LensSpecFeatures | undef[2] |

## Sony Tag9050c Tags

Valid from July 2020 for ILCE-1/7SM3, ILME-FX3.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 38 | Shutter | int16u[3] | '0 0 0' = Silent / Electronic (0 0 0)
> 57 | FlashStatus | int8u |
> 0 = No Flash present 2 = Flash Inhibited 64 = Built-in Flash present 65 = Built-in Flash Fired 66 = Built-in Flash Inhibited 128 = External Flash present 129 = External Flash Fired
> 58 | ShutterCount | int32u~ | (total number of image exposures made by the camera)
> 70 | SonyExposureTime | int16u |
> 72 | SonyFNumber | int16u |
> 75 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 80 | ShutterCount2 | int32u |
> 102 | SonyExposureTime | int16u |
> 104 | SonyFNumber | int16u |
> 107 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 136 | InternalSerialNumber | int8u[6]~ |
> 138 | InternalSerialNumber | int8u[6]~ |

## Sony Tag9400a Tags

Valid for many DSC, NEX and SLT models

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 8 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 12 | SequenceFileNumber | int32u | (file number in burst sequence)
> 16 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 18 | DigitalZoom | int8u | 0 = No 1 = Yes
> 26 | ShotNumberSincePowerUp | int32u |
> 34 | SequenceLength | int8u |
> 0 = Continuous 1 = 1 shot 2 = 2 shots 3 = 3 shots 4 = 4 shots 5 = 5 shots 6 = 6 shots 10 = 10 shots 100 = Continuous - iSweep Panorama 200 = Continuous - Sweep Panorama
> 40 | CameraOrientation | int8u | 1 = Horizontal (normal) 3 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 41 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG 3 = JPEG + MPO
> 68 | SonyImageHeight | int16u~ |
> 82 | ModelReleaseYear | int8u~ |

## Sony Tag9400b Tags

Valid for NEX-3N, ILCE-3000/3500, SLT-A58, DSC-WX60, DSC-WX300, DSC-RX100M2, DSC-HX50V, DSC-QX10/QX100.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 8 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 12 | SequenceFileNumber | int32u | (file number in burst sequence)
> 16 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 18 | DigitalZoom | int8u | 0 = No 1 = Yes
> 22 | ShotNumberSincePowerUp | int32u |
> 30 | SequenceLength | int8u |
> 0 = Continuous 1 = 1 shot 2 = 2 shots 3 = 3 shots 4 = 4 shots 5 = 5 shots 6 = 6 shots 10 = 10 shots 100 = Continuous - iSweep Panorama 200 = Continuous - Sweep Panorama
> 36 | CameraOrientation | int8u | 1 = Horizontal (normal) 3 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 37 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG 3 = JPEG + MPO
> 63 | SonyImageHeight | int16u~ |
> 70 | ModelReleaseYear | int8u~ |

## Sony Tag9400c Tags

Valid for DSC-HX60V/HX80/HX90V/HX99/HX350/HX400V/QX30/RX0/RX1RM2/RX10/ RX10M2/RX10M3/RX10M4/RX100M3/RX100M4/RX100M5/RX100M5A/RX100M6/RX100M7/WX220/ WX350/WX500, ILCE-1/7/7C/7R/7S/7M2/7M3/7RM2/7RM3/7RM4/7SM2/7SM3/9/9M2/5000/ 5100/6000/6100/6300/6400/6500/6600/QX1, ILCA-68/77M2/99M2.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 9 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 10 | ShotNumberSincePowerUp | int32u | (valid only for some models)
> 18 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 22 | SequenceLength | int8u |
> 0 = Continuous 1 = 1 shot 2 = 2 shots 3 = 3 shots 4 = 4 shots 5 = 5 shots 6 = 6 shots 7 = 7 shots 9 = 9 shots 10 = 10 shots 12 = 12 shots 16 = 16 shots 100 = Continuous - iSweep Panorama 200 = Continuous - Sweep Panorama
> 26 | SequenceFileNumber | int32u | (file number in burst sequence)
> 30 | SequenceLength | int8u |
> 0 = Continuous 1 = 1 file 2 = 2 files 3 = 3 files |  | 5 = 5 files 7 = 7 files 9 = 9 files 10 = 10 files
> 41 | CameraOrientation | int8u | 1 = Horizontal (normal) 3 = Rotate 180 6 = Rotate 90 CW 8 = Rotate 270 CW
> 42 | Quality2 | int8u | 0 = JPEG 1 = RAW 2 = RAW + JPEG 3 = JPEG + MPO 1 = JPEG 2 = RAW 3 = RAW + JPEG 4 = HEIF 6 = RAW + HEIF
> 71 | SonyImageHeight | int16u~ |
> 83 | ModelReleaseYear | int8u~ |

## Sony Tag9401 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1102 | ISOInfo | - | --> Sony ISOInfo Tags
> 1176 | ISOInfo | - | --> Sony ISOInfo Tags
> 1181 | ISOInfo | - | --> Sony ISOInfo Tags
> 1185 | ISOInfo | - | --> Sony ISOInfo Tags
> 1186 | ISOInfo | - | --> Sony ISOInfo Tags
> 1437 | ISOInfo | - | --> Sony ISOInfo Tags
> 1588 | ISOInfo | - | --> Sony ISOInfo Tags
> 1590 | ISOInfo | - | --> Sony ISOInfo Tags
> 1612 | ISOInfo | - | --> Sony ISOInfo Tags
> 1619 | ISOInfo | - | --> Sony ISOInfo Tags
> 1656 | ISOInfo | - | --> Sony ISOInfo Tags
> 1720 | ISOInfo | - | --> Sony ISOInfo Tags
> 1758 | ISOInfo | - | --> Sony ISOInfo Tags
> 1767 | ISOInfo | - | --> Sony ISOInfo Tags

## Sony ISOInfo Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | ISOSetting | int8u |
> 2 | ISOAutoMin | int8u |
> 4 | ISOAutoMax | int8u |

## Sony Tag9402 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | AmbientTemperature | int8s |
> 22 | FocusMode | int8u | [val & 0x7f] 0 = Manual 2 = AF-S 3 = AF-C 4 = AF-A 6 = DMF
> 23 | AFAreaMode | int8u |
> 0 = Multi 1 = Center 2 = Spot 3 = Flexible Spot 10 = Selective (for Miniature effect) 11 = Zone 12 = Expanded Flexible Spot 14 = Tracking 15 = Face Tracking 20 = Animal Eye Tracking 255 = Manual
> 45 | FocusPosition2 | int8u |

## Sony Tag9403 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 5 | CameraTemperature | int8s |

## Sony Tag9404a Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 11 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 13 | IntelligentAuto | int8u | 0 = Off 1 = On
> 25 | LensZoomPosition | int16u |

## Sony Tag9404b Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 12 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 14 | IntelligentAuto | int8u | 0 = Off 1 = On
> 30 | LensZoomPosition | int16u |
> 32 | FocusPosition2 | int8u |

## Sony Tag9404c Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 11 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 13 | IntelligentAuto | int8u | 0 = Off 1 = On

## Sony Tag9405a Tags

Valid for SLT, NEX, ILCE-3000/3500 and several DSC models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 1536 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 1537 | DistortionCorrection | int8u | 0 = None 1 = Applied
> 1539 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 1540 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 1541 | LensType2 | int16u | --> Sony LensType2 Values (E-mount lenses)
> 1544 | LensType | int16u | --> Sony LensType Values (A-mount lenses on SLT and NEX)
> 1610 | VignettingCorrParams | int16s[16] |
> 1642 | ChromaticAberrationCorrParams | int16s[32] |
> 1738 | DistortionCorrParams | int16s[16] |

## Sony Tag9405b Tags

Valid for DSC-HX60V/HX80/HX90V/HX99/HX350/HX400V/QX30/RX0/RX10/RX10M2/ RX10M3/RX10M4/RX100M3/RX100M4/RX100M5/RX100M5A/RX100M6/RX100M7/WX220/WX350, ILCE-7/7M2/7M3/7R/7RM2/7RM3/7RM4/7S/7SM2/9/9M2/5000/5100/6000/6100/6300/ 6400/6500/6600/QX1, ILCA-68/77M2/99M2.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | SonyISO | int16u |
> 6 | BaseISO | int16u |
> 10 | StopsAboveBaseISO | int16u |
> 14 | SonyExposureTime2 | int16u |
> 16 | ExposureTime | rational32u |
> 20 | SonyFNumber | int16u |
> 22 | SonyMaxApertureValue | int16u |
> 36 | SequenceImageNumber | int32u | (number of images captured in burst sequence)
> 52 | ReleaseMode2 | int8u | --> Sony ReleaseMode2 Values
> 62 | SonyImageWidthMax | int16u |
> 64 | SonyImageHeightMax | int16u |
> 66 | HighISONoiseReduction | int8u | 0 = Off 1 = Low 2 = Normal 3 = High
> 68 | LongExposureNoiseReduction | int8u | 0 = Off 1 = On
> 70 | PictureEffect2 | int8u | --> Sony PictureEffect2 Values
> 72 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 74 | CreativeStyle | int8u |
> 0 = Standard 1 = Vivid 2 = Neutral 3 = Portrait 4 = Landscape 5 = B&W 6 = Clear 7 = Deep 8 = Light 9 = Sunset 10 = Night View/Portrait 11 = Autumn Leaves 13 = Sepia
> 82 | Sharpness | int8s |
> 90 | DistortionCorrParamsPresent | int8u | 0 = No 1 = Yes
> 91 | DistortionCorrection | int8u | 0 = None 1 = Applied
> 93 | LensFormat | int8u | 0 = Unknown 1 = APS-C 2 = Full-frame
> 94 | LensMount | int8u | 0 = Unknown 1 = A-mount 2 = E-mount
> 96 | LensType2 | int16u | --> Sony LensType2 Values (E-mount lenses)
> 98 | LensType | int16u | --> Sony LensType Values (A-mount lenses on SLT and NEX)
> 100 | DistortionCorrParams | int16s[16] |
> 834 | LensZoomPosition | int16u |
> 842 | VignettingCorrParams | int16s[16] |
> 846 | LensZoomPosition | int16u |
> 848 | VignettingCorrParams | int16s[16] |
> 858 | LensZoomPosition | int16u |
> 860 | VignettingCorrParams | int16s[16] |
> 872 | VignettingCorrParams | int16s[16] |
> 892 | ChromaticAberrationCorrParams | int16s[32] |
> 900 | ChromaticAberrationCorrParams | int16s[32] |
> 924 | ChromaticAberrationCorrParams | int16s[32] |
> 944 | ChromaticAberrationCorrParams | int16s[32] |
> 952 | ChromaticAberrationCorrParams | int16s[32] |

## Sony Tag9406 Tags

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 5 | BatteryTemperature | int8u |
> 6 | BatteryLevelGrip1 | int8u |
> 7 | BatteryLevel | int8u |
> 8 | BatteryLevelGrip2 | int8u |

## Sony Tag940a Tags

These tags are currently extracted for SLT models only.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 4 | AFPointsSelected | int32u |
> 0x0 = (none) 0x7801 = Center Zone 0x1821c = Right Zone 0x3ffff = (all LA-EA4) 0x605c0 = Left Zone 0x7fffffff = (all) 0xffffffff = n/a Bit 0 = Center Bit 1 = Top Bit 2 = Upper-right Bit 3 = Right Bit 4 = Lower-right Bit 5 = Bottom |  | Bit 6 = Lower-left Bit 7 = Left Bit 8 = Upper-left Bit 9 = Far Right Bit 10 = Far Left Bit 11 = Upper-middle Bit 12 = Near Right Bit 13 = Lower-middle Bit 14 = Near Left Bit 15 = Upper Far Right Bit 16 = Lower Far Right Bit 17 = Lower Far Left Bit 18 = Upper Far Left

## Sony Tag940c Tags

E-mount cameras only.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 8 | LensMount2 | int8u | 0 = Unknown 1 = A-mount (1) 4 = E-mount 5 = A-mount (5)
> 9 | LensType3 | int16u | --> Sony LensType2 Values
> 11 | CameraE-mountVersion | int16u |
> 13 | LensE-mountVersion | int16u |
> 20 | LensFirmwareVersion | int16u~ |

## Sony AFInfo Tags

These tags are currently extracted for SLT models only.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 2 | AFType | int8u | 1 = 15-point 2 = 19-point 3 = 79-point
> 4 | AFStatusActiveSensor | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 5 | FocusMode | int8u | (ILCA models only) 0 = Manual 2 = AF-S 3 = AF-C 4 = AF-A 6 = DMF
> 7 | AFPoint | int8u | (models with 15-point AF)
> 0 = Upper-left 1 = Left 2 = Lower-left 3 = Far Left 4 = Top (horizontal) 5 = Near Right 6 = Center (horizontal) 7 = Near Left 8 = Bottom (horizontal) |  | 9 = Top (vertical) 10 = Center (vertical) 11 = Bottom (vertical) 12 = Far Right 13 = Upper-right 14 = Right 15 = Lower-right 16 = Upper-middle 17 = Lower-middle
> (models with 19-point AF)
> 0 = Upper Far Left 1 = Upper-left (horizontal) 2 = Far Left (horizontal) 3 = Left (horizontal) 4 = Lower Far Left 5 = Lower-left (horizontal) 6 = Upper-left (vertical) 7 = Left (vertical) 8 = Lower-left (vertical) 9 = Far Left (vertical) 10 = Top (horizontal) 11 = Near Right 12 = Center (horizontal) 13 = Near Left 14 = Bottom (horizontal) |  | 15 = Top (vertical) 16 = Upper-middle 17 = Center (vertical) 18 = Lower-middle 19 = Bottom (vertical) 20 = Upper Far Right 21 = Upper-right (horizontal) 22 = Far Right (horizontal) 23 = Right (horizontal) 24 = Lower Far Right 25 = Lower-right (horizontal) 26 = Far Right (vertical) 27 = Upper-right (vertical) 28 = Right (vertical) 29 = Lower-right (vertical)
> 8 | AFPointInFocus | int8u | (models with 15-point AF)
> 0 = Upper-left 1 = Left 2 = Lower-left 3 = Far Left 4 = Top (horizontal) 5 = Near Right 6 = Center (horizontal) 7 = Near Left 8 = Bottom (horizontal) 9 = Top (vertical) |  | 10 = Center (vertical) 11 = Bottom (vertical) 12 = Far Right 13 = Upper-right 14 = Right 15 = Lower-right 16 = Upper-middle 17 = Lower-middle 255 = (none)
> (models with 19-point AF)
> 0 = Upper Far Left 1 = Upper-left (horizontal) 2 = Far Left (horizontal) 3 = Left (horizontal) 4 = Lower Far Left 5 = Lower-left (horizontal) 6 = Upper-left (vertical) 7 = Left (vertical) 8 = Lower-left (vertical) 9 = Far Left (vertical) 10 = Top (horizontal) 11 = Near Right 12 = Center (horizontal) 13 = Near Left 14 = Bottom (horizontal) 15 = Top (vertical) |  | 16 = Upper-middle 17 = Center (vertical) 18 = Lower-middle 19 = Bottom (vertical) 20 = Upper Far Right 21 = Upper-right (horizontal) 22 = Far Right (horizontal) 23 = Right (horizontal) 24 = Lower Far Right 25 = Lower-right (horizontal) 26 = Far Right (vertical) 27 = Upper-right (vertical) 28 = Right (vertical) 29 = Lower-right (vertical) 255 = (none)
> 9 | AFPointAtShutterRelease | int8u | (models with 15-point AF)
> 0 = Upper-left 1 = Left 2 = Lower-left 3 = Far Left 4 = Top (horizontal) 5 = Near Right 6 = Center (horizontal) 7 = Near Left 8 = Bottom (horizontal) 9 = Top (vertical) |  | 10 = Center (vertical) 11 = Bottom (vertical) 12 = Far Right 13 = Upper-right 14 = Right 15 = Lower-right 16 = Upper-middle 17 = Lower-middle 30 = (out of focus)
> (models with 19-point AF)
> 0 = Upper Far Left 1 = Upper-left (horizontal) 2 = Far Left (horizontal) 3 = Left (horizontal) 4 = Lower Far Left 5 = Lower-left (horizontal) 6 = Upper-left (vertical) 7 = Left (vertical) 8 = Lower-left (vertical) 9 = Far Left (vertical) 10 = Top (horizontal) 11 = Near Right 12 = Center (horizontal) 13 = Near Left 14 = Bottom (horizontal) 15 = Top (vertical) |  | 16 = Upper-middle 17 = Center (vertical) 18 = Lower-middle 19 = Bottom (vertical) 20 = Upper Far Right 21 = Upper-right (horizontal) 22 = Far Right (horizontal) 23 = Right (horizontal) 24 = Lower Far Right 25 = Lower-right (horizontal) 26 = Far Right (vertical) 27 = Upper-right (vertical) 28 = Right (vertical) 29 = Lower-right (vertical) 30 = (out of focus)
> 10 | AFAreaMode | int8u | 0 = Wide 1 = Spot 2 = Local 3 = Zone
> 11 | FocusMode | int8u |
> 0 = Manual 2 = AF-S 3 = AF-C |  | 4 = AF-A 6 = DMF 7 = AF-D
> 16 | AFPointsUsed | int8u[10] |
> 0x0 = (none) Bit 0 = A5 Bit 1 = A6 Bit 2 = A7 Bit 3 = B2 Bit 4 = B3 Bit 5 = B4 Bit 6 = B5 Bit 7 = B6 Bit 8 = B7 Bit 9 = B8 Bit 10 = B9 Bit 11 = B10 Bit 12 = C1 Bit 13 = C2 Bit 14 = C3 Bit 15 = C4 Bit 16 = C5 Bit 17 = C6 Bit 18 = C7 Bit 19 = C8 Bit 20 = C9 Bit 21 = C10 Bit 22 = C11 Bit 23 = D1 Bit 24 = D2 Bit 25 = D3 |  | Bit 26 = D4 Bit 27 = D5 Bit 28 = D6 Bit 29 = D7 Bit 30 = D8 Bit 31 = D9 Bit 32 = D10 Bit 33 = D11 Bit 34 = E1 Bit 35 = E2 Bit 36 = E3 Bit 37 = E4 Bit 38 = E5 Bit 39 = E6 Bit 40 = E7 Bit 41 = E8 Bit 42 = E9 Bit 43 = E10 Bit 44 = E11 Bit 45 = F1 Bit 46 = F2 Bit 47 = F3 Bit 48 = F4 Bit 49 = F5 Bit 50 = F6 Bit 51 = F7 Bit 52 = F8 |  | Bit 53 = F9 Bit 54 = F10 Bit 55 = F11 Bit 56 = G1 Bit 57 = G2 Bit 58 = G3 Bit 59 = G4 Bit 60 = G5 Bit 61 = G6 Bit 62 = G7 Bit 63 = G8 Bit 64 = G9 Bit 65 = G10 Bit 66 = G11 Bit 67 = H2 Bit 68 = H3 Bit 69 = H4 Bit 70 = H5 Bit 71 = H6 Bit 72 = H7 Bit 73 = H8 Bit 74 = H9 Bit 75 = H10 Bit 76 = I5 Bit 77 = I6 Bit 78 = I7
> 17 | AFStatus15 AFStatus19 | - - | --> Sony AFStatus15 Tags --> Sony AFStatus19 Tags
> 55 | AFPoint | int8u |
> 0 = B4 1 = C4 2 = D4 3 = E4 4 = F4 5 = G4 6 = H4 7 = B3 8 = C3 9 = D3 10 = E3 11 = F3 12 = G3 13 = H3 14 = B2 15 = C2 16 = D2 17 = E2 18 = F2 19 = G2 20 = H2 21 = C1 22 = D1 23 = E1 24 = F1 25 = G1 26 = A7 Vertical 27 = A6 Vertical 28 = A5 Vertical 29 = C7 Vertical 30 = C6 Vertical 31 = C5 Vertical 32 = E7 Vertical 33 = E6 Center Vertical 34 = E5 Vertical 35 = G7 Vertical 36 = G6 Vertical 37 = G5 Vertical 38 = I7 Vertical 39 = I6 Vertical 40 = I5 Vertical 41 = A7 42 = B7 43 = C7 44 = D7 45 = E7 46 = F7 47 = G7 |  | 48 = H7 49 = I7 50 = A6 51 = B6 52 = C6 53 = D6 54 = E6 Center 55 = F6 56 = G6 57 = H6 58 = I6 59 = A5 60 = B5 61 = C5 62 = D5 63 = E5 64 = F5 65 = G5 66 = H5 67 = I5 68 = C11 69 = D11 70 = E11 71 = F11 72 = G11 73 = B10 74 = C10 75 = D10 76 = E10 77 = F10 78 = G10 79 = H10 80 = B9 81 = C9 82 = D9 83 = E9 84 = F9 85 = G9 86 = H9 87 = B8 88 = C8 89 = D8 90 = E8 91 = F8 92 = G8 93 = H8 94 = E6 Center F2.8 255 = (none)
> 56 | AFPointInFocus | int8u |
> 0 = B4 1 = C4 2 = D4 3 = E4 4 = F4 5 = G4 6 = H4 7 = B3 8 = C3 9 = D3 10 = E3 11 = F3 12 = G3 13 = H3 14 = B2 15 = C2 16 = D2 17 = E2 18 = F2 19 = G2 20 = H2 21 = C1 22 = D1 23 = E1 24 = F1 25 = G1 26 = A7 Vertical 27 = A6 Vertical 28 = A5 Vertical 29 = C7 Vertical 30 = C6 Vertical 31 = C5 Vertical 32 = E7 Vertical 33 = E6 Center Vertical 34 = E5 Vertical 35 = G7 Vertical 36 = G6 Vertical 37 = G5 Vertical 38 = I7 Vertical 39 = I6 Vertical 40 = I5 Vertical 41 = A7 42 = B7 43 = C7 44 = D7 45 = E7 46 = F7 47 = G7 |  | 48 = H7 49 = I7 50 = A6 51 = B6 52 = C6 53 = D6 54 = E6 Center 55 = F6 56 = G6 57 = H6 58 = I6 59 = A5 60 = B5 61 = C5 62 = D5 63 = E5 64 = F5 65 = G5 66 = H5 67 = I5 68 = C11 69 = D11 70 = E11 71 = F11 72 = G11 73 = B10 74 = C10 75 = D10 76 = E10 77 = F10 78 = G10 79 = H10 80 = B9 81 = C9 82 = D9 83 = E9 84 = F9 85 = G9 86 = H9 87 = B8 88 = C8 89 = D8 90 = E8 91 = F8 92 = G8 93 = H8 94 = E6 Center F2.8 255 = (none)
> 57 | AFPointAtShutterRelease | int8u |
> 0 = B4 1 = C4 2 = D4 3 = E4 4 = F4 5 = G4 6 = H4 7 = B3 8 = C3 9 = D3 10 = E3 11 = F3 12 = G3 13 = H3 14 = B2 15 = C2 16 = D2 17 = E2 18 = F2 19 = G2 20 = H2 21 = C1 22 = D1 23 = E1 24 = F1 25 = G1 26 = A7 Vertical 27 = A6 Vertical 28 = A5 Vertical 29 = C7 Vertical 30 = C6 Vertical 31 = C5 Vertical 32 = E7 Vertical 33 = E6 Center Vertical 34 = E5 Vertical 35 = G7 Vertical 36 = G6 Vertical 37 = G5 Vertical 38 = I7 Vertical 39 = I6 Vertical 40 = I5 Vertical 41 = A7 42 = B7 43 = C7 44 = D7 45 = E7 46 = F7 47 = G7 |  | 48 = H7 49 = I7 50 = A6 51 = B6 52 = C6 53 = D6 54 = E6 Center 55 = F6 56 = G6 57 = H6 58 = I6 59 = A5 60 = B5 61 = C5 62 = D5 63 = E5 64 = F5 65 = G5 66 = H5 67 = I5 68 = C11 69 = D11 70 = E11 71 = F11 72 = G11 73 = B10 74 = C10 75 = D10 76 = E10 77 = F10 78 = G10 79 = H10 80 = B9 81 = C9 82 = D9 83 = E9 84 = F9 85 = G9 86 = H9 87 = B8 88 = C8 89 = D8 90 = E8 91 = F8 92 = G8 93 = H8 94 = E6 Center F2.8 95 = (none)
> 58 | AFAreaMode | int8u | 0 = Wide 1 = Center 2 = Flexible Spot 3 = Zone 4 = Expanded Flexible Spot
> 59 | AFStatusActiveSensor | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 67 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values
> 80 | AFMicroAdj | int8s |
> 125 | AFStatus79 | - | --> Sony AFStatus79 Tags
> 366 | AFPointsUsed | int32u | (SLT models only)
> 0x0 = (none) Bit 0 = Center Bit 1 = Top Bit 2 = Upper-right Bit 3 = Right Bit 4 = Lower-right Bit 5 = Bottom Bit 6 = Lower-left Bit 7 = Left Bit 8 = Upper-left |  | Bit 9 = Far Right Bit 10 = Far Left Bit 11 = Upper-middle Bit 12 = Near Right Bit 13 = Lower-middle Bit 14 = Near Left Bit 15 = Upper Far Right Bit 16 = Lower Far Right Bit 17 = Lower Far Left Bit 18 = Upper Far Left
> 381 | AFMicroAdj | int8s |
> 382 | ExposureProgram | int8u | --> Sony ExposureProgram3 Values

## Sony AFStatus19 Tags

AF Status information for models with 19-point AF.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFStatusUpperFarLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 2 | AFStatusUpper-leftHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 4 | AFStatusFarLeftHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 6 | AFStatusLeftHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 8 | AFStatusLowerFarLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 10 | AFStatusLower-leftHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 12 | AFStatusUpper-leftVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 14 | AFStatusLeftVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 16 | AFStatusLower-leftVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 18 | AFStatusFarLeftVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 20 | AFStatusTopHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 22 | AFStatusNearRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 24 | AFStatusCenterHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 26 | AFStatusNearLeft | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 28 | AFStatusBottomHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 30 | AFStatusTopVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 32 | AFStatusUpper-middle | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 34 | AFStatusCenterVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 36 | AFStatusLower-middle | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 38 | AFStatusBottomVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 40 | AFStatusUpperFarRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 42 | AFStatusUpper-rightHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 44 | AFStatusFarRightHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 46 | AFStatusRightHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 48 | AFStatusLowerFarRight | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 50 | AFStatusLower-rightHorizontal | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 52 | AFStatusFarRightVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 54 | AFStatusUpper-rightVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 56 | AFStatusRightVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 58 | AFStatusLower-rightVertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus

## Sony AFStatus79 Tags

AF Status information for models with 79-point AF.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | AFStatus_00_B4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 2 | AFStatus_01_C4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 4 | AFStatus_02_D4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 6 | AFStatus_03_E4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 8 | AFStatus_04_F4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 10 | AFStatus_05_G4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 12 | AFStatus_06_H4 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 14 | AFStatus_07_B3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 16 | AFStatus_08_C3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 18 | AFStatus_09_D3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 20 | AFStatus_10_E3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 22 | AFStatus_11_F3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 24 | AFStatus_12_G3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 26 | AFStatus_13_H3 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 28 | AFStatus_14_B2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 30 | AFStatus_15_C2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 32 | AFStatus_16_D2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 34 | AFStatus_17_E2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 36 | AFStatus_18_F2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 38 | AFStatus_19_G2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 40 | AFStatus_20_H2 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 42 | AFStatus_21_C1 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 44 | AFStatus_22_D1 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 46 | AFStatus_23_E1 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 48 | AFStatus_24_F1 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 50 | AFStatus_25_G1 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 52 | AFStatus_26_A7_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 54 | AFStatus_27_A6_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 56 | AFStatus_28_A5_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 58 | AFStatus_29_C7_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 60 | AFStatus_30_C6_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 62 | AFStatus_31_C5_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 64 | AFStatus_32_E7_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 66 | AFStatus_33_E6_Center_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 68 | AFStatus_34_E5_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 70 | AFStatus_35_G7_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 72 | AFStatus_36_G6_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 74 | AFStatus_37_G5_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 76 | AFStatus_38_I7_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 78 | AFStatus_39_I6_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 80 | AFStatus_40_I5_Vertical | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 82 | AFStatus_41_A7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 84 | AFStatus_42_B7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 86 | AFStatus_43_C7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 88 | AFStatus_44_D7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 90 | AFStatus_45_E7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 92 | AFStatus_46_F7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 94 | AFStatus_47_G7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 96 | AFStatus_48_H7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 98 | AFStatus_49_I7 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 100 | AFStatus_50_A6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 102 | AFStatus_51_B6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 104 | AFStatus_52_C6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 106 | AFStatus_53_D6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 108 | AFStatus_54_E6_Center | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 110 | AFStatus_55_F6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 112 | AFStatus_56_G6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 114 | AFStatus_57_H6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 116 | AFStatus_58_I6 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 118 | AFStatus_59_A5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 120 | AFStatus_60_B5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 122 | AFStatus_61_C5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 124 | AFStatus_62_D5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 126 | AFStatus_63_E5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 128 | AFStatus_64_F5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 130 | AFStatus_65_G5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 132 | AFStatus_66_H5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 134 | AFStatus_67_I5 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 136 | AFStatus_68_C11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 138 | AFStatus_69_D11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 140 | AFStatus_70_E11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 142 | AFStatus_71_F11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 144 | AFStatus_72_G11 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 146 | AFStatus_73_B10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 148 | AFStatus_74_C10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 150 | AFStatus_75_D10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 152 | AFStatus_76_E10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 154 | AFStatus_77_F10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 156 | AFStatus_78_G10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 158 | AFStatus_79_H10 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 160 | AFStatus_80_B9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 162 | AFStatus_81_C9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 164 | AFStatus_82_D9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 166 | AFStatus_83_E9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 168 | AFStatus_84_F9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 170 | AFStatus_85_G9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 172 | AFStatus_86_H9 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 174 | AFStatus_87_B8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 176 | AFStatus_88_C8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 178 | AFStatus_89_D8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 180 | AFStatus_90_E8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 182 | AFStatus_91_F8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 184 | AFStatus_92_G8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 186 | AFStatus_93_H8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus
> 188 | AFStatus_94_E6_Center_F2-8 | int16s |
> -32768 = Out of Focus |  | 0 = In Focus

## Sony Tag940e Tags

E-mount models.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 6662 | TiffMeteringImageWidth | no |
> 6663 | TiffMeteringImageHeight | no |
> 6664 | TiffMeteringImage | no | (13(?)-bit intensity data from 1320 (1200) metering segments, extracted as a 16-bit TIFF image)

## Sony Tag9416 Tags

Valid for the ILCE-1/7M4/7SM3, ILME-FX3.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0 | Tag9416_0000 | no |
> 4 | SonyISO | no |
> 6 | StopsAboveBaseISO | no |
> 10 | SonyExposureTime2 | no |
> 12 | ExposureTime | no |
> 16 | SonyFNumber2 | no |
> 18 | SonyMaxApertureValue | no |
> 29 | SequenceImageNumber | no | (number of images captured in burst sequence)
> 53 | ExposureProgram | no | --> Sony ExposureProgram3 Values
> 72 | LensMount | no | 0 = Unknown 1 = A-mount 2 = E-mount 3 = A-mount (3)
> 73 | LensFormat | no | 0 = Unknown 1 = APS-C 2 = Full-frame
> 74 | LensMount | no | 0 = Unknown 1 = A-mount 2 = E-mount
> 75 | LensType2 | no | --> Sony LensType2 Values
> 77 | LensType | no | --> Sony LensType Values
> 79 | DistortionCorrParams | no |
> 112 | PictureProfile | no |
> 0 = Gamma Still - Standard/Neutral (PP2) 1 = Gamma Still - Portrait 3 = Gamma Still - Night View/Portrait 4 = Gamma Still - B&W/Sepia 5 = Gamma Still - Clear 6 = Gamma Still - Deep 7 = Gamma Still - Light 8 = Gamma Still - Vivid 9 = Gamma Still - Real 10 = Gamma Movie (PP1) 22 = Gamma ITU709 (PP3 or PP4) 24 = Gamma Cine1 (PP5) 25 = Gamma Cine2 (PP6) 26 = Gamma Cine3 27 = Gamma Cine4 28 = Gamma S-Log2 (PP7) 29 = Gamma ITU709 (800%) 31 = Gamma S-Log3 (PP8 or PP9) 33 = Gamma HLG2 (PP10) 34 = Gamma HLG3 37 = FL 38 = VV2 39 = IN 40 = SH
> 113 | FocalLength | no |
> 115 | MinFocalLength | no |
> 117 | MaxFocalLength | no |
> 2191 | VignettingCorrParams | no |
> 2193 | VignettingCorrParams | no |
> 2324 | ChromaticAberrationCorrParams | no |
> 2326 | ChromaticAberrationCorrParams | no |

## Sony PIC Tags

The TextInfo data is extracted as a block to preserve the formatting, and some of the more interesting information is extracted as separate tags.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 'BC:' | Barcode | no |
> 'BarCode:' | Barcode | no |
> 'Capt:' | SensorTemperature | no |
> 'FWVer:' | FirmwareVersion | no |
> 'IFD' | PIC_IFD | - | --> Sony Tags
> 'Temp:' | CameraTemperature | no |
> 'Temp:Clbt:' | BoardTemperature | no |
> 'TextInfo1' | TextInfo1 | no |
> 'TextInfo2' | TextInfo2 | no |
> 'VR Enable C:' | VibrationReduction | no | 0 = Off 1 = On
> 'barcode:' | Barcode | no |

## Sony Ericsson Tags

Maker notes found in images from some Sony Ericsson phones.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0201 | PreviewImageStart | int32u* | (a small 320x200 preview image)
> 0x0202 | PreviewImageLength | int32u* |
> 0x2000 | MakerNoteVersion | undef[4] |

## Sony SRF Tags

The maker notes in SRF (Sony Raw Format) images contain 7 IFD's with family 1 group names SRF0 through SRF6. SRF0 and SRF1 use the tags in this table, while SRF2 through SRF5 use the tags in the next table, and SRF6 uses standard EXIF tags. All information other than SRF0 is encrypted, but thanks to Dave Coffin the decryption algorithm is known. SRF images are written by the Sony DSC-F828 and DSC-V3.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0000 | SRF2Key | no | (key to decrypt maker notes from the start of SRF2)
> 0x0001 | DataKey | no | (key to decrypt the rest of the file from the end of the maker notes)

## Sony SRF2 Tags

These tags are found in the SRF2 through SRF5 IFD's.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x0002 | SRF6Offset | no |
> 0x0003 | SRFDataOffset? | no |
> 0x0004 | RawDataOffset | no |
> 0x0005 | RawDataLength | no |
> 0x0043 | MaxApertureAtMaxFocal | no |
> 0x0044 | MaxApertureAtMinFocal | no |
> 0x0045 | MinFocalLength | no |
> 0x0046 | MaxFocalLength | no |
> 0x00c0 | WBRedDaylight | no |
> 0x00c1 | WBGreenDaylight | no |
> 0x00c2 | WBBlueDaylight | no |
> 0x00c3 | WBRedCloudy | no |
> 0x00c4 | WBGreenCloudy | no |
> 0x00c5 | WBBlueCloudy | no |
> 0x00c6 | WBRedFluorescent | no |
> 0x00c7 | WBGreenFluorescent | no |
> 0x00c8 | WBBlueFluorescent | no |
> 0x00c9 | WBRedTungsten | no |
> 0x00ca | WBGreenTungsten | no |
> 0x00cb | WBBlueTungsten | no |
> 0x00cc | WBRedFlash | no |
> 0x00cd | WBGreenFlash | no |
> 0x00ce | WBBlueFlash | no |
> 0x00d0 | WBRedAsShot | no |
> 0x00d1 | WBGreenAsShot | no |
> 0x00d2 | WBBlueAsShot | no |

## Sony SR2Private Tags

The SR2 format uses the DNGPrivateData tag to reference a private IFD containing these tags. SR2 images are written by the Sony DSC-R1, but this information is also written to ARW images by other models.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x7200 | SR2SubIFDOffset | no |
> 0x7201 | SR2SubIFDLength | no |
> 0x7221 | SR2SubIFDKey | no | (key to decrypt SR2SubIFD)
> 0x7240 | IDC_IFD | - | --> SonyIDC Tags
> 0x7241 | IDC2_IFD | - | --> SonyIDC Tags
> 0x7250 | MRWInfo | - | --> MinoltaRaw Tags

## Sony SR2SubIFD Tags

Tags in the encrypted SR2SubIFD

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x7300 | BlackLevel | int16u[4]! |
> 0x7302 | WB_GRBGLevelsAuto | int16s[4]! |
> 0x7303 | WB_GRBGLevels | int16s[4]! |
> 0x7310 | BlackLevel | int16u[4]! |
> 0x7312 | WB_RGGBLevelsAuto | int16s[4]! |
> 0x7313 | WB_RGGBLevels | int16s[4]! |
> 0x7480 | WB_RGBLevelsDaylight | int16s[4]! |
> 0x7481 | WB_RGBLevelsCloudy | int16s[4]! |
> 0x7482 | WB_RGBLevelsTungsten | int16s[4]! |
> 0x7483 | WB_RGBLevelsFlash | int16s[4]! |
> 0x7484 | WB_RGBLevels4500K | int16s[4]! |
> 0x7486 | WB_RGBLevelsFluorescent | int16s[4]! |
> 0x74a0 | MaxApertureAtMaxFocal | no |
> 0x74a1 | MaxApertureAtMinFocal | no |
> 0x74a2 | MaxFocalLength | no |
> 0x74a3 | MinFocalLength | no |
> 0x74c0 | SR2DataIFD | - | --> Sony SR2DataIFD Tags
> 0x7800 | ColorMatrix | no |
> 0x7820 | WB_RGBLevelsDaylight | int16s[3]! |
> 0x7821 | WB_RGBLevelsCloudy | int16s[3]! |
> 0x7822 | WB_RGBLevelsTungsten | int16s[3]! |
> 0x7823 | WB_RGBLevelsFlash | int16s[3]! |
> 0x7824 | WB_RGBLevels4500K | int16s[3]! |
> 0x7825 | WB_RGBLevelsShade | int16s[3]! |
> 0x7826 | WB_RGBLevelsFluorescent | int16s[3]! |
> 0x7827 | WB_RGBLevelsFluorescentP1 | int16s[3]! |
> 0x7828 | WB_RGBLevelsFluorescentP2 | int16s[3]! |
> 0x7829 | WB_RGBLevelsFluorescentM1 | int16s[3]! |
> 0x782a | WB_RGBLevels8500K | int16s[3]! |
> 0x782b | WB_RGBLevels6000K | int16s[3]! |
> 0x782c | WB_RGBLevels3200K | int16s[3]! |
> 0x782d | WB_RGBLevels2500K | int16s[3]! |
> 0x787f | WhiteLevel | int16u[3]! |
> 0x797d | VignettingCorrParams | no |
> 0x7980 | ChromaticAberrationCorrParams | no |
> 0x7982 | DistortionCorrParams | no |

## Sony SR2DataIFD Tags

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x7770 | ColorMode | no |

## Sony PMP Tags

These tags are written in the proprietary-format header of PMP images from the DSC-F1.

> Index1 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 8 | JpgFromRawStart | no | (OK, not really a RAW file, but this mechanism is used to allow extraction of the JPEG image from a PMP file)
> 12 | JpgFromRawLength | no |
> 22 | SonyImageWidth | no |
> 24 | SonyImageHeight | no |
> 27 | Orientation | no | 0 = Horizontal (normal) 1 = Rotate 270 CW 2 = Rotate 180 3 = Rotate 90 CW
> 29 | ImageQuality | no | 8 = Snap Shot 23 = Standard 51 = Fine
> 52 | Comment | no |
> 76 | DateTimeOriginal | no |
> 84 | ModifyDate | no |
> 102 | ExposureTime | no |
> 106 | FNumber | no |
> 108 | ExposureCompensation | no |
> 112 | FocalLength | no |
> 118 | Flash | no | 0 = No Flash 1 = Fired

## Sony rtmd Tags

These tags are extracted from the 'rtmd' timed metadata of MP4 videos from some models when the ExtractEmbedded option is used.

> Tag ID | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 0x8000 | FNumber | no |
> 0x8109 | ExposureTime | no |
> 0x810a | MasterGainAdjustment | no |
> 0x810b | ISO | no |
> 0x810c | ElectricalExtenderMagnification | no |
> 0x8500 | GPSVersionID | no |
> 0x8501 | GPSLatitudeRef | no | 'N' = North 'S' = South
> 0x8502 | GPSLatitude | no |
> 0x8503 | GPSLongitudeRef | no | 'E' = East 'W' = West
> 0x8504 | GPSLongitude | no |
> 0x8507 | GPSTimeStamp | no |
> 0x8509 | GPSStatus | no | 'A' = Measurement Active 'V' = Measurement Void
> 0x850a | GPSMeasureMode | no | 2 = 2-Dimensional Measurement 3 = 3-Dimensional Measurement
> 0x8512 | GPSMapDatum | no |
> 0x851d | GPSDateStamp | no |
> 0xe303 | WhiteBalance | no |
> 1 = Incandescent 2 = Fluorescent 4 = Daylight |  | 5 = Cloudy 6 = Custom 255 = Preset
> 0xe304 | DateTime | no |
> 0xe43b | PitchRollYaw | no |
> 0xe44b | Accelerometer | no |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Oct 19, 2022

<-- ExifTool Tag Names