## DSF Tags

Tags read from the 'fmt ' header of a DSF (DSD Stream File) audio files. As well, ID3 metadata may also exist in these files. See https://dsd-guide.com/sites/default/files/white-papers/DSFFileFormatSpec_E.pdf for the specification.

> Index4 | Tag Name | Writable | Values / Notes
> --- | --- | --- | ---
> 3 | FormatVersion | no |
> 4 | FormatID | no | 0 = DSD Raw
> 5 | ChannelType | no | 1 = Mono 2 = Stereo (Left, Right) 3 = 3 Channels (Left, Right, Center) 4 = Quad (Left, Right, Back L, Back R) 5 = 4 Channels (Left, Right, Center, Bass) 6 = 5 Channels (Left, Right, Center, Back L, Back R) 7 = 5.1 Channels (Left, Right, Center, Bass, Back L, Back R)
> 6 | ChannelCount | no |
> 7 | SampleRate | no |
> 8 | BitsPerSample | no |
> 9 | SampleCount | no |
> 11 | BlockSize | no |

(This document generated automatically by Image::ExifTool::BuildTagLookup)
Last revised Sep 25, 2025

<-- ExifTool Tag Names